;; Realtek RTLWLANE PCI-E Wireless LAN Network Interface Cards.
;;
;; Copyright 2014, Realtek Semiconductor Corporation
;;

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Realtek%
CatalogFile = netrtwlane.cat                               ;; for WHQL certified
DriverVer = 08/01/2024,2024.10.142.0
PnpLockDown = 1
[Manufacturer]
%Realtek% = Realtek,NTamd64.10.0
%TPLINK% = TPLINK,NTamd64.10.0

[ControlFlags]
ExcludeFromSelect = *

[Realtek.NTamd64.10.0]

;;*******************************************************************************
;; RTK COMMON DEVICE DESC
;;*******************************************************************************





;;----------------------------------------------------------------------------
;; For 8822B RTK common
;;----------------------------------------------------------------------------
%RTL8822be.DeviceDesc%		= RTL8822be.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_B82210EC
%RTL8822be.DeviceDesc%		= RTL8822be.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_B12510EC ;; HP Dragon
%RTL8822be.DeviceDesc%		= RTL8822be.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_B12310EC

;;Lenovo
%RTL8822be.DeviceDesc%		= LNV8822be_pwr_limit.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_B02310EC ;; Lenovo China for preliminary designation for Thinkpad
%RTL8822be.DeviceDesc%		= LNV8822be_pwr_limit.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_B02417AA ;; Lenovo China for Thinkpad FCC sku
%RTL8822be.DeviceDesc%		= LNV8822be_pwr_limit.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_B02517AA ;; Lenovo China for Thinkpad 5GZ B4 Passive scan only SKU for Indonesia
%RTL8822be.DeviceDesc%		= LNV8822be_pwr_limit.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_B02617AA ;; Lenovo China for Thinkpad 11ac disable SKU for Egypt
%RTL8822be.DeviceDesc%		= LNV8822be_pwr_limit.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_B02717AA ;; Lenovo China for Thinkpad 5G B1/B2-only SKU for Tunisia

;;8822BE WAPI
%RTL8822be.DeviceDesc%		= LNV8822be_pwr_limit_wapi.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_B02317AA ;; Lenovo China for Thinkpad WW sku WAPI

;;HP
%HP8822be.DeviceDesc%		= HP8822be.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_831B103C ;; Foxconn
%HP8822be.DeviceDesc%		= HP8822be.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_840B103C ;; Dragon

;;NEC
%RTL8822be.DeviceDesc%		= NEC8822be.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_B02810EC

;;Acer
%RTL8822be.DeviceDesc%		= ACER8822be.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_B02910EC

;;Azurewave
%RTL8822be.DeviceDesc%		= RTL8822be.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_29511A3B
%RTL8822be.DeviceDesc%		= RTL8822be.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_30811A3B

;;Nexstgo (Module maker: GSD)
%RTL8822be.DeviceDesc%		= RTL8822be.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_54672A3B

;;ECS
%RTL8822be.DeviceDesc%		= ECS8822be.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_B03010EC
%RTL8822be.DeviceDesc%		= ECS8822be.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_B03110EC
%RTL8822be.DeviceDesc%		= ECS8822be.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_29551A3B
%RTL8822be.DeviceDesc%		= ECS8822be_WiFiDash.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_B03210EC ;;Mother board (WiFi Dash)

;;Fujitsu
%RTL8822be.DeviceDesc%		= FJT8822be.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_199510CF

;;Toshiba
%RTL8822be.DeviceDesc%		= RTL8822be.ndi,		PCI\VEN_10EC&DEV_B822&SUBSYS_B03510EC




;;----------------------------------------------------------------------------
;; For 8822C RTK common
;;----------------------------------------------------------------------------

;;Realtek demoboard
%RTL8822ce.DeviceDesc% = RTL8822ce.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_C82210EC
%RTL8822ce.DeviceDesc% = RTL8822ce.ndi, PCI\VEN_10EC&DEV_C82F&SUBSYS_C82F10EC ;;RTL8822CE-VS
%RTL8822ce.DeviceDesc% = RTL8822ce.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_C12810EC ;;NGFF1216

;;Lenovo
%RTL8822ce.DeviceDesc% = LNV8822ce.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_C12317AA
%RTL8822ce.DeviceDesc% = LNV8822ce.ndi, PCI\VEN_10EC&DEV_C82F&SUBSYS_C02F17AA ;;RTL8822CE-VS

;;ASUS
;;NB
%RTL8822ce.DeviceDesc% = ASUS8822ce_NB.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_37501A3B ;;Azurewave
%RTL8822ce.DeviceDesc% = ASUS8822ce_NB.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_30501DFB ;;GSD
%RTL8822ce.DeviceDesc% = ASUS8822ce_NB.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_87B11043 ;;ASUS MB

%RTL8822ce.DeviceDesc% = ASUS8822ce_NB_LPS.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_081011AD ;;LiteOn
%RTL8822ce.DeviceDesc% = ASUS8822ce_NB_LPS.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_42111A3B ;;Azurewave NGFF1216

;;Azurewave
%RTL8822ce.DeviceDesc% = RTL8822ce.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_37511A3B
%RTL8822ce.DeviceDesc% = STEAM8822ce.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_42101A3B ;;NGFF1216 for STEAMDECK

;;HP
%HP8822ce.DeviceDesc% = HP8822ce.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_85F7103C

;;Inet
%RTL8822ce.DeviceDesc% = RTL8822ce.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_C12410EC

;;Fujitsu
%RTL8822ce.DeviceDesc% = FJT8822ce.ndi,		PCI\VEN_10EC&DEV_C822&SUBSYS_003C1E26

;;NEC
%RTL8822ce.DeviceDesc% = NEC8822ce.ndi,	PCI\VEN_10EC&DEV_C822&SUBSYS_C12610EC
%RTL8822ce.DeviceDesc% = NEC8822ce.ndi, PCI\VEN_10EC&DEV_C82F&SUBSYS_C03F10EC ;;RTL8822CE-VS

;;Huawei
%RTL8822ce.DeviceDesc% = RTL8822ce.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_1E251058

;;Acer
%RTL8822ce.DeviceDesc% = ACER8822ce.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_305210EC

;;Xiaomi
%RTL8822ce.DeviceDesc% = RTL8822ce.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_C8231D2E

;;Dynabook
%RTL8822ce.DeviceDesc% = RTL8822ce.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_C12910EC ;;NGFF2230
%RTL8822ce.DeviceDesc% = Dynabook8822ce.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_C12710EC ;;NGFF1216

;;Microsoft
%RTL8822ce.DeviceDesc% = MS8822ce.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_C13510EC

;;DELL
%RTL8822ce.DeviceDesc% = DELL8822ce.ndi, PCI\VEN_10EC&DEV_C822&SUBSYS_C13010EC





;;----------------------------------------------------------------------------
;; For 8821C RTK common
;;----------------------------------------------------------------------------
%RTL8821ce.DeviceDesc%		= RTL8821ce.ndi,		PCI\VEN_10EC&DEV_B821&SUBSYS_B82110EC
%RTL8821ce.DeviceDesc%		= RTL8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C81110EC ;;NGFF1216 module
%RTL8821ce.DeviceDesc%		= RTL8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C82110EC
%RTL8821ce.DeviceDesc%		= HP8821ce.ndi,			PCI\VEN_10EC&DEV_C821&SUBSYS_C82310EC ;;single ant(connect to right one S1)
%RTL8821ce.DeviceDesc%		= RTL8821ce.ndi,		PCI\VEN_10EC&DEV_C82B&SUBSYS_C82B10EC

;;Xiaomi
%RTL8821ce.DeviceDesc%		= MI8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C82710EC

;;FN-link (RTL8821CE-VBL-CG, for China module maker that force disable MU-MIMO)
%RTL8821ce.DeviceDesc%		= FN8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C81510EC

;; ASUS
%RTL8821ce.DeviceDesc%		= ASUS8821ce_FCC_REG.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_30471DFB ;;GSD
%RTL8821ce.DeviceDesc%		= ASUS8821ce_FCC_REG.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_30481DFB ;;GSD
%RTL8821ce.DeviceDesc%		= ASUS8821ce_FCC_REG.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_30401A3B ;;Azurewave
%RTL8821ce.DeviceDesc%		= ASUS8821ce_FCC_REG.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_30411A3B ;;Azurewave
%RTL8821ce.DeviceDesc%		= ASUS8821ce_FCC_REG.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_30441A3B ;;Azurewave
%RTL8821ce.DeviceDesc%		= ASUS8821ce_FCC_REG.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_30451A3B ;;Azurewave
%RTL8821ce.DeviceDesc%		= ASUS8821ce_FCC_REG.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_304C1A3B ;;Azurewave, RTL8821CE-VB
%RTL8821ce.DeviceDesc%		= ASUS8821ce_FCC_REG.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_304D1A3B ;;Azurewave, RTL8821CE-VB
%RTL8821ce.DeviceDesc%		= ASUS8821ce_FCC_REG.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_304A1A3B ;;Azurewave, RTL8821CE-VC
%RTL8821ce.DeviceDesc%		= ASUS8821ce_FCC_REG.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_304B1A3B ;;Azurewave, RTL8821CE-VC
%RTL8821ce.DeviceDesc%		= ASUS8821ce_FCC_REG.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_180911AD ;;LiteOn, RTL8821CE-VC
%RTL8821ce.DeviceDesc%		= ASUS8821ce_FCC_REG.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_080911AD ;;LiteOn, RTL8821CE-VC
;; ASUS MB
%RTL8821ce.DeviceDesc%		= ASUS8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_87AE1043 ;;Dual antenna
%RTL8821ce.DeviceDesc%		= ASUS8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_87B01043 ;;Single antenna

;; Azurewave
%RTL8821ce.DeviceDesc%		= RTL8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_30421A3B
%RTL8821ce.DeviceDesc%		= RTL8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_30431A3B
%RTL8821ce.DeviceDesc%		= RTL8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_30491A3B

;; Lenovo
%RTL8821ce.DeviceDesc%		= LNV8821ce_WW_SKU.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C02417AA ;;w/ Dual antenna for diversity (for Ideapad/AIO/DT WW SKU)
%RTL8821ce.DeviceDesc%		= LNV8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C02617AA ;;w/ Dual antenna for diversity (for AIO/DT FCC SKU)
%RTL8821ce.DeviceDesc%		= LNV8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C02717AA ;;w/ Dual antenna for diversity (for AIO/DT Indonesia SKU)
%RTL8821ce.DeviceDesc%		= LNV8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C02817AA ;;w/ Dual antenna for diversity (for AIO/DT 11ac disable SKU for Egypt)
%RTL8821ce.DeviceDesc%		= LNV8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C02917AA ;;w/ Dual antenna for diversity (for AIO/DT Tunisia SKU)

;; HP
%RTL8821ce.DeviceDesc%		= RTL8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C025103C
%HP8821ce.DeviceDesc%		= HP8821ce.ndi,			PCI\VEN_10EC&DEV_C821&SUBSYS_831A103C
%HP8821ce.DeviceDesc%		= HP8821ce.ndi,			PCI\VEN_10EC&DEV_C821&SUBSYS_884D103C ;;RTL8821CE-VB that enables L1SS
%HP8821ce.DeviceDesc%		= HP8821ce.ndi,			PCI\VEN_10EC&DEV_C821&SUBSYS_C032103C ;;RTL8821CE-VC that enables L1SS

;; ACER
%RTL8821ce.DeviceDesc%		= ACER8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C82410EC
%RTL8821ce.DeviceDesc%		= ACER8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C83010EC ;;RTL8821CE-VC that enables L1SS

;; SAMSUNG
%RTL8821ce.DeviceDesc%		= RTL8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_4134144D

;; Vestel
%RTL8821ce.DeviceDesc%		= RTL8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_A4161019

;;Positivo
%RTL8821ce.DeviceDesc%		= RTL8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_304610EC ;;Foxconn for Positivo in Brazil

;;NEC
%RTL8821ce.DeviceDesc%		= RTL8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C03010EC

;;Dynabook
%RTL8821ce.DeviceDesc%		= RTL8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C03110EC

;;DELL
%RTL8821ce.DeviceDesc%		= DELL8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C82810EC ;;RTL8821CE-VC that enables L1SS

;;Tsinghua Unigroup
%RTL8821ce.DeviceDesc%		= RTL8821ce.ndi,		PCI\VEN_10EC&DEV_C821&SUBSYS_C85110EC ;;RTL8821CE-VC that enables L1SS


;;----------------------------------------------------------------------------
;; For 8723D RTK common		
;;----------------------------------------------------------------------------
%RTL8723de.DeviceDesc%		= RTL8723de.ndi,		PCI\VEN_10EC&DEV_D723&SUBSYS_D72310EC

;;HP
%HP8723de.DeviceDesc%		= HP8723de.ndi,			PCI\VEN_10EC&DEV_D723&SUBSYS_8319103C

;;FN-link
%RTL8723de.DeviceDesc%		= FN8723de.ndi,			PCI\VEN_10EC&DEV_D723&SUBSYS_D12310EC

;;DELL
%RTL8723de.DeviceDesc%		= DELL8723de.ndi,		PCI\VEN_10EC&DEV_D723&SUBSYS_D73810EC


[TPLINK.NTamd64.10.0]



;;****************************************************************************
;; Install
;;****************************************************************************






;;----------------------------------------------------------------------------
;; Realtek default installation
;;----------------------------------------------------------------------------


[RTL8822be.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = 11acWirelessMode.reg, RTL8822be.Common.reg, MSIEnable.reg, 32kEnable.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnablePG.reg, TcpReorderEnable.reg, RealWoW.reg, L1OffEnable.reg, DelayeMACePHY.reg, MCCEnable_v3.reg, S5Wake.reg, PowerConsumption_8822b.reg, LtrHWAuto.reg, IQKBeforeConnection.reg, EnhanceLPS_Enable.reg, AdvanceConductiveTest.reg, MCCReport.reg, ECS_SUPPORT_SCAN_P2P_ON.reg, EnableSupportMACRandom.reg, NewRxReorderSettingsEnable.reg, PreferBand5G_NewMethod.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[RTL8822be.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8822be.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; ECS installation
;;----------------------------------------------------------------------------


[ECS8822be.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = 11acWirelessMode.reg, RTL8822be.Common.reg, MSIEnable.reg, 32kEnable.reg, WowlanEnable.reg, WowlanPSModeLPS32k.reg, TcpReorderEnable.reg, RealWoW.reg, L1OffEnable.reg, DelayeMACePHY.reg, MCCDisable_v2.reg, S5Wake.reg, PowerConsumption_8822b.reg, LtrHWAuto.reg, IQKBeforeConnection.reg, EnhanceLPS_Enable.reg, AdvanceConductiveTest.reg, MCCReport.reg, EnableClassMode.reg, NewRxReorderSettingsEnable.reg, NonRoamingSensitivity.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ECS8822be.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[ECS8822be.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; Realtek default installation (ECS WiFi Dash)
;;----------------------------------------------------------------------------


[ECS8822be_WiFiDash.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = 11acWirelessMode.reg, RTL8822be.Common.reg, MSIEnable.reg, 32kEnable.reg, WowlanDisable.reg, TcpReorderEnable.reg, RealWoW.reg, L1OffEnable.reg, DelayeMACePHY.reg, MCCDisable_v2.reg, PowerConsumption_8822b.reg, LtrHWAuto.reg, IQKBeforeConnection.reg, EnhanceLPS_Enable.reg, AdvanceConductiveTest.reg, MCCReport.reg, NonRoamingSensitivity.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ECS8822be_WiFiDash.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[ECS8822be_WiFiDash.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; Fujitsu default installation
;;----------------------------------------------------------------------------


[FJT8822be.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, RTL8822be.Common.reg, MSIEnable.reg, 32kEnable.reg, ModernStandbyEnable.reg, WowlanPSModeLPS32k.reg, TcpReorderEnable.reg, RealWoW.reg, L1OffEnable.reg, DelayeMACePHY.reg, MCCEnable_v3.reg, AdvanceWdiGOon5GHzBandSupportedEnable.reg, S5Wake.reg, PowerConsumption_8822b.reg, LtrHWAuto.reg, IQKBeforeConnection.reg, EnableSupportMACRandom.reg, RoamingAggressiveness.reg, EnhanceLPS_Enable.reg, AdvanceConductiveTest.reg, ECS_SUPPORT_SWITCH_ON.reg, MCCReport.reg, FJT_EXTEND_PASSIVE_SCAN_CHNL_LIST.reg, SKU_From_SMBIOS_Enable.reg, NewRxReorderSettingsEnable.reg,FJT8822be_LBC.reg, Dot11dDisable.reg
DelReg          = DelRTLWLAN.reg
DelReg          = DelRoamingAggressiveness.reg, DelRegFujitsuRS5Inbox.reg,FJT8822beDelLBC.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[FJT8822be.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[FJT8822be.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg



;;----------------------------------------------------------------------------
;; NEC default installation
;;----------------------------------------------------------------------------


[NEC8822be.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, RTL8822be.Common.reg, MSIEnable.reg, 32kEnable.reg, WowlanEnable.reg, WowlanPSModeLPS32k.reg, TcpReorderEnable.reg, RealWoW.reg, L1OffEnable.reg, DelayeMACePHY.reg, MCCEnable_v2.reg, WdiGODfsErrorDisable.reg, PowerConsumption_8822b.reg, LtrHWAuto.reg, IQKBeforeConnection.reg, EnhanceLPS_Enable.reg, AdvanceConductiveTest.reg, MCCReport.reg, PreferBand5G.reg, NECRoamingAggressiveness.reg, NECRoamingAlog.reg, NewRxReorderSettingsEnable.reg, ECS_SUPPORT_SWITCH_ON.reg, ECS_Skype_TrafficDectect_ON.reg, NEC_EXTEND_PASSIVE_SCAN_CHNL_LIST.reg, AddExtCh.reg, SupportTxFeedback.reg, EnableScanTimerActionTimer.reg, EnableProbeReqTxFeedback.reg, NEC_ECS_SETTING.reg
DelReg          = DelRTLWLAN.reg, NECDelRoamingAggressiveness.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[NEC8822be.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[NEC8822be.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------

;;----------------------------------------------------------------------------
;; Lenovo China with daymic power limit installation
;;----------------------------------------------------------------------------


[LNV8822be_pwr_limit.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = 11acWirelessMode.reg, RTL8822be.Common.reg, LC.Common.reg, MSIEnable.reg, 32kEnable.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnable.reg, TcpReorderEnable.reg, L1OffEnable.reg, DelayeMACePHY_OFF.reg, APCI_Lenovo_WRDS_SAR.reg, MCCEnable_v3.reg, WdiGOon5GHzBandSupportedEnable.reg, 5GpassiveScan.reg, PowerConsumption_8822b.reg, IntMitDisable.reg, EnableSupportMACRandom.reg, LtrHWAuto.reg, IQKBeforeConnection.reg, EnhanceLPS_Enable.reg, MCCReport.reg, EnableTxPowerTableFromSingleFile.reg,RealWoW.reg,ECS_SUPPORT_SCAN_P2P_ON.reg, RetryTimes_32.reg, Specify8822beTxPwrLmtTableID_UpdateUkraine.reg, PreferBand5G.reg, NewRxReorderSettingsEnable.reg, IPSEnable.reg, LPSEnable.reg, Periodic_chk_twice.reg, SupportTxFeedback.reg, EnableScanTimerActionTimer.reg, EnableProbeReqTxFeedback.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[LNV8822be_pwr_limit.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[LNV8822be_pwr_limit.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; Lenovo China with daymic power limit installation wapi
;;----------------------------------------------------------------------------


[LNV8822be_pwr_limit_wapi.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = 11acWirelessMode.reg, RTL8822be.Common.reg, LC.Common.reg, MSIEnable.reg, 32kEnable.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnable.reg, TcpReorderEnable.reg, L1OffEnable.reg, DelayeMACePHY_OFF.reg, APCI_Lenovo_WRDS_SAR.reg, MCCEnable_v3.reg, WdiGOon5GHzBandSupportedEnable.reg, 5GpassiveScan.reg, PowerConsumption_8822b.reg, IntMitDisable.reg, EnableSupportMACRandom.reg, LtrHWAuto.reg, IQKBeforeConnection.reg, EnhanceLPS_Enable.reg, MCCReport.reg, EnableTxPowerTableFromSingleFile.reg,RealWoW.reg,ECS_SUPPORT_SCAN_P2P_ON.reg, RetryTimes_32.reg, Specify8822beTxPwrLmtTableID_UpdateUkraine.reg, PreferBand5G.reg, NewRxReorderSettingsEnable.reg, IPSEnable.reg, LPSEnable.reg, Periodic_chk_twice.reg, SupportTxFeedback.reg, EnableScanTimerActionTimer.reg, EnableProbeReqTxFeedback.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[LNV8822be_pwr_limit_wapi.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[LNV8822be_pwr_limit_wapi.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; HP installation
;;----------------------------------------------------------------------------


[HP8822be.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acAdvancedWirelessMode.reg, RTL8822be.Common.reg, HP.Common.reg, HP.Common_2017.reg, MSIEnable.reg, 32kEnable.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnable.reg, TcpReorderEnable.reg, RealWoW.reg, L1OffEnable.reg, DelayeMACePHY.reg, MCCEnable_v3.reg, PowerConsumption_8822b.reg, LtrHWAuto.reg, S5Wake.reg, WdiGOon5GHzBandSupportedEnable.reg, IQKBeforeConnection.reg, EnhanceLPS_Enable.reg, MCCReport.reg, PMEFollow.reg, Specify8822beTxPwrLmtTableID_UpdateUkraine.reg, RetryTimes_32.reg, NewRxReorderSettingsEnable.reg, ECS_SUPPORT_SCAN_P2P_ON.reg, Periodic_chk_twice.reg, PreferBand5G_NewMethod.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[HP8822be.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[HP8822be.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; ACER installation
;;----------------------------------------------------------------------------


[ACER8822be.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, RTL8822be.Common.reg, MSIEnable.reg, 32kEnable.reg, WowlanEnable.reg, WowlanPSModeLPS32k.reg, TcpReorderEnable.reg, RealWoW.reg, L1OffEnable.reg, DelayeMACePHY.reg, RSSI2GridMode_5.reg, MCCDisable_v2.reg, PowerConsumption_8822b.reg, LtrHWAuto.reg, IQKBeforeConnection.reg, EnhanceLPS_Enable.reg, AdvanceConductiveTest.reg, MCCReport.reg, NewRxReorderSettingsEnable.reg, NonRoamingSensitivity.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ACER8822be.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[ACER8822be.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; ASUS NB installation
;;----------------------------------------------------------------------------


[ASUS8822be_NB.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = 11acWirelessMode.reg, RTL8822be.Common.reg, MSIEnable.reg, 32kEnable.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnable.reg, TcpReorderEnable.reg, RealWoW.reg, L1OffEnable.reg, DelayeMACePHY_OFF.reg, MCCDisable_v3.reg, PowerConsumption_8822b.reg, EnableDynamicReloadTxPwrLmtTableByRegulation.reg, ASUS_AdvanceOTA.reg, LtrHWAuto.reg, ASUS8822be_ExtPwrTableDynamicSwitch.reg, IQKBeforeConnection.reg, EnhanceLPS_Enable.reg, AdvanceConductiveTest.reg, MCCReport.reg, APCI_ASUS_BIOS_SAR.reg, RetryTimes_5.reg, AdvancedRetryLimit.reg, WdiGOon5GHzBandSupportedEnable.reg, BTPowerDown_at_S5.reg, NonRoamingSensitivity.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ASUS8822be_NB.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[ASUS8822be_NB.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; ASUS OPBG installation
;;----------------------------------------------------------------------------


[ASUS8822be_OPBG.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = 11acWirelessMode.reg, RTL8822be.Common.reg, MSIEnable.reg, 32kEnable.reg, WowlanEnable.reg, WowlanPSModeLPS32k.reg, TcpReorderEnable.reg, L1OffEnable.reg, DelayeMACePHY_OFF.reg, MCCDisable_v3.reg, S5Wake.reg, PowerConsumption_8822b.reg, EnableDynamicReloadTxPwrLmtTableByRegulation.reg, LtrHWAuto.reg, IQKBeforeConnection.reg, EnhanceLPS_Enable.reg, AdvanceConductiveTest.reg, MCCReport.reg, WdiGOon5GHzBandSupportedEnable.reg, BTPowerDown_at_S5.reg, NonRoamingSensitivity.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ASUS8822be_OPBG.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[ASUS8822be_OPBG.ndi.NT.HW]
Include = netvwifibus.inf
Needs  = VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg



;;----------------------------------------------------------------------------
;; Realtek default installation
;;----------------------------------------------------------------------------


[RTL8822ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, RTL8822ce.Common.reg, RTL8822ce.ASPM.reg, PowerConsumption_8822c.reg, MSIEnable.reg, TcpReorderEnable.reg, ECS_SUPPORT_SCAN_P2P_ON_AND_RM.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnablePG.reg, RealWoW.reg, S5Wake.reg, WW.SingleSku.RTK.reg, MCCEnable_v3.reg, MCCReport.reg, WdiGOon5GHzBandSupportedEnable.reg, EnableSupportMACRandom.reg, NewRxReorderSettingsEnable.reg, FakeGCEnable.reg, PGEnable.reg, PreferBand5G_NewMethod.reg, GOPreferMode.reg
AddReg          = SKU_From_SMBIOS_Enable.reg, APCI_RTK_BIOS_SAR.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs = VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71 ; IF_TYPE_IEEE80211
*MediaType      = 16 ; NdisMediumNative802_11
*PhysicalMediaType = 9 ; NdisPhysicalMediumNative802_11

[RTL8822ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8822ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs  = VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; Microsoft 8822CE installation
;;----------------------------------------------------------------------------


[MS8822ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, RTL8822ce.Common.reg, RTL8822ce.ASPM.reg, PowerConsumption_8822c.reg, MSIEnable.reg, TcpReorderEnable.reg, ECS_SUPPORT_SCAN_P2P_ON_AND_RM.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnablePG.reg, RealWoW.reg, S5Wake.reg, WW.SingleSku.RTK.reg, MCCEnable_v3.reg, MCCReport.reg, WdiGOon5GHzBandSupportedEnable.reg, EnableSupportMACRandom.reg, NewRxReorderSettingsEnable.reg, FakeGCEnable.reg, PGEnable.reg, PreferBand5G_NewMethod.reg, MSCommon.reg
AddReg          = SKU_From_SMBIOS_Enable.reg, APCI_RTK_BIOS_SAR.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs = VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71 ; IF_TYPE_IEEE80211
*MediaType      = 16 ; NdisMediumNative802_11
*PhysicalMediaType = 9 ; NdisPhysicalMediumNative802_11

[MS8822ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[MS8822ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs  = VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; DELL 8822CE installation
;;----------------------------------------------------------------------------


[DELL8822ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, RTL8822ce.Common.reg, RTL8822ce.ASPM.reg, PowerConsumption_8822c.reg, MSIEnable.reg, TcpReorderEnable.reg, ECS_SUPPORT_SCAN_P2P_ON_AND_RM.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnablePG.reg, RealWoW.reg, S5Wake.reg, WW.SingleSku.RTK.reg, MCCEnable_v3.reg, WdiGOon5GHzBandSupportedEnable.reg, EnableSupportMACRandom.reg, NewRxReorderSettingsEnable.reg, FakeGCEnable.reg, PGEnable.reg, PreferBand5G_NewMethod.reg
AddReg          = DELL.Common.reg, APCI_DELL_BIOS_SAR.reg, RoamingSensitivity.reg, TPC_Support.reg, GOPreferMode_DELL.reg, IdnNewBandSupport.reg, Periodic_chk_twice.reg, AuthTimeoutPLDREn.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs = VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71 ; IF_TYPE_IEEE80211
*MediaType      = 16 ; NdisMediumNative802_11
*PhysicalMediaType = 9 ; NdisPhysicalMediumNative802_11

[DELL8822ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[DELL8822ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs = VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg


;;----------------------------------------------------------------------------
;; ASUS NB installation
;;----------------------------------------------------------------------------


[ASUS8822ce_NB.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, RTL8822ce.Common.reg, RTL8822ce.ASPM.reg, PowerConsumption_8822c.reg, MSIEnable.reg, TcpReorderEnable.reg, ECS_SUPPORT_SWITCH_ON.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnablePG.reg, RealWoW.reg, WW.SingleSku.RTK.reg, InterferenceTest.reg, MCCEnable_v3.reg, MCCReport.reg, APCI_ASUS_BIOS_SAR.reg, WdiGOon5GHzBandSupportedEnable.reg, PGEnable.reg, NonRoamingSensitivity.reg, L1BusyTh5000.reg, Periodic_chk_twice.reg
AddReg          = ASUS.NB.Common.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs = VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71 ; IF_TYPE_IEEE80211
*MediaType      = 16 ; NdisMediumNative802_11
*PhysicalMediaType = 9 ; NdisPhysicalMediumNative802_11

[ASUS8822ce_NB.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[ASUS8822ce_NB.ndi.NT.HW]
Include = netvwifibus.inf
Needs  = VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; ASUS NB LPS installation
;;----------------------------------------------------------------------------


[ASUS8822ce_NB_LPS.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, RTL8822ce.Common.reg, RTL8822ce.ASPM.reg, PowerConsumption_8822c.reg, MSIEnable.reg, TcpReorderEnable.reg, ECS_SUPPORT_SWITCH_ON.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnablePG.reg, RealWoW.reg, WW.SingleSku.RTK.reg, InterferenceTest.reg, MCCEnable_v3.reg, MCCReport.reg, APCI_ASUS_BIOS_SAR.reg, WdiGOon5GHzBandSupportedEnable.reg, PGEnable.reg, NonRoamingSensitivity.reg, ACModeDisable32K.reg, L1BusyTh5000.reg, Periodic_chk_twice.reg
AddReg          = ASUS.NB.Common.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs = VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71 ; IF_TYPE_IEEE80211
*MediaType      = 16 ; NdisMediumNative802_11
*PhysicalMediaType = 9 ; NdisPhysicalMediumNative802_11

[ASUS8822ce_NB_LPS.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[ASUS8822ce_NB_LPS.ndi.NT.HW]
Include = netvwifibus.inf
Needs  = VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg


;;----------------------------------------------------------------------------
;; HP installation
;;----------------------------------------------------------------------------


[HP8822ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acAdvancedWirelessMode.reg, RTL8822ce.Common.reg, RTL8822ce.ASPM.reg, PowerConsumption_8822c.reg, HP.CommonNew.reg, MSIEnable.reg, TcpReorderEnable.reg, ECS_SUPPORT_SCAN_P2P_ON.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnablePG.reg, RealWoW.reg, S5Wake.reg, MCCEnable_v3.reg, WdiGOon5GHzBandSupportedEnable.reg, PMEFollow.reg, RetryTimes_32.reg, NewRxReorderSettingsEnable.reg, FakeGCEnable.reg, PGEnable.reg, DisableIMPSWA.reg, Periodic_chk_twice.reg, PreferBand5G_NewMethod.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs = VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71 ; IF_TYPE_IEEE80211
*MediaType      = 16 ; NdisMediumNative802_11
*PhysicalMediaType = 9 ; NdisPhysicalMediumNative802_11

[HP8822ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[HP8822ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs  = VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg




;;----------------------------------------------------------------------------
;; LNV installation
;;----------------------------------------------------------------------------


[LNV8822ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, RTL8822ce.Common.reg, RTL8822ce.ASPM.reg, PowerConsumption_8822c.reg, LC.CommonNew.reg, MSIEnable.reg, TcpReorderEnable.reg, ECS_SUPPORT_SCAN_P2P_ON.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnablePG.reg, RealWoW.reg, WW.SingleSku.RTK.reg, MCCEnable_v3.reg, WdiGOon5GHzBandSupportedEnable.reg, 5GpassiveScan.reg, EnableSupportMACRandom.reg, APCI_Lenovo_WRDS_SAR.reg, PreferBand5G.reg, NewRxReorderSettingsEnable.reg, Periodic_chk_twice.reg, Enable_PA_Recover.reg, GOPreferMode_Lnv.reg, LNV_Skip_p2p_discover.reg, LNV_MCC_control_by_ECS.reg, ScanTh.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs = VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71 ; IF_TYPE_IEEE80211
*MediaType      = 16 ; NdisMediumNative802_11
*PhysicalMediaType = 9 ; NdisPhysicalMediumNative802_11

[LNV8822ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[LNV8822ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs  = VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; Fujitsu installation
;;----------------------------------------------------------------------------


[FJT8822ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, RTL8822ce.Common.reg, RTL8822ce.ASPM.reg, PowerConsumption_8822c.reg, MSIEnable.reg, TcpReorderEnable.reg, ECS_SUPPORT_SWITCH_ON.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnablePG.reg, RealWoW.reg, S5Wake.reg, MCCEnable_v3.reg, AdvanceWdiGOon5GHzBandSupportedEnable.reg, EnableSupportMACRandom.reg, PGEnable.reg, RoamingAggressiveness.reg, FJT_EXTEND_PASSIVE_SCAN_CHNL_LIST.reg, SKU_From_SMBIOS_Enable.reg, NewRxReorderSettingsEnable.reg, Dot11dDisable.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs = VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71 ; IF_TYPE_IEEE80211
*MediaType      = 16 ; NdisMediumNative802_11
*PhysicalMediaType = 9 ; NdisPhysicalMediumNative802_11

[FJT8822ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[FJT8822ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs  = VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg


;;----------------------------------------------------------------------------
;; NEC installation
;;----------------------------------------------------------------------------


[NEC8822ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, RTL8822ce.Common.reg, RTL8822ce.ASPM.reg, PowerConsumption_8822c.reg, MSIEnable.reg, TcpReorderEnable.reg, ECS_SUPPORT_SWITCH_ON.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnablePG.reg, RealWoW.reg, S5Wake.reg, WW.SingleSku.RTK.reg, MCCEnable_v3.reg, WdiGOon5GHzBandSupportedEnable.reg, EnableSupportMACRandom.reg, PGEnable.reg, PreferBand5G.reg, NECRoamingAggressiveness.reg, NECRoamingAlog.reg, WdiGODfsErrorDisable.reg, NewRxReorderSettingsEnable.reg, AddExtCh.reg, SupportTxFeedback.reg, EnableScanTimerActionTimer.reg, EnableProbeReqTxFeedback.reg, NEC_ECS_SETTING.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs = VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71 ; IF_TYPE_IEEE80211
*MediaType      = 16 ; NdisMediumNative802_11
*PhysicalMediaType = 9 ; NdisPhysicalMediumNative802_11

[NEC8822ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[NEC8822ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs  = VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; ACER 8822CE installation
;;----------------------------------------------------------------------------


[ACER8822ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, RTL8822ce.Common.reg, RTL8822ce.ASPM.reg, PowerConsumption_8822c.reg, MSIEnable.reg, TcpReorderEnable.reg, ECS_SUPPORT_SCAN_P2P_ON.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnablePG.reg, RealWoW.reg, S5Wake.reg, WW.SingleSku.RTK.reg, MCCEnable_v3.reg, WdiGOon5GHzBandSupportedEnable.reg, EnableSupportMACRandom.reg, NewRxReorderSettingsEnable.reg, FakeGCEnable.reg, PGEnable.reg, PreferBand5G_NewMethod.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs = VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71 ; IF_TYPE_IEEE80211
*MediaType      = 16 ; NdisMediumNative802_11
*PhysicalMediaType = 9 ; NdisPhysicalMediumNative802_11

[ACER8822ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[ACER8822ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs  = VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; STEAMDECK NB installation
;;----------------------------------------------------------------------------


[STEAM8822ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, RTL8822ce.Common.reg, RTL8822ce.ASPM.reg, PowerConsumption_8822c.reg, MSIEnable.reg, TcpReorderEnable.reg, ECS_SUPPORT_SCAN_P2P_ON_AND_RM.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnablePG.reg, RealWoW.reg, S5Wake.reg, WW.SingleSku.RTK.reg, MCCEnable_v3.reg, MCCReport.reg, WdiGOon5GHzBandSupportedEnable.reg, EnableSupportMACRandom.reg, NewRxReorderSettingsEnable.reg, FakeGCEnable.reg, PGEnable.reg, PreferBand5G_NewMethod.reg, SMPowerSaveEnable.reg, RoamingSensitivity.reg, SupportTxFeedback.reg
AddReg          = SKU_From_SMBIOS_Enable.reg, APCI_RTK_BIOS_SAR.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs = VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71 ; IF_TYPE_IEEE80211
*MediaType      = 16 ; NdisMediumNative802_11
*PhysicalMediaType = 9 ; NdisPhysicalMediumNative802_11

[STEAM8822ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[STEAM8822ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs  = VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; Dynabook 8822CE installation
;;----------------------------------------------------------------------------


[Dynabook8822ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, RTL8822ce.Common.reg, RTL8822ce.ASPM.reg, PowerConsumption_8822c.reg, MSIEnable.reg, TcpReorderEnable.reg, ECS_SUPPORT_SCAN_P2P_ON_AND_RM.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnablePG.reg, RealWoW.reg, S5Wake.reg, WW.SingleSku.RTK.reg, MCCEnable_v3.reg, MCCReport.reg, WdiGOon5GHzBandSupportedEnable.reg, EnableSupportMACRandom.reg, NewRxReorderSettingsEnable.reg, FakeGCEnable.reg, PGEnable.reg, PreferBand5G_NewMethod.reg, GOPreferMode.reg
AddReg          = SKU_From_SMBIOS_Enable.reg, APCI_RTK_BIOS_SAR.reg, Dynabook.Common.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs = VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71 ; IF_TYPE_IEEE80211
*MediaType      = 16 ; NdisMediumNative802_11
*PhysicalMediaType = 9 ; NdisPhysicalMediumNative802_11

[Dynabook8822ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[Dynabook8822ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs  = VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg






;;----------------------------------------------------------------------------
;; Realtek default installation
;;----------------------------------------------------------------------------


[RTL8821ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, RTL8821ce.Common.reg, MSIEnable.reg, 32kEnable.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnable.reg, TcpReorderEnable.reg, PGDisable.reg, RealWoW.reg, IntMitEnable_v1.reg, LtrHWAuto.reg, S5Wake.reg, IQKBeforeConnection.reg, AdvanceConductiveTest.reg, MCCEnable_v3.reg, MCCReport.reg, EnableSupportMACRandom.reg, NewRxReorderSettingsEnable.reg, ECS_SUPPORT_SCAN_P2P_ON_AND_RM.reg, PreferBand5G_NewMethod.reg, GOPreferMode.reg
AddReg          = WW.SingleSku.RTK.reg, SKU_From_SMBIOS_Enable.reg, APCI_RTK_BIOS_SAR.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[RTL8821ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8821ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; DELL RTL8821CE installation
;;----------------------------------------------------------------------------


[DELL8821ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = 11acWirelessMode.reg, RTL8821ce.Common.reg, MSIEnable.reg, 32kEnable.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnable.reg, TcpReorderEnable.reg, PGDisable.reg, RealWoW.reg, IntMitEnable_v1.reg, LtrHWAuto.reg, S5Wake.reg, IQKBeforeConnection.reg, AdvanceConductiveTest.reg, MCCEnable_v3.reg, EnableSupportMACRandom.reg, NewRxReorderSettingsEnable.reg, ECS_SUPPORT_SCAN_P2P_ON_AND_RM.reg, PreferBand5G_NewMethod.reg, AdvancedLPsEnable_v4.reg
AddReg          = DELL.Common.reg, WdiGOon5GHzBandSupportedEnable.reg, APCI_DELL_BIOS_SAR.reg, RoamingSensitivity.reg, TPC_Support.reg, GOPreferMode_DELL.reg, IdnNewBandSupport.reg, Periodic_chk_twice.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[DELL8821ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[DELL8821ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs = VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;--------------------------------------------------------------------------------------------------
;; Xiaomi installation
;;--------------------------------------------------------------------------------------------------


[MI8821ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = 11acWirelessMode.reg, MI8821ce.Common.reg, MSIEnable.reg, 32kEnable.reg, WowlanEnable.reg, WowlanPSModeLPS32k.reg, TcpReorderEnable.reg, PGDisable.reg, RealWoW.reg, WdiGOon5GHzBandSupportedEnable.reg, IntMitEnable_v1.reg, LtrHWAuto.reg, S5Wake.reg, IQKBeforeConnection.reg, AdvanceConductiveTest.reg, L1OffEnable.reg, MCCEnable_v3.reg, MCCReport.reg, GoMoveToStaEnable.reg, NewRxReorderSettingsEnable.reg, NonRoamingSensitivity.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[MI8821ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[MI8821ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;--------------------------------------------------------------------------------------------------
;; FN-Link installation (RTL8821CE-VBL-CG module, For China module maker that force disable MU-MIMO)
;;--------------------------------------------------------------------------------------------------


[FN8821ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acWirelessMode.reg, FN8821ce.Common.reg, MSIEnable.reg, 32kEnable.reg, WowlanEnable.reg, WowlanPSModeLPS32k.reg, TcpReorderEnable.reg, PGDisable.reg, RealWoW.reg, IntMitEnable_v1.reg, LtrHWAuto.reg, S5Wake.reg, IQKBeforeConnection.reg, AdvanceConductiveTest.reg, NewRxReorderSettingsEnable.reg, NonRoamingSensitivity.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[FN8821ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[FN8821ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; Lenovo China installation
;;----------------------------------------------------------------------------


[LNV8821ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = 11acWirelessMode.reg, RTL8821ce.Common.reg, LC.Common.reg, MSIEnable.reg, 32kEnable.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnable.reg, TcpReorderEnable.reg, PGDisable.reg, RealWoW.reg, WdiGOon5GHzBandSupportedEnable.reg, IntMitDisable.reg, AntSwBiasEnable.reg, STBCDisable.reg, DmCsiRptEnable.reg, MCCEnable_v3.reg, EnableTxPowerTableFromSingleFile.reg, IQKBeforeConnection.reg, MCCReport.reg, LtrHWAuto.reg, ApplyBModeOtaPatch.reg, RetryTimes_32.reg, Specify8821ceTxPwrLmtTableID_UpdateUkraine.reg, NewRxReorderSettingsEnable.reg, ECS_SUPPORT_SCAN_P2P_ON.reg, Periodic_chk_twice.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[LNV8821ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[LNV8821ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; Lenovo China (WW SKU) installation
;;----------------------------------------------------------------------------


[LNV8821ce_WW_SKU.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = 11acWirelessMode.reg, RTL8821ce.Common.reg, LC.Common.reg, MSIEnable.reg, 32kEnable.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnable.reg, TcpReorderEnable.reg, PGDisable.reg, RealWoW.reg, WdiGOon5GHzBandSupportedEnable.reg, IntMitDisable.reg, AntSwBiasEnable.reg, STBCDisable.reg, DmCsiRptEnable.reg, MCCEnable_v3.reg, EnableTxPowerTableFromSingleFile.reg, IQKBeforeConnection.reg, MCCReport.reg, LtrHWAuto.reg, ApplyBModeOtaPatch.reg, RetryTimes_32.reg, Specify8821ceTxPwrLmtTableID_UpdateUkraine.reg, ECS_SUPPORT_SCAN_P2P_ON.reg, Periodic_chk_twice.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[LNV8821ce_WW_SKU.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[LNV8821ce_WW_SKU.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; HP installation
;;----------------------------------------------------------------------------


[HP8821ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = 11acAdvancedWirelessMode.reg, RTL8821ce.Common.reg, HP.Common.reg, HP.Common_2017.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnable.reg, MSIEnable.reg, 32kEnable.reg, TcpReorderEnable.reg, PGDisable.reg, RealWoW.reg, IntMitEnable_v1.reg, MCCEnable_v3.reg, LtrHWAuto.reg, S5Wake.reg, IQKBeforeConnection.reg, WdiGOon5GHzBandSupportedEnable.reg, MCCReport.reg, PMEFollow.reg, Specify8821ceTxPwrLmtTableID_UpdateUkraine.reg, RetryTimes_32.reg, NewRxReorderSettingsEnable.reg, ECS_SUPPORT_P2P_ON.reg, Periodic_chk_twice.reg, PreferBand5G_NewMethod.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[HP8821ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[HP8821ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; ASUS installation
;;----------------------------------------------------------------------------


[ASUS8821ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = 11acWirelessMode.reg, RTL8821ce.Common.reg, MSIEnable.reg, 32kEnable.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnable.reg, TcpReorderEnable.reg, PGDisable.reg, RealWoW.reg, IntMitEnable_v1.reg, LtrHWAuto.reg, IQKBeforeConnection.reg, AdvanceConductiveTest.reg, APCI_ASUS_BIOS_SAR.reg, MCCEnable_v3.reg, MCCReport.reg, BTPowerDown_at_S5.reg, NewRxReorderSettingsEnable.reg, NonRoamingSensitivity.reg, WdiGOon5GHzBandSupportedEnable.reg
AddReg          = ASUS.MB.Common.reg, ECS_SUPPORT_SCAN_P2P_ON_AND_RM.reg, Periodic_chk_twice.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ASUS8821ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[ASUS8821ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; ASUS FCC Regulation installation
;;----------------------------------------------------------------------------


[ASUS8821ce_FCC_REG.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = 11acWirelessMode.reg, RTL8821ce.Common.reg, MSIEnable.reg, 32kEnable.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnable.reg, TcpReorderEnable.reg, PGDisable.reg, RealWoW.reg, IntMitEnable_v1.reg, LtrHWAuto.reg, IQKBeforeConnection.reg, AdvanceConductiveTest.reg, APCI_ASUS_BIOS_SAR.reg, MCCEnable_v3.reg, MCCReport.reg, BTPowerDown_at_S5.reg, NewRxReorderSettingsEnable.reg, Specify8821ceTxPwrLmtTableID_27.reg, EmacDelay_ASUS_8821CE.reg, NonRoamingSensitivity.reg, WdiGOon5GHzBandSupportedEnable.reg
AddReg          = ASUS.NB.Common.reg, ECS_SUPPORT_SCAN_P2P_ON_AND_RM.reg, Periodic_chk_twice.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ASUS8821ce_FCC_REG.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[ASUS8821ce_FCC_REG.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; ACER installation
;;----------------------------------------------------------------------------


[ACER8821ce.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = 11acWirelessMode.reg, RTL8821ce.Common.reg, ACER.Common.reg, MSIEnable.reg, 32kEnable.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnable.reg, TcpReorderEnable.reg, PGDisable.reg, RealWoW.reg, IntMitEnable_v1.reg, LtrHWAuto.reg, IQKBeforeConnection.reg, NewRxReorderSettingsEnable.reg, NonRoamingSensitivity.reg, WdiGOon5GHzBandSupportedEnable.reg, MCCEnable_v3.reg, MCCReport.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ACER8821ce.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[ACER8821ce.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg



;;----------------------------------------------------------------------------
;; Realtek default installation
;;----------------------------------------------------------------------------


[RTL8723de.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = RoamingSensitivity.reg, 11nWirelessMode.reg, RTL8723de.Common.reg, MSIEnable.reg, 32kDisable.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnable.reg, TcpReorderEnable.reg, RealWoW.reg, L1OffEnable.reg, AntDetectDisable.reg, LtrHWAuto.reg, EnableSupportMACRandom.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[RTL8723de.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8723de.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; HP installation
;;----------------------------------------------------------------------------


[HP8723de.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = RoamingSensitivity.reg, 11nAdvancedWirelessMode.reg, RTL8723de.Common.reg, HP.Common.reg, HP.Common_2017.reg, MSIEnable.reg, 32kEnable.reg, WowlanEnable.reg, WowlanPSModeLPS32k.reg, TcpReorderEnable.reg, RSSI2GridMode_3.reg, Class.reg, IsHPAdvanceSetting.reg, RealWoW.reg, AntDetectDisable.reg, AntDivDisable.reg, EnableForcedCCKTH.reg, LtrHWAuto.reg, S5Wake.reg, PMEFollow.reg, RetryTimes_32.reg, ECS_SUPPORT_P2P_ON.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[HP8723de.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[HP8723de.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg
;;----------------------------------------------------------------------------
;; ASUS installation
;;----------------------------------------------------------------------------


[ASUS8723de.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = RoamingSensitivity.reg, 11nWirelessMode.reg, RTL8723de.Common.reg, ASUS.NB.Common.reg, MSIEnable.reg, 32kDisable.reg, TcpReorderEnable.reg, RealWoW.reg, AntDetectDisable.reg, LtrHWAuto.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnable.reg, APCI_ASUS_BIOS_SAR.reg, MCCDisable_v2.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ASUS8723de.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[ASUS8723de.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; FN-LINK installation
;;----------------------------------------------------------------------------


[FN8723de.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = RoamingSensitivity.reg, 11nWirelessMode.reg, RTL8723de.Common.reg, MSIEnable.reg, 32kDisable.reg, WowlanEnable.reg, WowlanPSModeAllDisable.reg, TcpReorderEnable.reg, RealWoW.reg, L1OffDisable.reg, AntDetectDisable.reg, LtrHWAuto.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[FN8723de.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[FN8723de.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;----------------------------------------------------------------------------
;; DELL installation
;;----------------------------------------------------------------------------


[DELL8723de.ndi.NT]
AddReg          = NDIS_64.reg, RTLWLAN.reg
AddReg          = WW.SingleSku.RTK.reg
AddReg          = RoamingSensitivity.reg, 11nWirelessMode.reg, RTL8723de.Common.reg, MSIEnable.reg, 32kEnable.reg, ModernStandbyEnable.reg, WowlanPSModeAllEnable.reg, TcpReorderEnable.reg, RSSI2GridMode_3.reg, Class.reg, LtrHWAuto.reg, PMEFollow.reg, RetryTimes_32.reg, Dot11dEnable.reg, APCI_DELL_BIOS_SAR.reg, DELL8723de.ASPM.reg
DelReg          = DelRTLWLAN.reg
Include         = netvwifibus.inf
Needs		= VWiFiBus.CopyFiles
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTWlanE.CopyFiles
FeatureScore    = 0xFE
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[DELL8723de.ndi.NT.Services]
AddService = RTWlanE, 2, RTWlanE.Service, RTWlanE.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[DELL8723de.ndi.NT.HW]
Include = netvwifibus.inf
Needs = VWiFiBus.PnPFilterRegistration.Hw
AddReg = RTWlanE.MSI.AddReg

;;****************************************************************************
;; OS relative registry
;;****************************************************************************
;;----------------------------------------------------------------------------
;; NDIS Common Parameters
;;----------------------------------------------------------------------------
[NDIS_64.reg]
HKR, Ndi,                       Service,    0, "RTWlanE"
HKR, Ndi\Interfaces,		UpperRange, 0, "ndis5,mdcwifi,wifipro"
HKR, Ndi\Interfaces,		LowerRange, 0, "wlan,ethernet,vwifi"
;;----------------------------------------------------------------------------
;; RTWLAN Common Parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]
HKR,defaults,			AH_BcnIntv, 	0, "1000"

HKR,Ndi\params\AH_BcnIntv, 	default, 	0, "100"
HKR,Ndi\params\AH_BcnIntv,	ParamDesc, 	0, %AH_BCNINTV_STR%
HKR,Ndi\params\AH_BcnIntv, 	type, 		0, "int"
HKR,Ndi\params\AH_BcnIntv, 	min, 		0, "20"
HKR,Ndi\params\AH_BcnIntv, 	max, 		0, "1000"
HKR,Ndi\params\AH_BcnIntv, 	step, 		0, "1"

HKR,Ndi\params\Dot11dEnable,        ParamDesc,  0, %DOT11_ENABLE_STR%
HKR,Ndi\params\Dot11dEnable,        type,       0, "enum"
HKR,Ndi\params\Dot11dEnable,        default,    0, "0"
HKR,Ndi\params\Dot11dEnable\enum,   "0",        0, %DISABLE_STR%
HKR,Ndi\params\Dot11dEnable\enum,   "1",        0, %ENABLE_STR%

HKR,defaults,Dot11dEnable,0,"0"
HKR,,Dot11dEnable,0,"0"

HKR,Ndi\params\PreambleMode,        ParamDesc,  0, %PREAMBLE_MODE_STR%
HKR,Ndi\params\PreambleMode,        type,       0, "enum"
HKR,Ndi\params\PreambleMode,        default,    0, "2"
HKR,Ndi\params\PreambleMode\enum,   "1",        0, %LONG_PREAMBLE_STR%
HKR,Ndi\params\PreambleMode\enum,   "2",        0, %LONG_SHORT_PREAMBLE_STR%

HKR,defaults,PreambleMode,0,"2"
HKR,,PreambleMode,0,"2"

;; For WiFi test, 1: WiFi Config and 0: Performance Config
HKR,defaults,WiFiConfg,0,"0"
HKR,,WiFiConfg,0,"0"

HKR,defaults,bLeisurePs,0,"2"
HKR,,bLeisurePs,0,"2"
HKR,,bFwCtrlLPS,0,"1"
;; LPS Interval
HKR,,LPSIntvl,0,"5"
;; LPS synchronize mechanism
HKR,,bProtectLps,0,"1"

;; RF Off
;HKR,defaults,HwSwRfOffD3,0,"0"
HKR,,HwSwRfOffD3,0,"0"

;; Tx early mode
HKR,,bEarlymodeEnable,0,"0"

;; RTD3
HKR,,RTD3Enable,0,"0"

;; ASPM
HKR,defaults,PciASPM,0,"5"
HKR,,PciASPM,0,"5"

;; Delay selection for clock request to EPHY
HKR,defaults,ClkDelayToEphy,0,"1"
HKR,,ClkDelayToEphy,0,"1"

;Keep Alive Mechanism
HKR,,KeepAliveLevel,0,"1"

HKR,,SupportPNPCapabilities,0,"1"

;;Define enable status of each RT Bug Check IDs
HKR,,BugCheckIdLogEnConfig,0x10001,0x7FFF

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

HKR,defaults,RxSC,0,"0"
HKR,,RxSC,0,"0"

HKR,defaults,TxSC,0,"0"
HKR,,TxSC,0,"0"

HKR,defaults,BINumber,0,"10"
HKR,,BINumber,0,"10"

HKR,,Locale,0,%LOCALE_STR%

;; ASPM Support
HKR,,ClkReqSupport,0,"2"
HKR,,L0sSupport,0,"2"
HKR,,L1Support,0,"2"
HKR,,L1OffSupport,0,"0"

;; Packet Drop Mechanism
HKR,,PacketDrop,0,"1"

;; Adaptivity DM
HKR,,DynamicLinkAdaptivity,0,"0"

;; Fix Tx/Rx hang
HKR,defaults,RuntimeResetDMA,0,"1"
HKR,,RuntimeResetDMA,0,"1"

;; PCI ignore EIOS
HKR,defaults,PciIgnoreEIOS,0,"1"
HKR,,PciIgnoreEIOS,0,"1"

;; Rx reorder pending time
HKR,,RxReorder_PendTime,0,"100"

;; Enable SMBIOS parsing Processor ID
HKR,,LoadProcessorIDfromSMBIOS,0,"1"

HKR,defaults,PHYParaFromFolder,0,"0"
HKR,,PHYParaFromFolder,0,"0"

;; TxSuspectedFrameHandler
HKR,defaults,bEnableFrameAbort,0,"1"
HKR,,bEnableFrameAbort,0,"1"

;;DfsChnlScanTypeMonitorTime
HKR,,DfsChnlScanTypeMonitorTime,0x10001,0x00000060
;;Get pci bus information
HKR,,GetPciInfo,0,"0"

;;LiveKernelDump
HKR,,LKDSupport,0,"1"

;; ECSA Capability in WDI
HKR,,SupportECSA,0,"1"

;; ECSA Feature Enable
HKR,,ECSAMiracast,0,"1"

;; RoamingSensitivity default setting medium
HKR,,RegROAMSensitiveLevel,0,"70"

;; ConcurrentOpPref
HKR,Ndi\params\ConcurrentOpPref, 		ParamDesc, 	0, "Concurrent Operation Preference"
HKR,Ndi\params\ConcurrentOpPref, 		type, 		0, "enum"
HKR,Ndi\params\ConcurrentOpPref, 		default, 	0, "1"
HKR,Ndi\params\ConcurrentOpPref\enum, 	"0", 		0, "No Preference"
HKR,Ndi\params\ConcurrentOpPref\enum, 	"1", 		0, "2.4GHz Single Channel Operation"
HKR,defaults,ConcurrentOpPref, 0, "1"
HKR,,ConcurrentOpPref, 0, "1"

;;UIF EventLog
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession, Start, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession, GUID, 0x00000000,{810F5633-19B2-4BC7-BB98-5574411A7053}
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession, Start, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession, BufferSize, 0x00010001, 0x50
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession, LogFileMode, 0x00010001, 0x2
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession, MaxFileSize, 0x00010001, 0x8
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession, MaximumBuffers, 0x00010001, 0x10
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession, MinimumBuffers, 0x00010001, 0x2
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7b99cac3-85da-419b-a46d-452d9e1d1659}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7b99cac3-85da-419b-a46d-452d9e1d1659}, EnableLevel, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7b99cac3-85da-419b-a46d-452d9e1d1659}, EnableFlags, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7b99cac3-85da-419b-a46d-452d9e1d1659}, Status, 0x00010001, 0x0

;; Repro mode
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WiFiDriverIHVSessionRepro, Start, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WiFiDriverIHVSessionRepro\{0d520601-c0c1-4a23-a8d0-cc5b8ac77517}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WiFiDriverIHVSessionRepro\{0d520601-c0c1-4a23-a8d0-cc5b8ac77517}, EnableLevel, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WiFiDriverIHVSessionRepro\{0d520601-c0c1-4a23-a8d0-cc5b8ac77517}, EnableFlags, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WiFiDriverIHVSessionRepro\{0d520601-c0c1-4a23-a8d0-cc5b8ac77517}, Status, 0x00010001, 0x0

;;----------------------------------------------------------------------------
;; RTWLAN Common Parameters needs be remove before install new driver
;;----------------------------------------------------------------------------
[DelRTLWLAN.reg]
;; Antenna Diversity
HKR,,AntDivSel
HKR,,PhydmSelectAntenna
HKR, Ndi\params\AntDivSel
HKR, Ndi\params\PhydmSelectAntenna

;; Wireless Mode
HKR,,WirelessMode
HKR, Ndi\params\WirelessMode

;; Remove for mcc
HKR,Ndi\params\MultiChannelFcsMode
HKR,defaults,MultiChannelFcsMode
HKR,,MultiChannelFcsMode

;; Remove for ConcurrentOpPref
HKR,Ndi\params\ConcurrentOpPref
HKR,defaults,ConcurrentOpPref
HKR,,ConcurrentOpPref

;; Remove for IntrMit
HKR,,CapOfIntMit

HKR,,bAdvancedLPs
HKR,,RFType
HKR,,RefClkAutoK
HKR,,EmacDelayValue
HKR,,CmuDelayValue
HKR,,ClkDelayCount8723D
HKR,,bEarlymodeEnable
HKR,,RTD3Enable

HKR,,StbcCap
HKR, Ndi\params\StbcCap

HKR,,LdpcCap
HKR, Ndi\params\LdpcCap

HKR,,AMfactor
HKR, Ndi\params\AMfactor

HKR,,RFEType
HKR, Ndi\params\RFEType

;; WoWLAN
HKR,,PnpKeepLink
HKR,,*WakeOnMagicPacket
HKR,,*WakeOnPattern
HKR,,*PacketCoalescing
HKR,,ARPOffloadEnable
HKR,,GTKOffloadEnable
HKR,,NSOffloadEnable
HKR,,D2ListenIntvl
HKR,,NLOEnable
HKR,,WakeOnDisconnect
HKR,,WoWLANLPSLevel
HKR,,WoWLANPSMode
HKR, Ndi\params\*WakeOnMagicPacket
HKR, Ndi\params\*WakeOnPattern
HKR, Ndi\params\ARPOffloadEnable
HKR, Ndi\params\GTKOffloadEnable
HKR, Ndi\params\NSOffloadEnable
HKR, Ndi\params\WakeOnDisconnect
;;RoamingAggressiveness
HKR,,RegROAMSensitiveLevel
HKR, Ndi\params\RegROAMSensitiveLevel
;; Prefer Band
HKR,,PreferBand
HKR, Ndi\params\PreferBand

[DymcFastEDCA.reg]
HKR,,DymcFastEDCA,0,"1"
;;----------------------------------------------------------------------------
;; Roaming Sensitivity Level Parameters
;;----------------------------------------------------------------------------
[RoamingSensitivity.reg]
HKR,,RegROAMSensitiveLevel,0,"80"
HKR,Ndi\Params\RegROAMSensitiveLevel, ParamDesc, 0, %ROAMING_SENSITIVITY_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel, Type,      0, "enum"
HKR,Ndi\Params\RegROAMSensitiveLevel, Default,   0, "80"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "127",  0, %DISABLE_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "65",  0, %HIGH_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "70",  0, %MIDDLE_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "80",  0, %LOW_STR%

[NonRoamingSensitivity.reg]
HKR,,RegROAMSensitiveLevel,0,"127"

;;----------------------------------------------------------------------------
;; Roaming selection
;;----------------------------------------------------------------------------
[NECRoamingAlog.reg]
HKR,,RoamAlgo,0,"1"
HKR,,RoamCase,0,"1"

;;----------------------------------------------------------------------------
;; Roaming Sensitivity Level Like Intel Parameters
;;----------------------------------------------------------------------------
[RoamingAggressiveness.reg]
HKR,,RegROAMSensitiveLevel,0,"60"
HKR,Ndi\Params\RegROAMSensitiveLevel, ParamDesc, 0, "Roaming Aggressiveness"
HKR,Ndi\Params\RegROAMSensitiveLevel, Type,      0, "enum"
HKR,Ndi\Params\RegROAMSensitiveLevel, Default,   0, "60"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "40",  0, "6. Highest"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "50",  0, "5. Medium-High"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "60",  0, "4. Medium"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "70",  0, "3. Medium-Low"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "80",  0, "2. Lowest"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "127",  0, "1. Disable"

[DelRoamingAggressiveness.reg]
HKR,,RegROAMSensitiveLevel
HKR, Ndi\params\RegROAMSensitiveLevel


[NECRoamingAggressiveness.reg]
HKR,,RegROAMSensitiveLevel,0,"60"
HKR,Ndi\Params\RegROAMSensitiveLevel, ParamDesc, 0, "Roaming Aggressiveness"
HKR,Ndi\Params\RegROAMSensitiveLevel, Type,      0, "enum"
HKR,Ndi\Params\RegROAMSensitiveLevel, Default,   0, "60"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "40",  0, "6. Highest"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "50",  0, "5. Medium-High"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "60",  0, "4. Medium"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "70",  0, "3. Medium-Low"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "80",  0, "2. Lowest"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "127",  0, "1. Disable"

[NECDelRoamingAggressiveness.reg]
HKR,,RegROAMSensitiveLevel
HKR, Ndi\params\RegROAMSensitiveLevel

;FUJITSU delete Reg for old ChkRdTO
[FJT8822beDelLBC.reg]
HKR,,ChkRdTO
HKR, Ndi\params\ChkRdTO

;FUJITSU check lbc watchdog timeout
[FJT8822be_LBC.reg]
HKR,,New_ChkRdTO,0,"1"

[DelRegFujitsuRS5Inbox.reg]
;;[TxPwrLevel.reg]
HKR,,TxPwrLevel
HKR,Ndi\params\TxPwrLevel

;;[ProtectionMode.reg]
;; Mix protection mode
HKR,,ProtectionMode
HKR,Ndi\params\ProtectionMode

;;[FatChannelIntolerant.reg]
HKR,,b40Intolerant
HKR,Ndi\params\b40Intolerant



[RxinterruptWorkitem.reg]
HKR,defaults,UseRxInterruptWorkItem,0,"1"
HKR,,UseRxInterruptWorkItem,0,"1"

;;----------------------------------------------------------------------------
;; Wireless Mode Related Parameters
;;----------------------------------------------------------------------------
[11nWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %AUTO_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

;; 40MHz Support in 11n
HKR,Ndi\params\BWSetting, 			ParamDesc, 	0, "Bandwidth"
HKR,Ndi\params\BWSetting, 			type, 		0, "enum"
HKR,Ndi\params\BWSetting, 			default, 	0, "1"
HKR,Ndi\params\BWSetting\enum, 		"0", 		0, "20MHz Only"
HKR,Ndi\params\BWSetting\enum, 		"1", 		0, "20_40MHz"
HKR,defaults,BWSetting,0,"1"
HKR,,BWSetting,0,"1"
HKR,,BWSetting,,"1"

HKR,,Channel,0,"10"

[11nAdvancedWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "6"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, "1. 802.11b"
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, "2. 802.11g"
HKR,Ndi\params\WirelessMode\enum, 	"6", 		0, "3. 802.11b/g"
HKR,defaults,WirelessMode, 0, "6"
HKR,,WirelessMode, 0, "6"

HKR,Ndi\params\HTMode, 				ParamDesc, 	0, "HT mode"
HKR,Ndi\params\HTMode, 				type, 		0, "enum"
HKR,Ndi\params\HTMode, 				default, 	0, "2"
HKR,Ndi\params\HTMode\enum, 		"1", 		0, %DISABLE_STR%
HKR,Ndi\params\HTMode\enum, 		"2", 		0, %ENABLE_STR%
HKR,defaults,HTMode, 0, "2"
HKR,,HTMode, 0, "2"

;; Channel width for 2.4G
HKR,Ndi\params\BW40MHzFor2G, 			ParamDesc, 	0, "802.11n channel width for 2.4GHz"
HKR,Ndi\params\BW40MHzFor2G, 			type, 		0, "enum"
HKR,Ndi\params\BW40MHzFor2G, 			default, 	0, "1"
HKR,Ndi\params\BW40MHzFor2G\enum, 		"0", 		0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor2G\enum, 		"1", 		0, "Auto"
HKR,defaults,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,,"1"


HKR,,BWSetting,0,"1"
HKR,,BWSetting,,"1"

HKR,,Channel,0,"10"

[11gWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %AUTO_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"

HKR,,BWSetting,0,"0"

HKR,,Channel,0,"10"

[11agnWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %AUTO_STR%
HKR,Ndi\params\WirelessMode\enum, 	"1", 		0, %IEEE_802_11A_STR%
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"16", 		0, %IEEE_802_11BGN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"32", 		0, %IEEE_802_11AN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

HKR,,BWSetting,0,"1"

[11acWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %AUTO_STR%
HKR,Ndi\params\WirelessMode\enum, 	"1", 		0, %IEEE_802_11A_STR%
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"16", 		0, %IEEE_802_11BGN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"32", 		0, %IEEE_802_11AN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"64", 		0, %IEEE_802_11ANAC_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

HKR,,Channel,0,"36"

;; RFE Enable
HKR,,EnRFEType,0,"1"

HKR,defaults,BWSetting,0,"2"
HKR,,BWSetting,0,"2"

[5GpassiveScan.reg]
HKR,,5GPassiveScan,0,"1"

[80MHzBandwidth.reg]
HKR,Ndi\params\BWSetting,        ParamDesc,  0, "Bandwidth"
HKR,Ndi\params\BWSetting,        type,       0, "enum"
HKR,Ndi\params\BWSetting,        default,    0, "2"
HKR,Ndi\params\BWSetting\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BWSetting\enum,   "1",        0, "40_20MHz"
HKR,Ndi\params\BWSetting\enum,   "2",        0, "80_40_20MHz"
HKR,defaults,BWSetting,0,"2"
HKR,,BWSetting,0,"2"

[PKTMDisable.reg]
HKR,,TxPktTranEnable,0,"0"

[FakeGCEnable.reg]
HKR,,SupportFakeGC,0,"1"

[11acAdvancedWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "7"
HKR,Ndi\params\WirelessMode\enum, 	"1", 		0, "1. 802.11a"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, "2. 802.11b"
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, "3. 802.11g"
HKR,Ndi\params\WirelessMode\enum, 	"6", 		0, "4. 802.11b/g"
HKR,Ndi\params\WirelessMode\enum, 	"5", 		0, "5. 802.11a/g"
HKR,Ndi\params\WirelessMode\enum, 	"7", 		0, "6. 802.11a/b/g"
HKR,defaults,WirelessMode, 0, "7"
HKR,,WirelessMode, 0, "7"

HKR,Ndi\params\HTMode, 				ParamDesc, 	0, "HT mode"
HKR,Ndi\params\HTMode, 				type, 		0, "enum"
HKR,Ndi\params\HTMode, 				default, 	0, "4"
HKR,Ndi\params\HTMode\enum, 		"1", 		0, %DISABLE_STR%
HKR,Ndi\params\HTMode\enum, 		"2", 		0, "HT mode"
HKR,Ndi\params\HTMode\enum, 		"4", 		0, "VHT mode"
HKR,defaults,HTMode, 0, "4"
HKR,,HTMode, 0, "4"


;; Channel width foe 2.4G
HKR,Ndi\params\BW40MHzFor2G, 			ParamDesc, 	0, "802.11n channel width for 2.4GHz"
HKR,Ndi\params\BW40MHzFor2G, 			type, 		0, "enum"
HKR,Ndi\params\BW40MHzFor2G, 			default, 	0, "1"
HKR,Ndi\params\BW40MHzFor2G\enum, 		"0", 		0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor2G\enum, 		"1", 		0, "Auto"
HKR,defaults,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,,"1"

;; Channel width foe 5G
HKR,Ndi\params\BW40MHzFor5G, 			ParamDesc, 	0, "802.11n channel width for 5.2GHz"
HKR,Ndi\params\BW40MHzFor5G, 			type, 		0, "enum"
HKR,Ndi\params\BW40MHzFor5G, 			default, 	0, "1"
HKR,Ndi\params\BW40MHzFor5G\enum, 		"0", 		0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor5G\enum, 		"1", 		0, "Auto"
HKR,defaults,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,,"1"

HKR,,Channel,0,"36"

;; RFE Enable
HKR,,EnRFEType,0,"1"

HKR,defaults,BWSetting,0,"2"
HKR,,BWSetting,0,"2"

;; Prefer Band
HKR,Ndi\params\PreferBand, 			ParamDesc, 	0, "Preferred Band"
HKR,Ndi\params\PreferBand, 			default, 	0, "0"
HKR,Ndi\params\PreferBand, 			type, 		0, "enum"
HKR,Ndi\params\PreferBand\enum, 	"0", 		0, "1. No Preference"
HKR,Ndi\params\PreferBand\enum, 	"1", 		0, "2. 2.4G first"
HKR,Ndi\params\PreferBand\enum, 	"2", 		0, "3. 5G first"
HKR,,PreferBand,0,"0"


[PreferBand5G.reg]
;; Prefer Band
HKR,Ndi\params\PreferBand, 			ParamDesc, 	0, "Preferred Band"
HKR,Ndi\params\PreferBand, 			default, 	0, "0"
HKR,Ndi\params\PreferBand, 			type, 		0, "enum"
HKR,Ndi\params\PreferBand\enum, 	"0", 		0, "1. No Preference"
HKR,Ndi\params\PreferBand\enum, 	"1", 		0, "2. 2.4G first"
HKR,Ndi\params\PreferBand\enum, 	"2", 		0, "3. 5G first"
HKR,,PreferBand,0,"2"

[PreferBand5G_NewMethod.reg]
;;PreferBand set to "5G first"
HKR,,PreferBand,0,"2"
;;Use New PreferBand method
HKR,,PreferBestRSSI,0,"0"
HKR,,EnableRSSITH,0,"1"

;;----------------------------------------------------------------------------
;; Indonesia new band support setting (Registry key IdnBandSupport):
;;   0(RT_IDN_BAND_SUPPORT_5115_5350_DIS): Set 5.115-5.35GHz(band1, band2) to Disable in Indonesia (Default in driver)
;;   1(RT_IDN_BAND_SUPPORT_5115_5350_EN): Set 5.115-5.35GHz(band1, band2) to Enable in Indonesia
;;   2(Auto mode): Determine whether to support band1, band2 by evaluating ACPI _DSM method
;;----------------------------------------------------------------------------
[IdnNewBandSupport.reg]
;; Force to support Indonesia new band
HKR,,IdnBandSupport,0,"1"

[IdnNewBandSupByPltfm.reg]
;; Set Indonesia new band support as auto mode to determine by evaluating ACPI _DSM method
HKR,,IdnBandSupport,0,"2"

;;----------------------------------------------------------------------------
;; 11AC series IC VHT 2.4G Support
;;----------------------------------------------------------------------------
[VHT24G.reg]
HKR,Ndi\params\Vht24g, 		ParamDesc, 	0, "VHT 2.4G IOT"
HKR,Ndi\params\Vht24g, 		type, 		0, "enum"
HKR,Ndi\params\Vht24g, 		default, 	0, "255"
HKR,Ndi\params\Vht24g\enum, 	"0", 		0, "Disable"
HKR,Ndi\params\Vht24g\enum, 	"255", 		0, "Enable"
HKR,Ndi\params\Vht24g\enum, 	"254", 		0, "Not support Broadcom vendor"
HKR,defaults,Vht24g, 0, "255"
HKR,,Vht24g, 0, "255"

;;----------------------------------------------------------------------------
;; ADHOC Related Parameters
;;----------------------------------------------------------------------------
[11nAdhoc.reg]
HKR,Ndi\params\11nAdhoc,        ParamDesc,  0, %11NADHOC_ENABLE_STR%
HKR,Ndi\params\11nAdhoc,        type,       0, "enum"
HKR,Ndi\params\11nAdhoc,        default,    0, "0"
HKR,Ndi\params\11nAdhoc\enum,   "0",        0, %DISABLE_STR%
HKR,Ndi\params\11nAdhoc\enum,   "1",        0, %ENABLE_STR%
HKR,defaults,11nAdhoc,0,"0"
HKR,,11nAdhoc,0,"0"
;;----------------------------------------------------------------------------
;; MSI Control Parameters
;;----------------------------------------------------------------------------
[MSIEnable.reg]
HKR,,MSISupport,0,"1"
[MSIDisable.reg]
HKR,,MSISupport,0,"0"
;;----------------------------------------------------------------------------
;; WOWLAN Control Parameters
;;----------------------------------------------------------------------------
[WowlanEnable.reg]
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"
HKR,,*WakeOnMagicPacket,0,"1"
HKR,,*WakeOnPattern,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

[WowlanDisable.reg]
HKR,,ARPOffloadEnable,0,"0"
HKR,,GTKOffloadEnable,0,"0"
HKR,,WoWLANPSMode,0,"0"

[WowlanEnableNoPatternMatch.reg]
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"
HKR,,*WakeOnMagicPacket,0,"1"
HKR,,*WakeOnPattern,0,"0"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "0"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

;; Wake on disconnect (0: disable Wake-on(enable Sleep), 1: enable Wake-on(disable Sleep))
;; Only add this add-registry-section if WoWlan is enabled.
[SleepOnDisconnectDisable.reg]
HKR,,WakeOnDisconnect,0,"1"
HKR, Ndi\params\WakeOnDisconnect,             ParamDesc,  0, %SleepOnDisconnect%
HKR, Ndi\params\WakeOnDisconnect,             default,    0, "1"
HKR, Ndi\params\WakeOnDisconnect,             type,       0, "enum"
HKR, Ndi\params\WakeOnDisconnect\enum,        "1",        0, %DISABLE_STR%
HKR, Ndi\params\WakeOnDisconnect\enum,        "0",        0, %ENABLE_STR%

[ConnectedStandbyEnable.reg]
; AOAC reconnect
HKR,,PnpKeepLink,0,"1"

HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"
HKR,,D2ListenIntvl,0,"5"
HKR,,NSOffloadEnable,0,"1"
HKR,,NLOEnable,0,"1"
HKR,,*WakeOnMagicPacket,0,"1"
HKR,,*WakeOnPattern,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

;; Packet coalescing should be enabled in WHCK test
HKR,defaults,*PacketCoalescing,0,"0"
HKR,,*PacketCoalescing,0,"0"

[ModernStandbyEnable.reg]
; AOAC reconnect
HKR,,PnpKeepLink,0,"1"
HKR,,AlwaysStandby,0,"1"

HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"
HKR,,D2ListenIntvl,0,"5"
HKR,,NSOffloadEnable,0,"1"
HKR,,NLOEnable,0,"1"
HKR,,*WakeOnMagicPacket,0,"1"
HKR,,*WakeOnPattern,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

;; Packet coalescing should be enabled in WHCK test
HKR,defaults,*PacketCoalescing,0,"0"
HKR,,*PacketCoalescing,0,"0"

;;----------------------------------------------------------------------------
;; Earlymode Control Parameters
;;----------------------------------------------------------------------------
[EarlyModeEnable.reg]
HKR,,bEarlymodeEnable,0,"1"
[EarlyModeDisable.reg]
HKR,,bEarlymodeEnable,0,"0"
;;----------------------------------------------------------------------------
;; LPS OnOFF Parameters
;;----------------------------------------------------------------------------
;Leisure Power Save
[LPSEnable.reg]
HKR,defaults,bLeisurePs,0,"1"
HKR,,bLeisurePs,0,"1"

[LPSDisable.reg]
HKR,defaults,bLeisurePs,0,"0"
HKR,,bLeisurePs,0,"0"

[LPSAuto.reg]
HKR,defaults,bLeisurePs,0,"2"
HKR,,bLeisurePs,0,"2"

;;----------------------------------------------------------------------------
;; WoWLAN PS Mode
;;----------------------------------------------------------------------------
;; No Power Saving
[WowlanPSModeAllDisable.reg] 
HKR,,WoWLANPSMode,0,"0"

;; LPS 32K
[WowlanPSModeLPS32k.reg]
HKR,,WoWLANPSMode,0,"2"

;; LPS 32K + FW IPS
[WowlanPSModeAllEnable.reg]
HKR,,WoWLANPSMode,0,"6"

;; LPS PG + FW IPS
[WowlanPSModeAllEnablePG.reg]
HKR,,WoWLANPSMode,0,"14"

;;----------------------------------------------------------------------------
;; LPS Control Parameters
;;----------------------------------------------------------------------------
[FWLPSEnable.reg]
HKR,,bFwCtrlLPS,0,"1"
[FWLPSDisable.reg]
HKR,,bFwCtrlLPS,0,"0"

;;----------------------------------------------------------------------------
;; LPS Option
;;----------------------------------------------------------------------------
[DisableIMPSWA.reg]
HKR,,DisableIMPS,0,"1"

;;----------------------------------------------------------------------------
;; LPS 32k Control Parameters
;;----------------------------------------------------------------------------
[32kEnable.reg]
HKR,,bLowPowerEnable,0,"1"
[32kDisable.reg]
HKR,,bLowPowerEnable,0,"0"

;;----------------------------------------------------------------------------
;; LPS PG Control Parameters
;;----------------------------------------------------------------------------
[PGEnable.reg]
HKR,,bLPS_PG_En,0,"1"
[PGDisable.reg]
HKR,,bLPS_PG_En,0,"0"
;;----------------------------------------------------------------------------
;; IPS OnOFF Parameters
;;----------------------------------------------------------------------------
;Inactive Power Save
[IPSEnable.reg]
HKR,defaults,InactivePs,0,"1"
HKR,,InactivePs,0,"1"

[IPSDisable.reg]
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"

[IPSAuto.reg]
HKR,defaults,InactivePs,0,"2"
HKR,,InactivePs,0,"2"
;;----------------------------------------------------------------------------
;; RTD3 Control Parameters
;;----------------------------------------------------------------------------
[RTD3Enable.reg]
HKR,,RTD3Enable,0,"1"

HKR,Ndi\params\RTD3Enable, 			ParamDesc, 	0, "Runtime D3"
HKR,Ndi\params\RTD3Enable, 			default, 	0, "1"
HKR,Ndi\params\RTD3Enable, 			type, 		0, "enum"
HKR,Ndi\params\RTD3Enable\enum, 	"0", 		0, "Disabled"
HKR,Ndi\params\RTD3Enable\enum, 	"1", 		0, "Enabled"

[RTD3Disable.reg]
HKR,,RTD3Enable,0,"0"
;;----------------------------------------------------------------------------
;; TCP Reorder Control Parameters
;;----------------------------------------------------------------------------
[TcpReorderEnable.reg]
HKR,,TcpReorder,0,"1"
[TcpReorderDisable.reg]
HKR,,TcpReorder,0,"0"
;;----------------------------------------------------------------------------
;; Go Move to STA Parameters
;;----------------------------------------------------------------------------
[GoMoveToStaEnable.reg]
HKR,,bGoMoveToSta,0,"1"
;;----------------------------------------------------------------------------
;;GO prefer setting
;;----------------------------------------------------------------------------
[GOPreferMode.reg]
;; Enable Op Ch Select(BIT0: Enable, BIT1: follow 2G, BIT2: follow 5G)
HKR,,OpChSelect,0,"7"

;; GO Op ch Prefer list
HKR,,OpChnlList,0,"36,40,44,48,149,153,157,161,165,169,52,56,60,64,100,104,108,112,116,120,124,128,132,136,140,6,11,1,2,3,4,5,7,8,9,10"
;;----------------------------------------------------------------------------
;; LDPC, STBC  Parameters
;;----------------------------------------------------------------------------
[LDPCEnable.reg]
HKR,,LdpcCap,0,"48"

[LDPCDisable.reg]
HKR,,LdpcCap,0,"0"

[STBCEnable.reg] 
HKR,,StbcCap,0,"48"

[STBCDisable.reg] 
HKR,,StbcCap,0,"0"

[STBCHTRxEnable.reg] 
HKR,,StbcCap,0,"16"

;; ECS switch on system scan
[ECS_SUPPORT_SWITCH_ON.reg]
HKR,,ECSSupport,0,"1"

;; ECS switch on setting
[ECS_SUPPORT_P2P_ON.reg]
HKR,,ECSSupport,0,"2"

[ECS_SUPPORT_SCAN_P2P_ON.reg]
HKR,,ECSSupport,0,"3"

[ECS_Skype_TrafficDectect_ON.reg]
HKR,,ECSSkypeDetect,0,"1"

;; ECS switch on RSSI roaming scan
[ECS_SUPPORT_RSSI_ROAMING_SCAN_SWITCH_ON.reg]
HKR,,ECSSupport,0,"16"

;; NEC ECS setting
[NEC_ECS_SETTING.reg]
HKR,,ECSSupport,0,"17"

;; ECS_SUPPORT_SCAN_P2P_ON + ECS RM SCAN
[ECS_SUPPORT_SCAN_P2P_ON_AND_RM.reg]
HKR,,ECSSupport,0,"35"

[Enable_PA_Recover.reg]
HKR,,AutoEnPA,0,"1"


[LNV_Skip_p2p_discover.reg]
HKR,,P2PDiscoverSkipCondition,0,"0x3"

[LNV_MCC_control_by_ECS.reg]
HKR,,MCCControlbyECS,0,"0x2"


;; extend passive scan channel list for FUJITSU
[FJT_EXTEND_PASSIVE_SCAN_CHNL_LIST.reg]
HKR,,CustChnlList,0,"12,13"

;; extend passive scan channel list for NEC
[NEC_EXTEND_PASSIVE_SCAN_CHNL_LIST.reg]
HKR,,CustChnlList,0,"52,60,100,108,116,124,132,140"

[AddExtCh.reg]
HKR,,AddExtCh,0,"1"

[SupportTxFeedback.reg]
HKR,,SupportTxFeedback,0,"1"

[EnableScanTimerActionTimer.reg]
HKR,,ScanTimerType,0,"1"

[EnableProbeReqTxFeedback.reg]
HKR,,probereqTxfeedback,0,"1"

[1SS_TXMODE_PATH_A_SEL.reg]
HKR,,1ssTXMode,0,"1"

[ScanTh.reg]
HKR,,ScanTh,0,"28"

[AuthTimeoutPLDREn.reg]
HKR,,AuthTimeoutPLDREn,0,"1"
;;----------------------------------------------------------------------------
;; Tx PowerTable Dump Feature
;;----------------------------------------------------------------------------
[EnableTxPowerTableDump.reg]
HKR,,SupportTxPwrTableDump,0,"1"

;;----------------------------------------------------------------------------
;; Tx PowerTable Load From Single File Feature
;;----------------------------------------------------------------------------
[EnableTxPowerTableFromSingleFile.reg]
HKR,,TxPwrLmtTableFromSingleFile,0,"1"

;; Enable dynamically reload Tx power limit table by current determined regulation (FCC/IC)
[EnableDynamicReloadTxPwrLmtTableByRegulation.reg]
HKR,,DynamicReloadTxPwrLmtTableByRegulation,0,"1"

;; Specify HP 8723BE Tx Power limit table ID as 00003 (Increase 11b(CCK) Tx power to 16dBm)
[SpecifyHP8723beTxPwrLmtTableID.reg]
HKR,,ForcedCustomTxPwrLmtTableID,0,"3"

;; Specify HP 8188EE Tx Power limit table ID as 00004 (Increase 11b(CCK) Tx power to 16dBm)
[SpecifyHP8188eeTxPwrLmtTableID.reg]
HKR,,ForcedCustomTxPwrLmtTableID,0,"4"

;; Specify 8821CE Tx Power limit table ID as 00009 (For Ukraine)
[Specify8821ceTxPwrLmtTableID_UpdateUkraine.reg]
HKR,,SupportTxPwrTableDump,0,"1"
HKR,,TxPwrLmtTableFromSingleFile,0,"1"
HKR,,ForcedCustomTxPwrLmtTableID,0,"9"

;; Specify 8822BE Tx Power limit table ID as 00010 (For Ukraine)
[Specify8822beTxPwrLmtTableID_UpdateUkraine.reg]
HKR,,SupportTxPwrTableDump,0,"1"
HKR,,TxPwrLmtTableFromSingleFile,0,"1"
HKR,,ForcedCustomTxPwrLmtTableID,0,"10"

;; Specify 8821CE Tx Power limit table ID as 00027 (For ASUS FCC bandedge request)
[Specify8821ceTxPwrLmtTableID_27.reg]
HKR,,SupportTxPwrTableDump,0,"1"
HKR,,TxPwrLmtTableFromSingleFile,0,"1"
HKR,,ForcedCustomTxPwrLmtTableID,0,"27"

;;----------------------------------------------------------------------------
;; Transmit Power Control (TPC) Support
;;----------------------------------------------------------------------------
[TPC_Support.reg]
HKR,Ndi\params\TPCEnable,        ParamDesc,  0, "TPCEnable"
HKR,Ndi\params\TPCEnable,        type,       0, "enum"
HKR,Ndi\params\TPCEnable,        default,    0, "0"
HKR,Ndi\params\TPCEnable\enum,   "0",        0, "TPC Disable"
HKR,Ndi\params\TPCEnable\enum,   "1",        0, "ETSI Enable"
HKR,Ndi\params\TPCEnable\enum,   "2",        0, "MKK Enable"
HKR,Ndi\params\TPCEnable\enum,   "4",        0, "FCC Enable"
HKR,Ndi\params\TPCEnable\enum,   "8",        0, "WW Enable"
HKR,Ndi\params\TPCEnable\enum,   "15",        0, "Enable All"
HKR,defaults,TPCEnable,0,"0"
HKR,,TPCEnable,0,"0"

HKR,Ndi\params\TxPowerControl,        ParamDesc,  0, "TxPowerControl"
HKR,Ndi\params\TxPowerControl,        type,       0, "enum"
HKR,Ndi\params\TxPowerControl,        default,    0, "0"
HKR,Ndi\params\TxPowerControl\enum,   "0",        0, "100%%"
HKR,Ndi\params\TxPowerControl\enum,   "1",        0, "50%%"
HKR,Ndi\params\TxPowerControl\enum,   "2",        0, "0"
HKR,defaults,TxPowerControl,0,"0"
HKR,,TxPowerControl,0,"0"
;;----------------------------------------------------------------------------
;; 8192EE Disable Rx Reset.
;;----------------------------------------------------------------------------
[DisableRxReset.reg]
HKR,,DisableRxHangReset,0,"1"

;;----------------------------------------------------------------------------
;; Default Antenna Control Parameters
;;----------------------------------------------------------------------------
[DefaultAntennaMain.reg]
HKR,,bRegDefaultAntenna,0,"1"
[DefaultAntennaAux.reg]
HKR,,bRegDefaultAntenna,0,"0"
;;----------------------------------------------------------------------------
;; Adaptivity Control Parameters
;;----------------------------------------------------------------------------
[AdaptivityEnable.reg]
HKR,,EnableAdaptivity,0,"1"
[AdaptivityDisable.reg]
HKR,,EnableAdaptivity,0,"0"
;;----------------------------------------------------------------------------
;; Miracast Parameters
;;----------------------------------------------------------------------------
[MiracastDisable.reg]
HKR,,*MiracastSupported,0x10001,0x0
[MiracastEnable.reg]
HKR,,*MiracastSupported,0x10001,0x1

[MiracastScanHandleEnable.reg]
HKR,,MiracastScanHandle,0,"1"
;;----------------------------------------------------------------------------
;; BT HS mode Parameters
;;----------------------------------------------------------------------------
;BT High Speed
[hsForceEnable.reg]
HKR,,btHsMode,0,"1"
[hsForceDisable.reg]
HKR,,btHsMode,0,"0"
;BT lose workaround
[EnableBTWorkaround.reg]
HKR,,EnableBTWorkaround,0,"1"
;S5 power down BT
[BTPowerDown_at_S5.reg]
HKR,,BTPowerDown_at_S5,0,"1"

;;----------------------------------------------------------------------------
;; INT_MIT Parameters
;;----------------------------------------------------------------------------
[IntMitEnable_v1.reg]
HKR,,CapOfIntMit,0x10001,"0x3E"
HKR,,ValIntMitAC,0x10001,"0x0"
HKR,,ValIntMitDCLPS,0x10001,0xAAAA9C40
HKR,,ValIntMitDCLPSNo32k,0x10001,0x00AA9C40
HKR,,ValIntMitDCNonLPS,0x10001,0xAA009C40
HKR,,ValIntMitPing,0x10001,"0x0"
HKR,,ValIntMitFPing,0x10001,"0x0"

[IntMitDisable.reg]
HKR,,CapOfIntMit,0,"0"

;;----------------------------------------------------------------------------
;; FW INT_MIT Parameters
;;----------------------------------------------------------------------------
[IntMitEnable_v2.reg]
HKR,,CapOfIntMit,0,"0"
HKR,,EnableFwIntMtg,0,"1"
HKR,,FwRxBcnCntTH,0,"5"
;;----------------------------------------------------------------------------
;; Advanced LPs Parameters
;;----------------------------------------------------------------------------
[AdvancedLPsEnable.reg]
HKR,,bAdvancedLPs,0,"0"



[AdvancedLPsEnable_v1.reg] 
HKR,,bAdvancedLPs,0,"0"

[AdvancedLPsEnable_v2.reg]
HKR,,bAdvancedLPs,0,"55"

[AdvancedLPsEnable_v3.reg]
HKR,,bAdvancedLPs,0,"243"

[AdvancedLPsEnable_v4.reg]
HKR,,bAdvancedLPs,0,"227"

[MSCommon.reg]
HKR,,bPingPS,0,"0"
HKR,,ForceCTStoSelf,0,"1"
HKR,,LPSDataNum,0,"10"

;;----------------------------------------------------------------------------
;; L0s & L1 Parameters
;;----------------------------------------------------------------------------
[RuntimeL0sL1Enable.reg]
HKR,,RuntimeL0sL1,0,"1"
[RuntimeL0sL1Disable.reg]
HKR,,RuntimeL0sL1,0,"0"

;;----------------------------------------------------------------------------
;; L1 Parameters
;;----------------------------------------------------------------------------
[L1Enable.reg]
HKR,,L1Support,0,"1"
[L1Disable.reg]
HKR,,L1Support,0,"0"

;;----------------------------------------------------------------------------
;; L1 Off Parameters
;;----------------------------------------------------------------------------
[L1OffEnable.reg]
HKR,,L1OffSupport,0,"1"
[L1OffAuto.reg]
HKR,,L1OffSupport,0,"2"
[L1OffDisable.reg]
HKR,,L1OffSupport,0,"0"

;;----------------------------------------------------------------------------
;; L1 busy traffic threshold
;;----------------------------------------------------------------------------
[L1BusyTh5000.reg]
HKR,,L1BusyThreshold,0,"5000"

;;----------------------------------------------------------------------------
;; L2 Power Gating Parameters
;;----------------------------------------------------------------------------
[L2PGEnable.reg]
HKR,,L2PGSupport,0,"1"
[L2PGDisable.reg]
HKR,,L2PGSupport,0,"0"

;;----------------------------------------------------------------------------
;; Ltr Parameters
;;----------------------------------------------------------------------------
[LtrDisable.reg]
HKR,,LtrSupport,0,"0"

[LtrHWAuto.reg]
HKR,,LtrSupport,0,"2"

[LtrSWDCEnable.reg]
HKR,,LtrSupport,0,"3"
;;----------------------------------------------------------------------------
;; Delay eMAC/ePHY Parameters
;;----------------------------------------------------------------------------
[DelayeMACePHY.reg]
HKR,,DelayeMACePHY,0,"1"

[DelayeMACePHY_OFF.reg]
HKR,,DelayeMACePHY,0,"0"
;;----------------------------------------------------------------------------
;; PCI Bridge Parameters
;;----------------------------------------------------------------------------
[GetPciInfoDisable.reg]
HKR,,GetPciInfo,0,"0"
;;----------------------------------------------------------------------------
;; Improve PCI Capability Parameters
;;----------------------------------------------------------------------------
[IpvPciCapEnable.reg]
HKR,,ImprovePciCap,0,"1"
;;----------------------------------------------------------------------------
;; KFREE parameters
;;----------------------------------------------------------------------------
[KFREE_COMMON.reg]
HKR,,RfKFreeEnable,0,"0"
;;----------------------------------------------------------------------------
;; Sniffer parameters
;;----------------------------------------------------------------------------
[AdvSniffer.reg]
HKR,,AdvanceSnifferMode,0,"8"
;;----------------------------------------------------------------------------
;; Reference Clock Auto K function Parameters
;;----------------------------------------------------------------------------
[RefClkAutoKEnable.reg]
HKR,,RefClkAutoK,0,"1"
;;----------------------------------------------------------------------------
;; Transmit Power Level Parameters
;;----------------------------------------------------------------------------

;;----------------------------------------------------------------------------
;; Periodic scan in the IPS mode 
;;----------------------------------------------------------------------------
[Scan_IPS.reg]
HKR,,Scan_IPSEnable,0,"1"
;;----------------------------------------------------------------------------
;; 1RCCA
;;----------------------------------------------------------------------------
[1RCCA.reg]
HKR,,1RCCA,0,"1"
;;----------------------------------------------------------------------------
;; TBTT Shift
;;----------------------------------------------------------------------------
[TBTT_Shift.reg]
HKR,,TBTTShift,0,"2"
;;----------------------------------------------------------------------------
;; Do fwIQK before connection
;;----------------------------------------------------------------------------
[IQKBeforeConnection.reg]
HKR,,IQKBeforeConnection,0,"1"

[InterferenceTest.reg]
HKR,,InterferenceTest,0,"1"

;;----------------------------------------------------------------------------
;; Follow Power Management Enable bit mode.
;;----------------------------------------------------------------------------
[PMEFollow.reg]
HKR,,IgnorePMEMode,0,"0"

[PMEIgnore.reg]
HKR,,IgnorePMEMode,0,"1"

[PMEEfuse.reg]
HKR,,IgnorePMEMode,0,"2"

[ACModeDisable32K.reg]
HKR,,bLeisurePs,0,"1"
HKR,,bRegACModeDisable32k,0,"1"

[DisableLPS.reg]
HKR,,bLeisurePs,0,"0"
HKR,,bLowPowerEnable,0,"0"
HKR,,bLPS_PG_En,0,"0"


;;----------------------------------------------------------------------------
;; FW enhanced Leisure Power Save mechanism
;;----------------------------------------------------------------------------
[EnhanceLPS_Enable.reg]
HKR,,bLPSTuningEnable,0,"1"
;;----------------------------------------------------------------------------
;; Related power Consumption
;;----------------------------------------------------------------------------
[PowerConsumption_8822b.reg]
HKR,,Scan_IPSEnable,0,"1"
HKR,,bAdvancedLPs,0,"243"

HKR,,1RCCA,0,"1"

HKR,,TBTTShift,0,"2"

[PowerConsumption_8822c.reg]

;; LPS Setting
HKR,,bLeisurePs,0,"2"
HKR,,bLowPowerEnable,0,"1"
HKR,,bLPS_PG_En,0,"1"
HKR,,bLPSTuningEnable,0,"1"
HKR,,TBTTShift,0,"2"
HKR,,1RCCA,0,"0"
HKR,,bAdvancedLPs,0,"243"
HKR,,BusyTraffic_TH2,0,"120"
HKR,,BusyTraffic_TH3,0,"200"

;; IPS Setting
HKR,,Scan_IPSEnable,0,"1"

;; Interrupter Mitigation
HKR,,CapOfIntMit,0,"0"
HKR,,EnableFwIntMtg,0,"0"
HKR,,FwRxBcnCntTH,0,"5"

[TxPwrLevel.reg]
HKR,,TxPwrLevel,0,"0"
HKR,Ndi\params\TxPwrLevel, 			ParamDesc, 	0, "Transmit power"
HKR,Ndi\params\TxPwrLevel, 			default, 	0, "0"
HKR,Ndi\params\TxPwrLevel, 			type, 		0, "enum"
HKR,Ndi\params\TxPwrLevel\enum, 	"0", 		0, "5. Highest"
HKR,Ndi\params\TxPwrLevel\enum, 	"1", 		0, "4. Medium-high"
HKR,Ndi\params\TxPwrLevel\enum, 	"2", 		0, "3. Medium"
HKR,Ndi\params\TxPwrLevel\enum, 	"3", 		0, "2. Medium-low"
HKR,Ndi\params\TxPwrLevel\enum, 	"4", 		0, "1. Lowest"
;;----------------------------------------------------------------------------
;; Classroom mode Parameters
;;----------------------------------------------------------------------------
[EnableClassMode.reg]
HKR,,ActingAsClassMode,0,"1"

[Class.reg]
HKR,Ndi\params\ActingAsClassMode,        ParamDesc,  0, "Classroom mode"
HKR,Ndi\params\ActingAsClassMode,        type,       0, "enum"
HKR,Ndi\params\ActingAsClassMode,        default,    0, "0"
HKR,Ndi\params\ActingAsClassMode\enum,   "0",        0, %DISABLE_STR%
HKR,Ndi\params\ActingAsClassMode\enum,   "1",        0, %ENABLE_STR%
HKR,defaults,ActingAsClassMode,0,"0"
HKR,,ActingAsClassMode,0,"0"
;;----------------------------------------------------------------------------
;; B mode OTA Special Patch
;;----------------------------------------------------------------------------
[ApplyBModeOtaPatch.reg]
HKR,,BModeOtaPatch,0,"1"
;;----------------------------------------------------------------------------
;; RSSI to Grid Mode Parameters
;;----------------------------------------------------------------------------
[RSSI2GridRealMode.reg]
HKR,,RSSI2GridMode,0,"1"
[RSSI2GridMode_2.reg]
HKR,,RSSI2GridMode,0,"2"
[RSSI2GridMode_3.reg]
HKR,,RSSI2GridMode,0,"3"
[RSSI2GridMode_5.reg]
HKR,,RSSI2GridMode,0,"5"
;;----------------------------------------------------------------------------
;; RealWow and S5Wake Parameters
;;----------------------------------------------------------------------------
[RealWoW.reg]
HKR,defaults,RtHwCapability,0x00010001,8
HKR,,RtHwCapability,0x00010001,8

[S5Wake.reg]
HKR,defaults,WoWLANS5Support,0,"1"
HKR,,WoWLANS5Support,0,"1"

[S5SleepEnable.reg]
HKR,defaults,S5SleepEnable,0,"1"
HKR,,S5SleepEnable,0,"1"
;;----------------------------------------------------------------------------
;; EmacDelay Settings
;;----------------------------------------------------------------------------
[EmacDelay_200.reg]
HKR,,EmacDelayValue,0,"3"
[EmacDelay_ASUS_8821CE.reg]
HKR,,EmacDelayValue,0,"15"
;;----------------------------------------------------------------------------
;; UEFI Settings
;;----------------------------------------------------------------------------
[UEFI_Lenovo.reg]
;; Default use UEFI (0: disable, 1: Load country code & SAR Table ID, 2: Load SAR Table ID only, 3: Load country code only)
HKR,,LoadSystemSKUfromUEFI,0,"2"
;; Profile: Lenovo
HKR,,UEFIProfile,0,"1"

;;----------------------------------------------------------------------------
;; Clk Req Settings
;;----------------------------------------------------------------------------
[DisableClkReq_Lenovo.reg]
;; For Lenovo disable clkreq
HKR,,ClkReqSupport,0,"0"

;;----------------------------------------------------------------------------
;; SMBIOS Settings
;;----------------------------------------------------------------------------
[SKU_From_SMBIOS_Enable.reg]
;; Enable SMBIOS parsing (0: disable, 1: Load country code & SAR Table ID, 2: Load SAR Table ID only, 3: Load country code only)
HKR,,LoadSystemSKUfromSMBIOS,0,"1"

[SAR_ID_From_SMBIOS_Enable.reg]
;; Enable SMBIOS parsing (0: disable, 1: Load country code & SAR Table ID, 2: Load SAR Table ID only, 3: Load country code only)
HKR,,LoadSystemSKUfromSMBIOS,0,"2"

;; Rule to define BIOS single SKU information source priority configuration
;;   1. Prority is determined by order of alphabet, i.e. A>B>C>....>H
;;   2. The index of each letter in this registry string indicates the order of the enum definition of BIOS_METHOD, i.e. "UEFI","SMBIOS","ACPI",....
;; So if defined BiosMethodPriority = "ABC", the single SKU info source priority will be UEFI > SMBIOS > ACPI.
[SingleSkuInfo_SrcPrio_Cfg1.reg]
HKR,,BiosMethodPriority,0,"ABC"
;;----------------------------------------------------------------------------
;; ACPI Settings
;;----------------------------------------------------------------------------
[APCI_Lenovo_WRDS_SAR.reg]
;; Enable ACPI Table parsing
HKR,,LoadWrdsSarTablefromACPI,0,"1"
;; Specify ACPIProfile as ACPI_PROFILE_LENOVO_SAR (0x2) to enable Lenovo Single SKU SAR Solution
HKR,,ACPIProfile,0,"4"
HKR,,SupportBiosDynamicSAR,0,"1"
HKR,,SupportTxPwrTableDump,0,"1"

[APCI_HP_WRDS_SAR.reg]
;; Enable ACPI Table parsing
HKR,,LoadWrdsSarTablefromACPI,0,"1"
;; Specify ACPIProfile as ACPI_PROFILE_HP_SAR (0x3) to enable HP Single SKU SAR Solution
HKR,,ACPIProfile,0,"3"
HKR,,SupportTxPwrTableDump,0,"1"

[APCI_ASUS_BIOS_SAR.reg]
;; Enable ACPI Table parsing
HKR,,LoadWrdsSarTablefromACPI,0,"1"
;; Specify ACPIProfile as ACPI_PROFILE_ASUS_SAR (0x4) to enable ASUS BIOS dynamic SAR Solution
HKR,,ACPIProfile,0,"4"
HKR,,SupportBiosDynamicSAR,0,"1"
HKR,,SupportTxPwrTableDump,0,"1"

[APCI_DELL_BIOS_SAR.reg]
;; Enable ACPI Table parsing
HKR,,LoadWrdsSarTablefromACPI,0,"1"
;; Specify ACPIProfile as ACPI_PROFILE_ASUS_SAR (0x4) to enable ASUS BIOS dynamic SAR Solution
HKR,,ACPIProfile,0,"4"
HKR,,SupportBiosDynamicSAR,0,"1"
HKR,,SupportTxPwrTableDump,0,"1"

[APCI_RTK_BIOS_SAR.reg]
;; Enable ACPI Table parsing
HKR,,LoadWrdsSarTablefromACPI,0,"1"
;; Specify ACPIProfile as ACPI_PROFILE_ASUS_SAR (0x4) to enable ASUS BIOS dynamic SAR Solution
HKR,,ACPIProfile,0,"4"
HKR,,SupportBiosDynamicSAR,0,"1"
HKR,,SupportTxPwrTableDump,0,"1"


;;----------------------------------------------------------------------------
;; Antenna diversity Control Parameters
;;----------------------------------------------------------------------------
[AntDivEnable.reg]
HKR,,AntDiv,0,"1"

[AntDivDisable.reg]
HKR,,AntDiv,0,"0"
;;----------------------------------------------------------------------------
;; Antenna Detection Control Parameters
;;----------------------------------------------------------------------------
[AntDetectDisable.reg]
HKR,,EnableAntDet,0,"0"

[AntDetectEnable.reg]
HKR,,EnableAntDet,0,"1"


;;----------------------------------------------------------------------------
;; Antenna Detection Control Parameters
;;----------------------------------------------------------------------------
[NewRxReorderSettingsDisable.reg]
HKR,,NewRxReorderSettings,0,"0"

[NewRxReorderSettingsEnable.reg]
HKR,,NewRxReorderSettings,0,"0x80000003"

;;----------------------------------------------------------------------------
;; MAC Random Control Parameters
;;----------------------------------------------------------------------------
[EnableSupportMACRandom.reg]
HKR,,SupportMACRandom,0,"1"

HKR, Ndi\params\SupportMACRandom,       ParamDesc,  0, "MAC Randomization"
HKR, Ndi\params\SupportMACRandom,       default,    0, "1"
HKR, Ndi\params\SupportMACRandom,       type,       0, "enum"
HKR, Ndi\params\SupportMACRandom\enum,       "0",        0, %DISABLE_STR%
HKR, Ndi\params\SupportMACRandom\enum,       "1",        0, %ENABLE_STR%
;;----------------------------------------------------------------------------
;; CCK Threshold Control Parameters
;;----------------------------------------------------------------------------
[EnableForcedCCKTH.reg]
HKR,,ForcedCCKTh,0,"1"
;;----------------------------------------------------------------------------
;; Disable Clone Busy Queue
;;----------------------------------------------------------------------------
[DisableCloneBusyQueue.reg]
HKR,,DisableCloneBusyQueue,0,"1"

;;----------------------------------------------------------------------------
;; Worldwide Single SKU (Realtek Proposed) parameters
;;----------------------------------------------------------------------------
[WW.SingleSku.RTK.reg]
;; Enable SMBIOS parsing (0: disable, 1: Load country code & SAR Table ID, 2: Load SAR Table ID only, 3: Load country code only)
HKR,,LoadSystemSKUfromSMBIOS,0,"1"
;; Enable Power Table dump for checking SAR table in ACPI table.
HKR,,SupportTxPwrTableDump,0,"1"
;; Enable Dynamic SKU Determining Process
HKR,,EnableDynamicSkuProcess,0,"1"
;; Enable 802.11d
HKR,,Dot11dEnable,0,"1"
HKR,,DecisionByCountry,0,"1"
HKR,,CountryThreshold,0,"0"
HKR,,Majority,0,"0"

[Dot11dEnable.reg]
HKR,defaults,Dot11dEnable,0,"1"
HKR,,Dot11dEnable,0,"1"

[Dot11dDisable.reg]
HKR,defaults,Dot11dEnable,0,"0"
HKR,,Dot11dEnable,0,"0"

[SMPowerSaveEnable.reg]
HKR,defaults,SMPowerSave,0,"1"
HKR,,SMPowerSave,0,"1"

;;----------------------------------------------------------------------------
;; Customer Define Parameters
;;----------------------------------------------------------------------------
;;----------------------------------------------------------------------------
;; HP BW Advanced Setting Control Parameters
;;----------------------------------------------------------------------------
[IsHPAdvanceSetting.reg]
HKR,,IsHPAdvanceSetting,0,"1"

;;-------------------------
;; HP Common parameters
;;-------------------------
[HP.CommonNew.reg]
;;copy from HP.Common.reg
;;HP CusDefine ID is 1
HKR,,CusDefine,0,"1"
;;HP common CUSTOMER ID is RT_CID_HP
HKR,,CustomerID,0,"62"

;;HP workaround configuration (bitwise setting)
;;BIT0: HP_WA_TIE_CLKREQ_LOW, a worksound to tie CLKREQ to low to avoid card loss issue.
HKR,,HP_WA_Config,0,"0"
;; 0: Disable, 1: Enable, 2: Auto(keep original setting after IC auto-load)
HKR,,PciSerrConfig,0,"0"
;; 0: Disable, 1: Enable WDIF information transfer to BIOS
HKR,,EnWdifInfoTrans,0,"1"

;;[RoamingAggressiveness.reg]
HKR,,RegROAMSensitiveLevel,0,"75"
HKR,Ndi\Params\RegROAMSensitiveLevel, ParamDesc, 0, "Roaming Aggressiveness"
HKR,Ndi\Params\RegROAMSensitiveLevel, Type,      0, "enum"
HKR,Ndi\Params\RegROAMSensitiveLevel, Default,   0, "75"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "65",  0, "6. Highest"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "70",  0, "5. Medium-High"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "75",  0, "4. Medium"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "80",  0, "3. Medium-Low"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "85",  0, "2. Lowest"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "127",  0, "1. Disable"

;;[TxPwrLevel.reg]
HKR,,TxPwrLevel,0,"0"
HKR,Ndi\params\TxPwrLevel, 			ParamDesc, 	0, "Transmit power"
HKR,Ndi\params\TxPwrLevel, 			default, 	0, "0"
HKR,Ndi\params\TxPwrLevel, 			type, 		0, "enum"
HKR,Ndi\params\TxPwrLevel\enum, 	"0", 		0, "5. Highest"
HKR,Ndi\params\TxPwrLevel\enum, 	"1", 		0, "4. Medium-high"
HKR,Ndi\params\TxPwrLevel\enum, 	"2", 		0, "3. Medium"
HKR,Ndi\params\TxPwrLevel\enum, 	"3", 		0, "2. Medium-low"
HKR,Ndi\params\TxPwrLevel\enum, 	"4", 		0, "1. Lowest"

;;[ProtectionMode.reg]
;; Mix protection mode
HKR,Ndi\params\ProtectionMode, 			ParamDesc, 	0, "Mixed mode protection"
HKR,Ndi\params\ProtectionMode, 			type, 		0, "enum"
HKR,Ndi\params\ProtectionMode, 			default, 	0, "1"
HKR,Ndi\params\ProtectionMode\enum, 		"0", 	0, "RTS/CTS Enabled"
HKR,Ndi\params\ProtectionMode\enum, 		"1", 	0, "CTS-to-self Enabled"
HKR,defaults,ProtectionMode,0,"1"
HKR,,ProtectionMode,0,"1"
HKR,,ProtectionMode,,"1"

;;[FatChannelIntolerant.reg]
HKR,Ndi\params\b40Intolerant, 			ParamDesc, 	0, "Fat Channel Intolerant"
HKR,Ndi\params\b40Intolerant, 			type, 		0, "enum"
HKR,Ndi\params\b40Intolerant, 			default, 	0, "0"
HKR,Ndi\params\b40Intolerant\enum, 		"0", 		0, %DISABLE_STR%
HKR,Ndi\params\b40Intolerant\enum, 		"1", 		0, %ENABLE_STR%
HKR,,b40Intolerant,0,"0"
HKR,,b40Intolerant,,"0"

;;Advance Conductive Test
;;BIT1:Skip Sensitivity Roaming
;;BIT2:Disable RTS on AMPDU
;;IsConductive() criteria: RSSI,Performance,SSID
HKR,,AdvanceConductiveTest,0,"1286"

;;copy from HP.Common_2017.reg
;; Enable ACPI Table parsing
HKR,,LoadWrdsSarTablefromACPI,0,"1"
;; Specify ACPIProfile as ACPI_PROFILE_HP_SAR (0x3) to enable HP Single SKU SAR Solution
HKR,,ACPIProfile,0,"3"
HKR,,SupportBiosDynamicSAR,0,"1"	
;; Eaable Power Table dump for checking SAR table in ACPI table.
HKR,,SupportTxPwrTableDump,0,"1"

;; Enable SMBIOS SKU Number Parsing(For mapping SKU Num to specific country code for regulation assignment)
HKR,,LoadSkuNumberFromSMBIOS,0,"1"

;; Enable Dynamic SKU Determining Process
HKR,,EnableDynamicSkuProcess,0,"2"
;; Enable 802.11d
HKR,,Dot11dEnable,0,"1"
HKR,,DecisionByCountry,0,"1"
HKR,,Majority,0,"1"
HKR,,PriorCountry,,"US"
HKR,,CountryThreshold,0,"3"


;;[WowlanAllEnableNoLPS.reg]
HKR,,WoWLANPSMode,0,"0"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"
HKR,,NSOffloadEnable,0,"1"
HKR,,*WakeOnMagicPacket,0,"1"
HKR,,*WakeOnPattern,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

;;[WowlanOffload.reg] only enable when WoWlan is enabled
;; ARPOffload enable/disable
HKR,Ndi\params\ARPOffloadEnable, 			ParamDesc, 	0, "ARP offload for WoWLAN"
HKR,Ndi\params\ARPOffloadEnable, 			type, 		0, "enum"
HKR,Ndi\params\ARPOffloadEnable, 			default, 	0, "1"
HKR,Ndi\params\ARPOffloadEnable\enum, 		"0", 		0, "Disabled"
HKR,Ndi\params\ARPOffloadEnable\enum, 		"1", 		0, "Enabled"
;; GTK rekeying enable/disable
HKR,Ndi\params\GTKOffloadEnable, 			ParamDesc, 	0, "GTK rekeying for WoWLAN"
HKR,Ndi\params\GTKOffloadEnable, 			type, 		0, "enum"
HKR,Ndi\params\GTKOffloadEnable, 			default, 	0, "1"
HKR,Ndi\params\GTKOffloadEnable\enum, 		"0", 		0, "Disabled"
HKR,Ndi\params\GTKOffloadEnable\enum, 		"1", 		0, "Enabled"
;; NSOffload enable/disable
HKR,Ndi\params\NSOffloadEnable, 			ParamDesc, 	0, "NS offload for WoWLAN"
HKR,Ndi\params\NSOffloadEnable, 			type, 		0, "enum"
HKR,Ndi\params\NSOffloadEnable, 			default, 	0, "1"
HKR,Ndi\params\NSOffloadEnable\enum, 		"0", 		0, "Disabled"
HKR,Ndi\params\NSOffloadEnable\enum, 		"1", 		0, "Enabled"

;;[SleepOnDisconnectDisable.reg]
HKR,,WakeOnDisconnect,0,"1"
HKR, Ndi\params\WakeOnDisconnect,             ParamDesc,  0, %SleepOnDisconnect%
HKR, Ndi\params\WakeOnDisconnect,             default,    0, "1"
HKR, Ndi\params\WakeOnDisconnect,             type,       0, "enum"
HKR, Ndi\params\WakeOnDisconnect\enum,        "1",        0, %DISABLE_STR%
HKR, Ndi\params\WakeOnDisconnect\enum,        "0",        0, %ENABLE_STR%

;;[IdnNewBandSupByPltfm.reg]
;; Set Indonesia new band support as auto mode to determine by evaluating ACPI _DSM method
HKR,,IdnBandSupport,0,"2"



[HP.Common.reg]
;;HP CusDefine ID is 1
HKR,,CusDefine,0,"1"
;;HP common CUSTOMER ID is RT_CID_HP
HKR,,CustomerID,0,"62"

;; 0: Disable, 1: Enable, 2: Auto(keep original setting after IC auto-load)
HKR,,PciSerrConfig,0,"0"

;;[RoamingAggressiveness.reg]
HKR,,RegROAMSensitiveLevel,0,"75"
HKR,Ndi\Params\RegROAMSensitiveLevel, ParamDesc, 0, "Roaming Aggressiveness"
HKR,Ndi\Params\RegROAMSensitiveLevel, Type,      0, "enum"
HKR,Ndi\Params\RegROAMSensitiveLevel, Default,   0, "75"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "65",  0, "6. Highest"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "70",  0, "5. Medium-High"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "75",  0, "4. Medium"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "80",  0, "3. Medium-Low"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "85",  0, "2. Lowest"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "127",  0, "1. Disable"

;;[TxPwrLevel.reg]
HKR,,TxPwrLevel,0,"0"
HKR,Ndi\params\TxPwrLevel, 			ParamDesc, 	0, "Transmit power"
HKR,Ndi\params\TxPwrLevel, 			default, 	0, "0"
HKR,Ndi\params\TxPwrLevel, 			type, 		0, "enum"
HKR,Ndi\params\TxPwrLevel\enum, 	"0", 		0, "5. Highest"
HKR,Ndi\params\TxPwrLevel\enum, 	"1", 		0, "4. Medium-high"
HKR,Ndi\params\TxPwrLevel\enum, 	"2", 		0, "3. Medium"
HKR,Ndi\params\TxPwrLevel\enum, 	"3", 		0, "2. Medium-low"
HKR,Ndi\params\TxPwrLevel\enum, 	"4", 		0, "1. Lowest"

;;[ProtectionMode.reg]
;; Mix protection mode
HKR,Ndi\params\ProtectionMode, 			ParamDesc, 	0, "Mixed mode protection"
HKR,Ndi\params\ProtectionMode, 			type, 		0, "enum"
HKR,Ndi\params\ProtectionMode, 			default, 	0, "1"
HKR,Ndi\params\ProtectionMode\enum, 		"0", 	0, "RTS/CTS Enabled"
HKR,Ndi\params\ProtectionMode\enum, 		"1", 	0, "CTS-to-self Enabled"
HKR,defaults,ProtectionMode,0,"1"
HKR,,ProtectionMode,0,"1"
HKR,,ProtectionMode,,"1"

;;[FatChannelIntolerant.reg]
HKR,Ndi\params\b40Intolerant, 			ParamDesc, 	0, "Fat Channel Intolerant"
HKR,Ndi\params\b40Intolerant, 			type, 		0, "enum"
HKR,Ndi\params\b40Intolerant, 			default, 	0, "0"
HKR,Ndi\params\b40Intolerant\enum, 		"0", 		0, %DISABLE_STR%
HKR,Ndi\params\b40Intolerant\enum, 		"1", 		0, %ENABLE_STR%
HKR,,b40Intolerant,0,"0"
HKR,,b40Intolerant,,"0"

;;Advance Conductive Test
;;BIT1:Skip Sensitivity Roaming
;;BIT2:Disable RTS on AMPDU
;;IsConductive() criteria: RSSI,Performance,SSID
HKR,,AdvanceConductiveTest,0,"1286"

;;Waiting for leaving IPS before indicating task scan M4
HKR,,ScanM4WaitForIPSLeave,0,"1"


[HP.Common_2017.reg]
;; 0: Disable, 1: Enable WDIF information transfer to BIOS
HKR,,EnWdifInfoTrans,0,"1"
;; Enable ACPI Table parsing
HKR,,LoadWrdsSarTablefromACPI,0,"1"
;; Specify ACPIProfile as ACPI_PROFILE_HP_SAR (0x3) to enable HP Single SKU SAR Solution
HKR,,ACPIProfile,0,"3"
HKR,,SupportBiosDynamicSAR,0,"1"	
;; Eaable Power Table dump for checking SAR table in ACPI table.
HKR,,SupportTxPwrTableDump,0,"1"

;; Enable SMBIOS SKU Number Parsing(For mapping SKU Num to specific country code for regulation assignment)
HKR,,LoadSkuNumberFromSMBIOS,0,"1"

;; Enable Dynamic SKU Determining Process
HKR,,EnableDynamicSkuProcess,0,"2"
;; Enable 802.11d
HKR,,Dot11dEnable,0,"1"
HKR,,DecisionByCountry,0,"1"
HKR,,Majority,0,"1"
HKR,,PriorCountry,,"US"
HKR,,CountryThreshold,0,"3"

;; Enable AdvanceOTA setting for HP
HKR,,AdvanceOTA,0,"2"

;;Phydm Adaptive SOML 
;;Disable for HP OTA Test
HKR,,bSupportAdaptiveSOML,0,"0"

;;[WowlanAllEnableNoLPS.reg]
HKR,,WoWLANPSMode,0,"0"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"
HKR,,NSOffloadEnable,0,"1"
HKR,,*WakeOnMagicPacket,0,"1"
HKR,,*WakeOnPattern,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

;;[WowlanOffload.reg] only enable when WoWlan is enabled
;; ARPOffload enable/disable
HKR,Ndi\params\ARPOffloadEnable, 			ParamDesc, 	0, "ARP offload for WoWLAN"
HKR,Ndi\params\ARPOffloadEnable, 			type, 		0, "enum"
HKR,Ndi\params\ARPOffloadEnable, 			default, 	0, "1"
HKR,Ndi\params\ARPOffloadEnable\enum, 		"0", 		0, "Disabled"
HKR,Ndi\params\ARPOffloadEnable\enum, 		"1", 		0, "Enabled"
;; GTK rekeying enable/disable
HKR,Ndi\params\GTKOffloadEnable, 			ParamDesc, 	0, "GTK rekeying for WoWLAN"
HKR,Ndi\params\GTKOffloadEnable, 			type, 		0, "enum"
HKR,Ndi\params\GTKOffloadEnable, 			default, 	0, "1"
HKR,Ndi\params\GTKOffloadEnable\enum, 		"0", 		0, "Disabled"
HKR,Ndi\params\GTKOffloadEnable\enum, 		"1", 		0, "Enabled"
;; NSOffload enable/disable
HKR,Ndi\params\NSOffloadEnable, 			ParamDesc, 	0, "NS offload for WoWLAN"
HKR,Ndi\params\NSOffloadEnable, 			type, 		0, "enum"
HKR,Ndi\params\NSOffloadEnable, 			default, 	0, "1"
HKR,Ndi\params\NSOffloadEnable\enum, 		"0", 		0, "Disabled"
HKR,Ndi\params\NSOffloadEnable\enum, 		"1", 		0, "Enabled"

;;[SleepOnDisconnectDisable.reg]
HKR,,WakeOnDisconnect,0,"1"
HKR, Ndi\params\WakeOnDisconnect,             ParamDesc,  0, %SleepOnDisconnect%
HKR, Ndi\params\WakeOnDisconnect,             default,    0, "1"
HKR, Ndi\params\WakeOnDisconnect,             type,       0, "enum"
HKR, Ndi\params\WakeOnDisconnect\enum,        "1",        0, %DISABLE_STR%
HKR, Ndi\params\WakeOnDisconnect\enum,        "0",        0, %ENABLE_STR%

;;[IdnNewBandSupByPltfm.reg]
;; Set Indonesia new band support as auto mode to determine by evaluating ACPI _DSM method
HKR,,IdnBandSupport,0,"2"
;;-------------------------
;; ASUS NB Common parameters
;;-------------------------
[ASUS.NB.Common.reg]
HKR,,CustomerID,0,"47"
;; Decide adopting China new or old regulation by BIOS
HKR,,cn_reg_sel, 0, "0"
;;-------------------------
;; ASUS MB Common parameters
;;-------------------------
[ASUS.MB.Common.reg]
;; Decide adopting China new or old regulation by BIOS
HKR,,cn_reg_sel, 0, "0"
;;-------------------------
;; Lenovo Common parameters
;;-------------------------
[LC.CommonNew.reg]
HKR,,CustomerID,0,"40"
HKR,,SupportTxPwrTableDump,0,"1"
HKR,,TxPwrLmtTableFromSingleFile,0,"1"
;; Decide adopting China new or old regulation by BIOS
HKR,,cn_reg_sel, 0, "0"

;; Enable loading single SKU info from UEFI (0: disable, 1: Load country code & SAR Table ID, 2: Load SAR Table ID only, 3: Load country code only)
HKR,,LoadSystemSKUfromUEFI,0,"2"
;; Profile: Lenovo
HKR,,UEFIProfile,0,"1"
;; Enable loading single SKU info from SMBIOS (0: disable, 1: Load country code & SAR Table ID, 2: Load SAR Table ID only, 3: Load country code only)
HKR,,LoadSystemSKUfromSMBIOS,0,"2"
;; Rule to define BIOS single SKU information source priority configuration
;;   1. Prority is determined by order of alphabet, i.e. A>B>C>....>H
;;   2. The index of each letter in this registry string indicates the order of the enum definition of BIOS_METHOD, i.e. "UEFI","SMBIOS","ACPI",....
;; So if defined BiosMethodPriority = "ABC", the single SKU info source priority will be UEFI > SMBIOS > ACPI.
HKR,,BiosMethodPriority,0,"ABC"

;;BIT1 Skip Sensitivity Roaming
;;BIT2 Diable RTSonAMPDU
;;IsConductive() : RSSI,APNUM,Performance  
HKR,,AdvanceConductiveTest,0,"1542"

HKR,Ndi\params\BWSetting,        ParamDesc,  0, "Bandwidth"
HKR,Ndi\params\BWSetting,        type,       0, "enum"
HKR,Ndi\params\BWSetting,        default,    0, "2"
HKR,Ndi\params\BWSetting\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BWSetting\enum,   "1",        0, "40_20MHz"
HKR,Ndi\params\BWSetting\enum,   "2",        0, "80_40_20MHz"
HKR,defaults,BWSetting,0,"2"
HKR,,BWSetting,0,"2"

HKR,,RegROAMSensitiveLevel,0,"80"
HKR,Ndi\Params\RegROAMSensitiveLevel, ParamDesc, 0, %ROAMING_SENSITIVITY_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel, Type,      0, "enum"
HKR,Ndi\Params\RegROAMSensitiveLevel, Default,   0, "80"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "127",  0, %DISABLE_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "65",  0, %HIGH_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "70",  0, %MIDDLE_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "80",  0, %LOW_STR%

;; Prefer Band
HKR,Ndi\params\PreferBand, 			ParamDesc, 	0, "Preferred Band"
HKR,Ndi\params\PreferBand, 			default, 	0, "0"
HKR,Ndi\params\PreferBand, 			type, 		0, "enum"
HKR,Ndi\params\PreferBand\enum, 	"0", 		0, "1. No Preference"
HKR,Ndi\params\PreferBand\enum, 	"1", 		0, "2. 2.4G first"
HKR,Ndi\params\PreferBand\enum, 	"2", 		0, "3. 5G first"
HKR,,PreferBand,0,"0"

[LC.Common.reg]
HKR,,CustomerID,0,"40"
HKR,,SupportTxPwrTableDump,0,"1"
HKR,,PortMacAddressRandom,0,"1"
;; Decide adopting China new or old regulation by BIOS
HKR,,cn_reg_sel, 0, "0"

;; Enable loading single SKU info from UEFI (0: disable, 1: Load country code & SAR Table ID, 2: Load SAR Table ID only, 3: Load country code only)
HKR,,LoadSystemSKUfromUEFI,0,"2"
;; Profile: Lenovo
HKR,,UEFIProfile,0,"1"
;; Enable loading single SKU info from SMBIOS (0: disable, 1: Load country code & SAR Table ID, 2: Load SAR Table ID only, 3: Load country code only)
HKR,,LoadSystemSKUfromSMBIOS,0,"2"
;; Rule to define BIOS single SKU information source priority configuration
;;   1. Prority is determined by order of alphabet, i.e. A>B>C>....>H
;;   2. The index of each letter in this registry string indicates the order of the enum definition of BIOS_METHOD, i.e. "UEFI","SMBIOS","ACPI",....
;; So if defined BiosMethodPriority = "ABC", the single SKU info source priority will be UEFI > SMBIOS > ACPI.
HKR,,BiosMethodPriority,0,"ABC"

;;BIT0 Reload Tx Power Limit
;;BIT1 Skip Sensitivity Roaming
;;BIT2 Diable RTSonAMPDU
;;IsConductive() : RSSI,APNUM,Performance  
HKR,,AdvanceConductiveTest,0,"1543"

HKR,Ndi\params\BWSetting,        ParamDesc,  0, "Bandwidth"
HKR,Ndi\params\BWSetting,        type,       0, "enum"
HKR,Ndi\params\BWSetting,        default,    0, "2"
HKR,Ndi\params\BWSetting\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BWSetting\enum,   "1",        0, "40_20MHz"
HKR,Ndi\params\BWSetting\enum,   "2",        0, "80_40_20MHz"
HKR,defaults,BWSetting,0,"2"
HKR,,BWSetting,0,"2"

HKR,,RegROAMSensitiveLevel,0,"80"
HKR,Ndi\Params\RegROAMSensitiveLevel, ParamDesc, 0, %ROAMING_SENSITIVITY_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel, Type,      0, "enum"
HKR,Ndi\Params\RegROAMSensitiveLevel, Default,   0, "80"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "127",  0, %DISABLE_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "65",  0, %HIGH_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "70",  0, %MIDDLE_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "80",  0, %LOW_STR%

;; Prefer Band
HKR,Ndi\params\PreferBand, 			ParamDesc, 	0, "Preferred Band"
HKR,Ndi\params\PreferBand, 			default, 	0, "0"
HKR,Ndi\params\PreferBand, 			type, 		0, "enum"
HKR,Ndi\params\PreferBand\enum, 	"0", 		0, "1. No Preference"
HKR,Ndi\params\PreferBand\enum, 	"1", 		0, "2. 2.4G first"
HKR,Ndi\params\PreferBand\enum, 	"2", 		0, "3. 5G first"
HKR,,PreferBand,0,"0"

;; Adaptivity Method
;; 0: Old method (Shared-L2H => 2.4G & 5G share one L2H value) 1: New method (In-Band L2H => 2.4G & 5G maintain separate L2H values)
HKR,,AdaptivityMethod,0,"1"

;;-------------------------
;; ACER Common parameters
;;-------------------------
[ACER.Common.reg]
HKR,,RSSI2GridMode,0,"5"

;;BIT0 Reload Tx Power Limit
;;BIT1 Skip Sensitivity Roaming
;;BIT2 Diable RTSonAMPDU
;;IsConductive() : RSSI,APNUM,Performance
HKR,,AdvanceConductiveTest,0,"1543"
;;-------------------------
;; Dynabook Common parameters
;;-------------------------
[Dynabook.Common.reg]
HKR,,CustomerID,0,"64"
;;-------------------------
;; DELL Common parameters
;;-------------------------
[DELL.Common.reg]
;; Decide adopting China new or old regulation by BIOS
HKR,,cn_reg_sel, 0, "0"

;----------------------------------------------------------------------------
;; Advance Conductive Test
;;----------------------------------------------------------------------------
[AdvanceConductiveTest.reg]
;;BIT2 Diable RTSonAMPDU
HKR,,AdvanceConductiveTest,0,"1030"
;----------------------------------------------------------------------------
;; Select Antenna by RSSI Control Parameters
;;----------------------------------------------------------------------------
[SelectAntByRssi.reg]
HKR,,SelectAntByRssi,0,"1"
;----------------------------------------------------------------------------
;; Antenna Switch Bias Control Parameters
;;----------------------------------------------------------------------------
[AntSwBiasEnable.reg]
HKR,,DmAntSwPwdbBias,0,"1"
;----------------------------------------------------------------------------
;; DM CSI Report Control Parameters
;;----------------------------------------------------------------------------
[DmCsiRptEnable.reg]
HKR,,DmCsiRpt,0,"1"
;*******************************************************************************
; RTL8822BE Special Parameters
;*******************************************************************************
[RTL8822be.Common.reg]
HKR,,BeamformCap,0,"10"
HKR,,ValidRFPath,0,"51"
HKR,,PreInitMem,0,"1"
HKR,,BeamformeeCapRfNum,0,"3"
HKR,,AvoidRxDpcWDViolation,0,"1"
HKR,,EmacDelayValue,0,"15"
HKR,,TxPwrIndex,0,"1"

;Set Forced AMSDU in AMPDU in default
HKR,,AMfactor,0,"253"

HKR,,ECSSupport,0,"0"

;Force to Gen 1
HKR,,ForcePCIeRate,0,"1"

;;Enable dumping ePHY register in initializing Adapter by setting DumpInterfacePhyRegMaxCount as 0xFF. (Otherwise, set 0 to disable it)
HKR,,DumpInterfacePhyRegMaxCount,0,"255"

;Set default Channel to 10
HKR,,Channel,0,"10"

;; STBC 
;;HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
;;HKR,Ndi\params\StbcCap,        type,       0, "enum"
;;HKR,Ndi\params\StbcCap,        default,    0, "51"
;;HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
;;HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
;;HKR,Ndi\params\StbcCap\enum,   "17",        0, "HT/VHT STBC RX"
;;HKR,Ndi\params\StbcCap\enum,   "34",        0, "HT/VHT STBC TX"
;;HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
;;HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
;;HKR,,StbcCap,,"51"

;; LDPC 
;;HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
;;HKR,Ndi\params\LdpcCap,        type,       0, "enum"
;;HKR,Ndi\params\LdpcCap,        default,    0, "51"
;;HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
;;HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
;;HKR,Ndi\params\LdpcCap\enum,   "17",        0, "HT/VHT LDPC RX"
;;HKR,Ndi\params\LdpcCap\enum,   "34",        0, "HT/VHT LDPC TX"
;;HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
;;HKR,defaults,LdpcCap,0,"51"
HKR,,LdpcCap,0,"51"
;;HKR,,LdpcCap,,"51"

HKR,,SupportFakeGC,0,"1"

;;Avoid desc with error
HKR,,bRxDescErrorChk,0,"1"

;; Enable BT YB Workaround in F/W
HKR,,EnBTWA,0,"1"


[ASUS8822be_ExtPwrTableDynamicSwitch.reg]
;; For Dynamic Loading external Primary/Secondary TxPowerLimitTable
;; If TxPowerLimitTableSel = 0xFF(255), it will not load external primary file until user issue "set pwrTable 0" by WlanCLI tool
HKR,,EnableTxPowerLimit,0,"1"
HKR,,PwrLimitFile,0,"DEFAULT_REALTEK.txt"
HKR,,SecondaryPwrLimitFile,0,"LOW_REALTEK.txt"
HKR,,TxPowerLimitTableSel,0,"255"
HKR,,TxPwrLmtDynamicLoading,0,"1"



;*******************************************************************************
; RTL8822CE Special Parameters
;*******************************************************************************
[RTL8822ce.Common.reg]
HKR,,BeamformCap,0,"10"
HKR,,ValidRFPath,0,"51"
HKR,,PreInitMem,0,"1"
HKR,,BeamformeeCapRfNum,0,"3"
HKR,,AvoidRxDpcWDViolation,0,"1"
HKR,,EmacDelayValue,0,"1"
HKR,,TxPwrIndex,0,"1"

;;Advance Conductive Test
;;BIT1:Skip Sensitivity Roaming
;;BIT2:Disable RTS on AMPDU
;;IsConductive() criteria: RSSI,Performance,SSID
HKR,,AdvanceConductiveTest,0,"1286"

;Set Forced AMSDU in AMPDU in default
HKR,,AMfactor,0,"253"

HKR,,ECSSupport,0,"0"

;Force to Gen 1
HKR,,ForcePCIeRate,0,"1"

;;Enable dumping ePHY register in initializing Adapter by setting DumpInterfacePhyRegMaxCount as 0xFF. (Otherwise, set 0 to disable it)
HKR,,DumpInterfacePhyRegMaxCount,0,"255"

;Set default Channel to 10
HKR,,Channel,0,"10"

;; STBC 
;;HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
;;HKR,Ndi\params\StbcCap,        type,       0, "enum"
;;HKR,Ndi\params\StbcCap,        default,    0, "51"
;;HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
;;HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
;;HKR,Ndi\params\StbcCap\enum,   "17",        0, "HT/VHT STBC RX"
;;HKR,Ndi\params\StbcCap\enum,   "34",        0, "HT/VHT STBC TX"
;;HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
;;HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
;;HKR,,StbcCap,,"51"

;; LDPC 
;;HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
;;HKR,Ndi\params\LdpcCap,        type,       0, "enum"
;;HKR,Ndi\params\LdpcCap,        default,    0, "51"
;;HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
;;HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
;;HKR,Ndi\params\LdpcCap\enum,   "17",        0, "HT/VHT LDPC RX"
;;HKR,Ndi\params\LdpcCap\enum,   "34",        0, "HT/VHT LDPC TX"
;;HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
;;HKR,defaults,LdpcCap,0,"51"
HKR,,LdpcCap,0,"51"
;;HKR,,LdpcCap,,"51"

HKR,,MCCDbg,0,"3"

;; Specify 8822CE Tx Power limit table ID as 00017 (For supporting ACMA/CHILE/UKRAINE/MEXICO regulation)
HKR,,SupportTxPwrTableDump,0,"1"
HKR,,TxPwrLmtTableFromSingleFile,0,"1"
HKR,,ForcedCustomTxPwrLmtTableID,0,"17"

;;Avoid desc with error
HKR,,bRxDescErrorChk,0,"1"

;; Enable BT YB Workaround in F/W
;; 4 = hwid_chk_en
HKR,,EnBTWA,0,"4"
;;Maximum TPC Deduction power index (24 = 6dBm)
HKR,,MaxTPCDeduction,0,"24"


;;VHT - Rx MPDU Size
;; 0: 4k, 1: 8k, 2: 12k
HKR,,RxMPDUMaxSize,0,"1"

[RTL8822ce.ASPM.reg]
HKR,,ClkReqDelayValue,0,"11"
HKR,,L0sDelayValue,0,"255"
HKR,,L1DelayValue,0,"254"
HKR,,L1DelayLongValue,0,"3"
HKR,,RefClkAutoK,0,"1"


HKR,,L0sSupport,0,"0"
HKR,,ClkReqSupport,0,"2"
HKR,,L1Support,0,"2"
HKR,,L1OffSupport,0,"1"
HKR,,LtrSupport,0,"2"





;*******************************************************************************
; RTL8821CE Special Parameters
;*******************************************************************************
[RTL8821ce.Common.reg]
HKR,,RefClkAutoK,0,"1"
HKR,,AutoKOnTempChange,0,"0"
HKR,,BeamformCap,0,"10"
HKR,,BeamformeeCapRfNum,0,"3"
HKR,,ValidRFPath,0,"17"
HKR,,PreInitMem,0,"1"
HKR,,EmacDelayForAutoKEn,0,"15"
HKR,,EmacDelayValue,0,"13"
HKR,,DynamicClk,0,"0"
HKR,,RdAtWt,0,"0"
HKR,,ChkRdTO,0,"1"
HKR,,DmAggNum,0,"1"
HKR,,PWRSavingType,0,"2"
HKR,,TxPwrIndex,0,"1"

;; Power Consumption
HKR,,Scan_IPSEnable,0,"1"
HKR,,bAdvancedLPs,0,"243"
HKR,,TBTTShift,0,"2"
HKR,,bLPSTuningEnable,0,"1"
HKR,,L1OffSupport,0,"2"

;; STBC 
;;HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
;;HKR,Ndi\params\StbcCap,        type,       0, "enum"
;;HKR,Ndi\params\StbcCap,        default,    0, "17"
;;HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
;;HKR,Ndi\params\StbcCap\enum,   "1",        0, "VHT STBC RX"
;;HKR,Ndi\params\StbcCap\enum,   "17",       0, "HT/VHT STBC RX"
;;HKR,defaults,StbcCap,0,"17"
HKR,,StbcCap,0,"17"
;;HKR,,StbcCap,,"17"

;; LDPC 
;;HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
;;HKR,Ndi\params\LdpcCap,        type,       0, "enum"
;;HKR,Ndi\params\LdpcCap,        default,    0, "34"
;;HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
;;HKR,Ndi\params\LdpcCap\enum,   "2",        0, "VHT LDPC TX"
;;HKR,Ndi\params\LdpcCap\enum,   "34",       0, "HT/VHT LDPC TX"
;;HKR,defaults,LdpcCap,0,"34"
HKR,,LdpcCap,0,"34"
;;HKR,,LdpcCap,,"34"

;;Enable dumping ePHY register in initializing Adapter by setting DumpInterfacePhyRegMaxCount as 0xFF. (Otherwise, set 0 to disable it)
HKR,,DumpInterfacePhyRegMaxCount,0,"255"

HKR,,SupportFakeGC,0,"1"

;;Avoid desc with error
HKR,,bRxDescErrorChk,0,"1"

;; Enable BT YB Workaround in F/W
HKR,,EnBTWA,0,"1"

;; Enable FW PCIe Recovery feature
HKR,,EnPciRecov,0,"1"


[MI8821ce.Common.reg]

HKR,,BeamformCap,0,"10"
HKR,,BeamformeeCapRfNum,0,"3"
HKR,,ValidRFPath,0,"17"
HKR,,PreInitMem,0,"1"
HKR,,EmacDelayValue,0,"14"
HKR,,DynamicClk,0,"0"
HKR,,RdAtWt,0,"0"
HKR,,ChkRdTO,0,"1"
HKR,,DmAggNum,0,"1"
HKR,,PWRSavingType,0,"2"
HKR,,TxPwrIndex,0,"1"

;; Power Consumption
HKR,,Scan_IPSEnable,0,"1"
HKR,,bAdvancedLPs,0,"243"
HKR,,TBTTShift,0,"2"
HKR,,bLPSTuningEnable,0,"1"
HKR,,L1OffSupport,0,"2"

;; STBC 
;;HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
;;HKR,Ndi\params\StbcCap,        type,       0, "enum"
;;HKR,Ndi\params\StbcCap,        default,    0, "17"
;;HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
;;HKR,Ndi\params\StbcCap\enum,   "1",        0, "VHT STBC RX"
;;HKR,Ndi\params\StbcCap\enum,   "17",       0, "HT/VHT STBC RX"
;;HKR,defaults,StbcCap,0,"17"
HKR,,StbcCap,0,"17"
;;HKR,,StbcCap,,"17"

;; LDPC 
;;HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
;;HKR,Ndi\params\LdpcCap,        type,       0, "enum"
;;HKR,Ndi\params\LdpcCap,        default,    0, "34"
;;HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
;;HKR,Ndi\params\LdpcCap\enum,   "2",        0, "VHT LDPC TX"
;;HKR,Ndi\params\LdpcCap\enum,   "34",       0, "HT/VHT LDPC TX"
;;HKR,defaults,LdpcCap,0,"34"
HKR,,LdpcCap,0,"34"
;;HKR,,LdpcCap,,"34"

;;Enable dumping ePHY register in initializing Adapter by setting DumpInterfacePhyRegMaxCount as 0xFF. (Otherwise, set 0 to disable it)
HKR,,DumpInterfacePhyRegMaxCount,0,"255"

HKR,,SupportFakeGC,0,"1"

;; Enable BT YB Workaround in F/W
HKR,,EnBTWA,0,"1"


[FN8821ce.Common.reg]
HKR,,BeamformCap,0,"34"
HKR,,BeamformeeCapRfNum,0,"3"
HKR,,ValidRFPath,0,"17"
HKR,,PreInitMem,0,"1"
HKR,,EmacDelayValue,0,"13"
HKR,,DynamicClk,0,"0"
HKR,,RdAtWt,0,"0"
HKR,,ChkRdTO,0,"1"
HKR,,DmAggNum,0,"1"
HKR,,PWRSavingType,0,"2"
HKR,,TxPwrIndex,0,"1"

;; STBC 
;;HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
;;HKR,Ndi\params\StbcCap,        type,       0, "enum"
;;HKR,Ndi\params\StbcCap,        default,    0, "17"
;;HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
;;HKR,Ndi\params\StbcCap\enum,   "1",        0, "VHT STBC RX"
;;HKR,Ndi\params\StbcCap\enum,   "17",       0, "HT/VHT STBC RX"
;;HKR,defaults,StbcCap,0,"17"
HKR,,StbcCap,0,"17"
;;HKR,,StbcCap,,"17"

;; LDPC 
;;HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
;;HKR,Ndi\params\LdpcCap,        type,       0, "enum"
;;HKR,Ndi\params\LdpcCap,        default,    0, "34"
;;HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
;;HKR,Ndi\params\LdpcCap\enum,   "2",        0, "VHT LDPC TX"
;;HKR,Ndi\params\LdpcCap\enum,   "34",       0, "HT/VHT LDPC TX"
;;HKR,defaults,LdpcCap,0,"34"
HKR,,LdpcCap,0,"34"
;;HKR,,LdpcCap,,"34"

;;Enable dumping ePHY register in initializing Adapter by setting DumpInterfacePhyRegMaxCount as 0xFF. (Otherwise, set 0 to disable it)
HKR,,DumpInterfacePhyRegMaxCount,0,"255"

;; Enable BT YB Workaround in F/W
HKR,,EnBTWA,0,"1"
;*******************************************************************************
; RTL8723DE Special Parameters
;*******************************************************************************
[RTL8723de.Common.reg]
HKR,,StbcCap,0,"16"
HKR,,LdpcCap,0,"0"
HKR,,RefClkAutoK,0,"0"
HKR,,EmacDelayValue,0,"0"
HKR,,CmuDelayValue,0,"0"
HKR,,ClkDelayCount8723D,0,"70"
HKR,,WdiGOon5GHzBandSupported,0,"0"

;;Enable dumping ePHY register in initializing Adapter by setting DumpInterfacePhyRegMaxCount as 0xFF. (Otherwise, set 0 to disable it)
HKR,,DumpInterfacePhyRegMaxCount,0,"255"

[DELL8723de.ASPM.reg]
HKR,,RefClkAutoK,0,"0"
HKR,,EmacDelayValue,0,"0"
HKR,,CmuDelayValue,0,"90"
HKR,,ClkDelayCount8723D,0,"255"
HKR,,L1OffSupport,0,"2"



;*******************************************************************************
; AdvanceOTA Settings
;*******************************************************************************
[ASUS_AdvanceOTA.reg]
;; Enable AdvanceOTA setting for ASUS
HKR,,AdvanceOTA,0,"24"
;;Phydm Adaptive SOML 
;;Disable for ASUS OTA Test
HKR,,bSupportAdaptiveSOML,0,"0"

;*******************************************************************************
; RetryTimes Settings (0x42a)
;*******************************************************************************
[RetryTimes_32.reg]
HKR,,RetryTimes,0,"32"
[RetryTimes_5.reg]
HKR,,RetryTimes,0,"5"
[AdvancedRetryLimit.reg]
HKR,,AdvancedRetryLimit,0,"1"


;-------------------------------------------------------------------------------
;	Auto Channel Selection
;-------------------------------------------------------------------------------
[AutoChnlSelon.reg]
HKR,,AutoChnlSel,0,"1"
[AutoChnlSeloff.reg]
HKR,,AutoChnlSel,0,"0"
;*******************************************************************************
; GO prefer setting
;*******************************************************************************
[GOPreferMode_Lnv.reg]
HKR,,OpChSelect,0,"5"

;; GO Op ch Prefer list
HKR,,OpChnlList,0,"36,40,44,48,149,153,157,161,165,169,52,56,60,64,100,104,108,112,116,120,124,128,132,136,140,6,11,1,2,3,4,5,7,8,9,10"

HKR,,MCCDynamicGOTime,0,"0"

;; ECSA Feature Enable
HKR,,ECSAMiracast,0,"1"

HKR,,ConcurrentOpPref, 0, "7"

[GOPreferMode_DELL.reg]
HKR,,ConcurrentOpPref, 0, "0"

;*******************************************************************************
; Multi-Channel Concurrent section
;*******************************************************************************
[MCCDisable.reg]
HKR,Ndi\params\MultiChannelFcsMode, 		ParamDesc, 	0, "Multi-Channel Concurrent"
HKR,Ndi\params\MultiChannelFcsMode, 		type, 		0, "enum"
HKR,Ndi\params\MultiChannelFcsMode, 		default, 	0, "0"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"0", 		0, "Disabled"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"4", 		0, "Enabled"
HKR,defaults,MultiChannelFcsMode, 0, "0"
HKR,,MultiChannelFcsMode, 0, "0"

[MCCEnable.reg]
HKR,Ndi\params\MultiChannelFcsMode, 		ParamDesc, 	0, "Multi-Channel Concurrent"
HKR,Ndi\params\MultiChannelFcsMode, 		type, 		0, "enum"
HKR,Ndi\params\MultiChannelFcsMode, 		default, 	0, "4"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"0", 		0, "Disabled"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"4", 		0, "Enabled"
HKR,defaults,MultiChannelFcsMode, 0, "4"
HKR,,MultiChannelFcsMode, 0, "4"

[MCCDisable_v2.reg]
HKR,Ndi\params\MultiChannelFcsMode, 		ParamDesc, 	0, "Multi-Channel Concurrent"
HKR,Ndi\params\MultiChannelFcsMode, 		type, 		0, "enum"
HKR,Ndi\params\MultiChannelFcsMode, 		default, 	0, "0"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"0", 		0, "Disabled"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"12", 		0, "Enabled"
HKR,defaults,MultiChannelFcsMode, 0, "0"
HKR,,MultiChannelFcsMode, 0, "0"

[MCCEnable_v2.reg]
HKR,Ndi\params\MultiChannelFcsMode, 		ParamDesc, 	0, "Multi-Channel Concurrent"
HKR,Ndi\params\MultiChannelFcsMode, 		type, 		0, "enum"
HKR,Ndi\params\MultiChannelFcsMode, 		default, 	0, "12"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"0", 		0, "Disabled"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"12", 		0, "Enabled"
HKR,defaults,MultiChannelFcsMode, 0, "12"
HKR,,MultiChannelFcsMode, 0, "12"

[MCCDisable_v3.reg]
HKR,Ndi\params\MultiChannelFcsMode, 		ParamDesc, 	0, "Multi-Channel Concurrent"
HKR,Ndi\params\MultiChannelFcsMode, 		type, 		0, "enum"
HKR,Ndi\params\MultiChannelFcsMode, 		default, 	0, "0"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"0", 		0, "Disabled"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"12", 		0, "Enabled"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"28", 		0, "Enabled + Hotspot"
HKR,defaults,MultiChannelFcsMode, 0, "0"
HKR,,MultiChannelFcsMode, 0, "0"

[MCCEnable_v3.reg]
HKR,Ndi\params\MultiChannelFcsMode, 		ParamDesc, 	0, "Multi-Channel Concurrent"
HKR,Ndi\params\MultiChannelFcsMode, 		type, 		0, "enum"
HKR,Ndi\params\MultiChannelFcsMode, 		default, 	0, "28"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"0", 		0, "Disabled"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"12", 		0, "Enabled"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"28", 		0, "Enabled + Hotspot"
HKR,defaults,MultiChannelFcsMode, 0, "28"
HKR,,MultiChannelFcsMode, 0, "28"

[MCCReport.reg]
HKR,,MCCDbg,0,"3"
;;----------------------------------------------------------------------------
;; WDI GO on 5GHz Supported
;;----------------------------------------------------------------------------
[WdiGOon5GHzBandSupportedEnable.reg]
HKR,,WdiGOon5GHzBandSupported,0,"1"

[Periodic_chk_twice.reg]
HKR,,perdic_chk_twice_rx,0,"1"

[AdvanceWdiGOon5GHzBandSupportedEnable.reg]
HKR,,WdiGOon5GHzBandSupported,0,"1"

HKR, Ndi\params\WdiGOon5GHzBandSupported,       ParamDesc,  0, "Hot Spot Dual Band"
HKR, Ndi\params\WdiGOon5GHzBandSupported,       default,    0, "1"
HKR, Ndi\params\WdiGOon5GHzBandSupported,       type,       0, "enum"
HKR, Ndi\params\WdiGOon5GHzBandSupported\enum,       "0",        0, %DISABLE_STR%
HKR, Ndi\params\WdiGOon5GHzBandSupported\enum,       "1",        0, %ENABLE_STR%
;;----------------------------------------------------------------------------
;; Disable WDI GO DFS Operating Channel Error Reported to WDI
;;----------------------------------------------------------------------------
[WdiGODfsErrorDisable.reg]
HKR,,WdiGODfsError,0,"0"
;;----------------------------------------------------------------------------
;; Enable FW PCIe Recovery feature
;;----------------------------------------------------------------------------
[EnFwPciRecov.reg]
;; Enable FW PCIe Recovery feature
HKR,,EnPciRecov,0,"1"
;;****************************************************************************
;; OS relative service.
;;****************************************************************************
[RTWlanE.Service]
DisplayName     = %RTWlanE.DeviceDesc.DispName%
ServiceType     = 1 		;SERVICE_KERNEL_DRIVER
StartType       = 3 		;SERVICE_DEMAND_START
ErrorControl    = 1 		;SERVICE_ERROR_NORMAL
ServiceBinary   = %12%\rtwlane.sys
LoadOrderGroup  = NDIS

[RTWlanE.EventLog]
AddReg = RTWlanE.AddEventLog.reg

[RTWlanE.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7
[RTWlanE.CopyFiles]
rtwlane.sys,,,2
rtldata.txt,,,2
[RTWlanE.MSI.AddReg]
HKR, "Interrupt Management", 0x00000010 
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1
;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
RTWlanE.CopyFiles          = 12
DefaultDestDir             = 11        ; LDID_SYS
RtlUI2.CopyFiles           = 10
CoInstaller.CopyFiles      = 11
;;****************************************************************************
;; Source Files
;;****************************************************************************
[RtlUI2.CopyFiles]
RtlUI2.exe,,,2
[SourceDisksNames]
1 = %DISKNAME%,,,
[SourceDisksFiles]
rtwlane.sys = 1
rtldata.txt = 1
rtlCoInst.dll = 1
rtlCoInst.dat = 1
[CoInstaller.AddReg]
HKR,,CoInstallers32,0x10000,"rtlCoInst.DLL,rtlCoInst"

[CoInstaller.CopyFiles]
rtlCoInst.dll,,,0x04
rtlCoInst.dat,,,0x04
;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
Realtek     				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0000"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Channel"
NETWORK_TYPE_STR 			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"

TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
CHANNEL_PLAN_STR			= "Channel Plan"
WL_MODE_STR				= "Wireless Mode"
PREAMBLE_MODE_STR			= "Preamble Mode"
FRAGTHRESH_STR				= "Fragmentation Threshold"
RTSTHRESH_STR				= "RTS Threshold"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Disabled"
ENABLE_STR 				= "Enabled"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastructure"
AUTO_SELECT_STR 			= "Auto select"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spain"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"	
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Roam Retry Limit(sec)"
LEISURE_POWER_SAVE_STR			= "Leisure Power Save"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Beacon Interval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"


;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0009] ; English
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0009"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Channel"
NETWORK_TYPE_STR 			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
CHANNEL_PLAN_STR			= "Channel Plan"
WL_MODE_STR				= "Wireless Mode"
PREAMBLE_MODE_STR			= "Preamble Mode"
FRAGTHRESH_STR				= "Fragmentation Threshold"
RTSTHRESH_STR				= "RTS Threshold"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Disabled"
ENABLE_STR 				= "Enabled"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastructure"
AUTO_SELECT_STR 			= "Auto select"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
SHORT_PREAMBLE_STR 			= "Short Preamble"
LONG_SHORT_PREAMBLE_STR			= "Short & long"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spain"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Roam Retry Limit(sec)"
LEISURE_POWER_SAVE_STR			= "Leisure Power Save"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Beacon Interval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0404] ; Chinese (Traditional)
Realtek					= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0404"
SSID_STR 				= "服務組合識別碼"
CHANNEL_STR				= "通訊頻道"
NETWORK_TYPE_STR 			= "無線網路操作模式"
LED_CONTROL_STR				= "驅動程式控制 LED 閃爍模式" 
POWER_SAVE_STR				= "省電模式"
WIFI_IBSS_STR				= "對等式網路只使用 802.11b 標準"
RATE_ADAPTIVE_STR			= "適應性傳輸率調變自動化模式"
QOS_STR					= "流量管控"
WMM_APSD				= "WiFi 多媒體自動化省電參數 (WMM APSD)"
CCX_RM_STR				= "CCX 無線網路環境監控"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX 非連線頻道最大量測時間 (0: 無限大)"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "支援 PSP XLink 連線模式"
CHANNEL_PLAN_STR			= "頻道規劃"
WL_MODE_STR				= "無線網路標準"
PREAMBLE_MODE_STR			= "前序訊號模式"
FRAGTHRESH_STR				= "區段臨界值"
RTSTHRESH_STR				= "RTS 臨界值"
DOT11_ENABLE_STR			= "802.11d 無線頻道區域規範"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "禁用"
ENABLE_STR 				= "啟用"
CAM_STR 				= "無"
MAX_PSP_STR 				= "最大"
FAST_PSP_STR 				= "最小"
AD_HOC_STR 				= "對等式網路"
INFRASTRUCTURE_STR 			= "主從式網路"
AUTO_SELECT_STR 			= "自動選擇"
DOMAIN_FROM_EEPROM_STR 			= "硬體決定"
AUTO_STR 				= "自動選擇"
LONG_PREAMBLE_STR 			= "唯獨長前序訊號"
SHORT_PREAMBLE_STR 			= "短前序訊號"
LONG_SHORT_PREAMBLE_STR			= "長與短前序訊號"

FCC_STR 				= "FCC"

IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spain"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "漫遊重試限制（秒）"
LEISURE_POWER_SAVE_STR			= "空閒電力節省"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "信標間隔"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0011] ; Japanese
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0011"
SSID_STR 				= "SSID"
CHANNEL_STR				= "チャンネル"
NETWORK_TYPE_STR 			= "ネットワークの種類"
LED_CONTROL_STR				= "LEDコントロール" 
POWER_SAVE_STR				= "省電力モード"
WIFI_IBSS_STR				= "IBSS既定11bモード"
RATE_ADAPTIVE_STR			= "適応レート"
QOS_STR					= "QoS "
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCXラジオ測定"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX最大オフライン測定（0: 無制限）"
HW_PARA_STR				= "HwParaFileからのInit "
THREE_WIRE_MODE_STR			= "三線式プログラミングモード"
BOARD_TYPE_STR				= "基板の種類"
PROTECTION_MODE_STR			= "保護モード"
TPC_STR					= "送信電力制御"
TPC_POLARITY_STR			= "TPC極性選択"
HIGH_POWER_STR				= "高出力機構"
INIT_GAIN_STR				= "初期ゲイン状態"
CW_MAX_MIN_STR				= "コンテンションウィンドウ"
PSP_XLINK_STR				= "PSP XLinkモード"
CHANNEL_PLAN_STR			= "チャンネルプラン"
WL_MODE_STR				= "ワイヤレスモード"
PREAMBLE_MODE_STR			= "プレアンブルモード"
FRAGTHRESH_STR				= "フラグメンテーションしきい値"
RTSTHRESH_STR				= "RTSしきい値"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "無効"
ENABLE_STR 				= "有効"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "臨時"
INFRASTRUCTURE_STR 			= "インフラストラクチャ"
AUTO_SELECT_STR 			= "自動選択"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "自動"
LONG_PREAMBLE_STR 			= "長いプリアンブル"
SHORT_PREAMBLE_STR 			= "短いプリアンブル"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "スペイン"
FRANCE_STR 				= "フランス"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "イスラエル"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "ローミング再試行制限 (秒)"
LEISURE_POWER_SAVE_STR			= "レジャーパワーセーブ"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "ビーコン間隔"


ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0007] ; German
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0007"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanal"
NETWORK_TYPE_STR 			= "Netzwerktyp"
LED_CONTROL_STR				= "LED-Anzeige" 
POWER_SAVE_STR				= "Energiesparmodus"
WIFI_IBSS_STR				= "IBSS Default 11b Modus"
RATE_ADAPTIVE_STR			= "Ratenadaptive"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Funkmessung"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max. Offline Messung (0: unbeschrankt)"
HW_PARA_STR				= "Init. von HwParaFile"
THREE_WIRE_MODE_STR			= "Dreileiter-Programmiermodus"
BOARD_TYPE_STR				= "Kartentyp"
PROTECTION_MODE_STR			= "Schutzmodus"
TPC_STR					= "Ubertragungsleistungsstuerung"
TPC_POLARITY_STR			= "TPC Polaritatsauswahl"
HIGH_POWER_STR				= "Hochleistungsmechanismus"
INIT_GAIN_STR				= "Anfangl. Verstarkungszustand"
CW_MAX_MIN_STR				= "Konkurrenz-Fenster"
PSP_XLINK_STR				= "PSP XLink Modus"
CHANNEL_PLAN_STR			= "Kanalplan"
WL_MODE_STR				= "Wireless-Modus"
PREAMBLE_MODE_STR			= "Praambelmodus"
FRAGTHRESH_STR				= "Fragmentierungsschwelle"
RTSTHRESH_STR				= "RTS-Schwelle:"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Deaktivieren"
ENABLE_STR 				= "Aktivieren"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktur"
AUTO_SELECT_STR 			= "Autom. Auswahl"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Lange Praambel"
SHORT_PREAMBLE_STR 			= "Kurze Praambel"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spanien"
FRANCE_STR 				= "Frankreich"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Roaming-Wiederholungslimit (Sek.)"
LEISURE_POWER_SAVE_STR			= "Leerlauf-Energiesparen"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Bakenintervall"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.000c] ; French
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "000c"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Canal"
NETWORK_TYPE_STR 			= "Type de reseau"
LED_CONTROL_STR				= "Commande DEL" 
POWER_SAVE_STR				= "Mode economie d'energie"
WIFI_IBSS_STR				= "Mode 11b par defaut IBSS"
RATE_ADAPTIVE_STR			= "Debit adaptable"
QOS_STR					= "QoS"
WMM_APSD				= "APSD WMM"
CCX_RM_STR				= "Mesure radio CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Mesure hors ligne max. (0: illimitee)"

HW_PARA_STR				= "Init de HwParaFile"
THREE_WIRE_MODE_STR			= "Mode de programmation trois fils"
BOARD_TYPE_STR				= "Type de carte"
PROTECTION_MODE_STR			= "Mode de protection"
TPC_STR					= "Transmission du reglage"
TPC_POLARITY_STR			= "Choix de la polarite TPC"
HIGH_POWER_STR				= "Mecanisme grande puissance"
INIT_GAIN_STR				= "Etat du gain initial"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "Mode XLink PSP"
CHANNEL_PLAN_STR			= "Plan de canal"
WL_MODE_STR				= "Mode sans fil"
PREAMBLE_MODE_STR			= "Mode preambule"
FRAGTHRESH_STR				= "Seuil de fragmentation"
RTSTHRESH_STR				= "Seuil RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Desactiver"
ENABLE_STR 				= "Activer"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastructure"
AUTO_SELECT_STR 			= "Selection automatique"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "preambule long"
SHORT_PREAMBLE_STR 			= "Preambule court"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Espagne"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Limite essais roam (sec)"
LEISURE_POWER_SAVE_STR			= "Economie d'energie loisirs"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Intervalle balise "

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0010] ; Italian
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0010"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Canale"
NETWORK_TYPE_STR 			= "Tipo di rete"
LED_CONTROL_STR				= "Controllo LED" 
POWER_SAVE_STR				= "Modalita risparmio energetico"
WIFI_IBSS_STR				= "Modalita IBBS predefinita 11b"
RATE_ADAPTIVE_STR			= "Si adatta alla velocita"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "Misurazione radio CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Misurazione CCD max non in linea (0: illimitata)"
HW_PARA_STR				= "Init da HwParaFile"
THREE_WIRE_MODE_STR			= "Tre modalita di programmazione cablata"
BOARD_TYPE_STR				= "Tipo di piastra"

PROTECTION_MODE_STR			= "Modalita protezione"
TPC_STR					= "Trasmissione risparmio energetico"
TPC_POLARITY_STR			= "Selezione della polarita TPC"
HIGH_POWER_STR				= "Meccanismo ad alto potenziale"
INIT_GAIN_STR				= "Stato di guadagno iniziale"
CW_MAX_MIN_STR				= "Finestra di competizione"
PSP_XLINK_STR				= "Modalita PSP XLink"
CHANNEL_PLAN_STR			= "Piano canale"
WL_MODE_STR				= "Modalita wireless"
PREAMBLE_MODE_STR			= "Modalita preambolo"
FRAGTHRESH_STR				= "Soglia di frammentazione"
RTSTHRESH_STR				= "Soglia RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Disabilita"
ENABLE_STR 				= "Abilita"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruttura"
AUTO_SELECT_STR 			= "Selezione automatica"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Preambolo lungo"
SHORT_PREAMBLE_STR 			= "Preambolo breve"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spagna"
FRANCE_STR 				= "Francia"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israele"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Limite tentativi roam (sec)"
LEISURE_POWER_SAVE_STR			= "Risparmio energetico tempo libero"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Beacon Interval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.000a] ; Spanish
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "000a"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Canal"
NETWORK_TYPE_STR 			= "Tipo de red"
LED_CONTROL_STR				= "Control de LED" 
POWER_SAVE_STR				= "Modo de ahorro de energia"
WIFI_IBSS_STR				= "Modo 11b predeterminado IBSS"
RATE_ADAPTIVE_STR			= "Velocidad adaptable"
QOS_STR					= "QoS"
WMM_APSD				= "APSD WMM"
CCX_RM_STR				= "Medicion de radio CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Medicion sin conexion maxima CCX (0: sin limite)"
HW_PARA_STR				= "Inicio desde HwParaFile"
THREE_WIRE_MODE_STR			= "Modo de programacion de tres cables"
BOARD_TYPE_STR				= "Tipo de tablero"
PROTECTION_MODE_STR			= "Modo de proteccion"
TPC_STR					= "Transmitir control de potencia"
TPC_POLARITY_STR			= "Seleccionar polaridad TPC"
HIGH_POWER_STR				= "Mecanismo de alta potencia"
INIT_GAIN_STR				= "Estado de ganancia inicial"
CW_MAX_MIN_STR				= "Ventana de discusiones"
PSP_XLINK_STR				= "Modo XLink PSP"
CHANNEL_PLAN_STR			= "Plan de canal"
WL_MODE_STR				= "Modo inalambrico"
PREAMBLE_MODE_STR			= "Modo de preambulo"
FRAGTHRESH_STR				= "Umbral de fragmentacion"
RTSTHRESH_STR				= "Umbral RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Deshabilitar"
ENABLE_STR 				= "Habilitar"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "PSP_rapido"
AD_HOC_STR 				= "Especial"
INFRASTRUCTURE_STR 			= "Infraestructura"
AUTO_SELECT_STR 			= "Seleccion automatica"
DOMAIN_FROM_EEPROM_STR 			= "DOMINIO_DE_EEPROM"
AUTO_STR 				= "Automatico"
LONG_PREAMBLE_STR 			= "Preambulo largo"
SHORT_PREAMBLE_STR 			= "Preambulo corto"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Espana"
FRANCE_STR 				= "Francia"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Limite de reintentos en transito (seg)"
LEISURE_POWER_SAVE_STR			= "Ahorro de energia por inactividad"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Intervalo de baliza"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0c04] ; Chinese (Traditional) (Hong Kong)
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0c04"
SSID_STR				= "服務組合識別碼"
CHANNEL_STR				= "通訊頻道"
NETWORK_TYPE_STR			= "無線網路操作模式"
LED_CONTROL_STR				= "驅動程式控制 LED 閃爍模式" 
POWER_SAVE_STR				= "省電模式"
WIFI_IBSS_STR				= "對等式網路只使用 802.11b 標準"
RATE_ADAPTIVE_STR			= "適應性傳輸率調變自動化模式"
QOS_STR					= "流量管控"
WMM_APSD				= "WiFi 多媒體自動化省電參數 (WMM APSD)"
CCX_RM_STR				= "CCX 無線網路環境監控"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX 非連線頻道最大量測時間 (0: 無限大)"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "支援 PSP XLink 連線模式"
CHANNEL_PLAN_STR			= "頻道規劃"
WL_MODE_STR				= "無線網路標準"
PREAMBLE_MODE_STR			= "前序訊號模式"
FRAGTHRESH_STR				= "區段臨界值"
RTSTHRESH_STR				= "RTS 臨界值"
DOT11_ENABLE_STR			= "802.11d 無線頻道區域規範"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "禁用"
ENABLE_STR 				= "啟用"
CAM_STR 				= "無"
MAX_PSP_STR 				= "最大"
FAST_PSP_STR 				= "最小"
AD_HOC_STR 				= "對等式網路"
INFRASTRUCTURE_STR 			= "主從式網路"
AUTO_SELECT_STR 			= "自動選擇"
DOMAIN_FROM_EEPROM_STR 			= "硬體決定"
AUTO_STR 				= "自動選擇"
LONG_PREAMBLE_STR 			= "長前序訊號"
SHORT_PREAMBLE_STR 			= "短前序訊號"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spain"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "漫遊重試上限（秒）"
LEISURE_POWER_SAVE_STR			= "閑置中電源管理"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "信標間隔"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0804] ; Chinese (Simplified)
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0804"
SSID_STR 				= "SSID"
CHANNEL_STR				= "频道"
NETWORK_TYPE_STR 			= "网络类型"
LED_CONTROL_STR				= "LED 控制" 
POWER_SAVE_STR				= "省电模式"
WIFI_IBSS_STR				= "IBSS 默认 11b 模式"
RATE_ADAPTIVE_STR			= "速率适应"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX 无线电测量"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX 最大脱机测量（0：无限制）"
HW_PARA_STR				= "从硬件参数文件初始化"
THREE_WIRE_MODE_STR			= "三线编程模式"
BOARD_TYPE_STR				= "板子类型"
PROTECTION_MODE_STR			= "保护模式"
TPC_STR					= "发射功率控制"
TPC_POLARITY_STR			= "TPC 极性选择"
HIGH_POWER_STR				= "高功率机制"
INIT_GAIN_STR				= "初始增益状态"
CW_MAX_MIN_STR				= "争用窗口"
PSP_XLINK_STR				= "PSP XLink 模式"
CHANNEL_PLAN_STR			= "频道计划"
WL_MODE_STR				= "无线模式"
PREAMBLE_MODE_STR			= "前导码模式"
FRAGTHRESH_STR				= "碎片阈值"
RTSTHRESH_STR				= "RTS 阈值"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "禁用"
ENABLE_STR 				= "启用"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "对等网络"
INFRASTRUCTURE_STR 			= "基础架构"
AUTO_SELECT_STR 			= "自动选择"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "自动"
LONG_PREAMBLE_STR 			= "长前导码"
SHORT_PREAMBLE_STR 			= "短前导码"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "西班牙"
FRANCE_STR 				= "法国"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "以色列"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "漫游重试限制(秒)"
LEISURE_POWER_SAVE_STR			= "空闲省电"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "信标间隔"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0012] ; Korean
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0012"
SSID_STR				= "SSID"
CHANNEL_STR				= "채널"
NETWORK_TYPE_STR			= "네트워크 종류"
LED_CONTROL_STR				= "LED 제어" 
POWER_SAVE_STR				= "절전 모드"
WIFI_IBSS_STR				= "IBSS 기본 11b 모드"

RATE_ADAPTIVE_STR			= "속도 적응"
QOS_STR					= " QoS "
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX 무선 측정"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX 최대 오프라인 측정(0: 제한 없음)"
HW_PARA_STR				= "HwParaFile에서 초기화"
THREE_WIRE_MODE_STR			= "3선 식 프로그래밍 모드"
BOARD_TYPE_STR				= "보드 종류"
PROTECTION_MODE_STR			= "보호 모드"

TPC_STR					= "송신 출력 제어"
TPC_POLARITY_STR			= "TPC 극성 선택"
HIGH_POWER_STR				= "고출력 메커니즘"
INIT_GAIN_STR				= "초기 게인 상태"
CW_MAX_MIN_STR				= "경합 창"
PSP_XLINK_STR				= "PSP XLink 모드"

CHANNEL_PLAN_STR			= "채널 계획"
WL_MODE_STR				= "무선 모드"
PREAMBLE_MODE_STR			= "프리앰블 모드"
FRAGTHRESH_STR 				= "조각화 임계값"
RTSTHRESH_STR				= "RTS 임계값"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "사용 안 함"
ENABLE_STR 				= "사용"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "애드혹"
INFRASTRUCTURE_STR 			= "인프라"
AUTO_SELECT_STR 			= "자동 선택"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "자동"
LONG_PREAMBLE_STR 			= "긴 프리앰블"
SHORT_PREAMBLE_STR 			= "짧은 프리앰블"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "스페인"
FRANCE_STR 				= "프랑스"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "이스라엘"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "로밍 재시도 제한시간(초)"
LEISURE_POWER_SAVE_STR			= "대기 절전"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "비컨 간격"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0013] ; Dutch
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0013"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanaal"
NETWORK_TYPE_STR 			= "Netwerktype"
LED_CONTROL_STR				= "LED-besturing" 
POWER_SAVE_STR				= "Spaarstandmodus"
WIFI_IBSS_STR				= "IBSS standaard 11b-modus"
RATE_ADAPTIVE_STR			= "Aanpasbare snelheid"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX-radiometing"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX max. verschuivingsmeting (0: onbeperkt)"
HW_PARA_STR				= "Init van HwParaFile"
THREE_WIRE_MODE_STR			= "Driedraads programmeermodus"
BOARD_TYPE_STR				= "Bordtype"
PROTECTION_MODE_STR			= "Beveiligingsmodus"
TPC_STR					= "Zendvermogenbeheer"
TPC_POLARITY_STR			= "Selectie TPC-polariteit"

HIGH_POWER_STR				= "Mechanisme met hoog vermogen"
INIT_GAIN_STR				= "Eerste versterkingsstatus"
CW_MAX_MIN_STR				= "Conflictvenster"
PSP_XLINK_STR				= "PSP XLink-modus"
CHANNEL_PLAN_STR			= "Kanaalplan"
WL_MODE_STR				= "Draadloze modus"
PREAMBLE_MODE_STR			= "Preambulemodus"
FRAGTHRESH_STR				= "Fragmentatiedrempel"
RTSTHRESH_STR				= "RTS-drempel"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Uitschakelen"
ENABLE_STR 				= "Inschakelen"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad hoc"
INFRASTRUCTURE_STR 			= "Infrastructuur"
AUTO_SELECT_STR 			= "Auto selectie"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Lange preambule"
SHORT_PREAMBLE_STR 			= "Korte preambule"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spanje"
FRANCE_STR 				= "Frankrijk"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Limiet van roamingspogingen(sec)"
LEISURE_POWER_SAVE_STR			= "Energiebesparing"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Bakeninterval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0014] ; Norwegian
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0014"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanal"
NETWORK_TYPE_STR 			= "Nettverkstype"
LED_CONTROL_STR				= "LED-kontroll" 
POWER_SAVE_STR				= "Stromsparingsmodus"
WIFI_IBSS_STR				= "IBSS standard 11b-modus"
RATE_ADAPTIVE_STR			= "Hastighet adaptiv"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radiomaling"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX maks offline-maling (0: ubegrenset)"
HW_PARA_STR				= "Init fra HwParaFile"
THREE_WIRE_MODE_STR			= "Tre tradet programmeringsmodus"
BOARD_TYPE_STR				= "Korttype"
PROTECTION_MODE_STR			= "Beskyttelsesmodus"
TPC_STR					= "Stromsendingskontroll"
TPC_POLARITY_STR			= "Velg TPC-polaritet"
HIGH_POWER_STR				= "Hoystyrke-mekanisme"
INIT_GAIN_STR				= "Opprinnelig okningstilstand"
CW_MAX_MIN_STR				= "Konflikt-vindu"
PSP_XLINK_STR				= "PSP XLink-modus"
CHANNEL_PLAN_STR			= "Kanalplan"
WL_MODE_STR				= "Tradlos modus"
PREAMBLE_MODE_STR			= "Innledende modus"
FRAGTHRESH_STR				= "Fragmenteringsgrense"
RTSTHRESH_STR				= "RTS-grense"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Deaktiver"
ENABLE_STR 				= "Aktiver"
CAM_STR 				= "KAM"
MAX_PSP_STR 				= "MAKS_PSP"
FAST_PSP_STR 				= "Rask_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktur"
AUTO_SELECT_STR 			= "Autovelg"
DOMAIN_FROM_EEPROM_STR 			= "DOMENE_FRA_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Lang innledning"
SHORT_PREAMBLE_STR 			= "Kort innledning"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spania"
FRANCE_STR 				= "Frankrike"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Repeteringsgrense (i sek.) for roaming"
LEISURE_POWER_SAVE_STR			= "Stromsparing ved uvirksomhet"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Blinkintervall"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.001d] ; Swedish
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "001d"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanal"
NETWORK_TYPE_STR 			= "Natverkstyp"
LED_CONTROL_STR				= "LED-kontroll" 
POWER_SAVE_STR				= "Energisparlage"
WIFI_IBSS_STR				= "IBSS standard 11b Mode"
RATE_ADAPTIVE_STR			= "Anpassningsbar hastighet"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX radiomatning"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Offline matning (0: obegransat)"
HW_PARA_STR				= "Init fran HwParaFile"
THREE_WIRE_MODE_STR			= "Tretrads programmeringslage"
BOARD_TYPE_STR				= "Korttyp"
PROTECTION_MODE_STR			= "Skyddslage"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR			= "Valj TPC-polaritet"
HIGH_POWER_STR				= "Hogkraftsmekanism"
INIT_GAIN_STR				= "Ursprungligt forstarkningslage"
CW_MAX_MIN_STR				= "Konkurrensfonster"
PSP_XLINK_STR				= "PSP XLink-lage"
CHANNEL_PLAN_STR			= "Kanalplan"
WL_MODE_STR				= "Tradlost lage"
PREAMBLE_MODE_STR			= "Inledningslage"
FRAGTHRESH_STR				= "Fragmenteringstroskel"
RTSTHRESH_STR				= "RTS-troskel"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Inaktivera"
ENABLE_STR 				= "Aktivera"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktur"
AUTO_SELECT_STR 			= "Autoval"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Lang inledning"
SHORT_PREAMBLE_STR 			= "Kort inledning"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spanien"
FRANCE_STR 				= "Frankrike"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Grans for nytt roamingforsok (sek)"
LEISURE_POWER_SAVE_STR			= "Leisure energibesparning"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Fyrintervall"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0006] ; Danish
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0006"
SSID_STR				= "SSID"
CHANNEL_STR				= "Kanal"
NETWORK_TYPE_STR 			= "Netvarkstype"
LED_CONTROL_STR				= "LED-kontrol" 
POWER_SAVE_STR				= "Stromstyrings-tilstand"
WIFI_IBSS_STR				= "IBSS standard 11b-tilstand"
RATE_ADAPTIVE_STR			= "Hastighed tilpasset"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX radiomaling"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX maks. offline-maling (0: ubegranset)"
HW_PARA_STR				= "Init. fra HwParaFile"
THREE_WIRE_MODE_STR			= "Tre ledninger programmering-tilstand"
BOARD_TYPE_STR				= "Korttype"
PROTECTION_MODE_STR			= "Beskyttelse-tilstand"
TPC_STR					= "Overfor strom-kontrol"
TPC_POLARITY_STR			= "Valg TPC polaritet"
HIGH_POWER_STR				= "Hojeffekt-mekanisme"
INIT_GAIN_STR				= "Initiel forstarkning-tilstand"
CW_MAX_MIN_STR				= "Konflikt-vindue"
PSP_XLINK_STR				= "PSP XLink-tilstand"
CHANNEL_PLAN_STR			= "Kanal-plan"
WL_MODE_STR				= "Tradlos-tilstand"
PREAMBLE_MODE_STR			= "Start-tilstand"
FRAGTHRESH_STR				= "Fragmenteringstarskel"
RTSTHRESH_STR				= "RTS-tarskel"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Deaktiver"
ENABLE_STR 				= "Aktiver"
CAM_STR 				= "KAM"
MAX_PSP_STR 				= "MAKS._PSP"
FAST_PSP_STR 				= "Hurtig_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktur"
AUTO_SELECT_STR 			= "Auto-valg"
DOMAIN_FROM_EEPROM_STR 			= "DOMANE_FRA_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Lang preamble"
SHORT_PREAMBLE_STR 			= "Kort preamble"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spanien"
FRANCE_STR 				= "Frankrig"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Begransning for gentagne roam forsog (sek)"
LEISURE_POWER_SAVE_STR			= "Fritid - stromstyring"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Lys interval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.000b] ; Finnsih
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "000b"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanava"
NETWORK_TYPE_STR 			= "Verkkotyyppi"
LED_CONTROL_STR				= "LED-hallinta" 
POWER_SAVE_STR				= "Virransaastotila"
WIFI_IBSS_STR				= "IBSS-oletus 11b-tila"
RATE_ADAPTIVE_STR			= "Nopeuteen mukautuva"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX-radiomittaus"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX-maksimi-offline-mittaus (0: rajoittamaton)"
HW_PARA_STR				= "Alustus HwParaFilesta"
THREE_WIRE_MODE_STR			= "Kolmen langan ohjelmointitila"
BOARD_TYPE_STR				= "Levytyyppi"
PROTECTION_MODE_STR			= "Suojaustila"
TPC_STR					= "Virranhallinnan siirto"
TPC_POLARITY_STR			= "TPC-polariteetin valinta"
HIGH_POWER_STR				= "Korkeatehomekanismi"
INIT_GAIN_STR				= "Ensimmainen vahvistustila"
CW_MAX_MIN_STR				= "Vaiteikkuna"
PSP_XLINK_STR				= "PSP XLink -tila"
CHANNEL_PLAN_STR			= "Kanavasuunnitelma"
WL_MODE_STR				= "Langaton tila"
PREAMBLE_MODE_STR			= "Synkronointitila"
FRAGTHRESH_STR				= "Sirpaleisuuden kynnys"
RTSTHRESH_STR				= "RTS-kynnys"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Pois paalta"
ENABLE_STR 				= "Paalle"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktuuri"
AUTO_SELECT_STR 			= "Automaattinen valinta"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Autom."
LONG_PREAMBLE_STR 			= "Pitka tahdistuskuvio"
SHORT_PREAMBLE_STR 			= "Lyhyt tahdistuskuvio"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Espanja"
FRANCE_STR 				= "Ranska"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Roamingin uudelleen yrittamisen rajoitus (sek.)"
LEISURE_POWER_SAVE_STR			= "Joutenolon virransaasto"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Paikkatietopakettien intervalli"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0019] ; Russian
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0019"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Канал"
NETWORK_TYPE_STR 			= "Тип сети"
LED_CONTROL_STR				= "Индикатор" 
POWER_SAVE_STR				= "Режим энергосбережения"
WIFI_IBSS_STR				= "Режим IBSS Default 11b"
RATE_ADAPTIVE_STR			= "Адаптивная скорость"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: неограниченно)"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Режим Three Wire Programming Mode"
BOARD_TYPE_STR				= "Тип карты"
PROTECTION_MODE_STR			= "Защищенный режим"
TPC_STR					= "Управление мощностью передачи"
TPC_POLARITY_STR			= "Выбор полярности TPC"
HIGH_POWER_STR				= "Повышение мощности"
INIT_GAIN_STR				= "Первоначальное состояние усиления"
CW_MAX_MIN_STR				= "Окно соединения"
PSP_XLINK_STR				= "Режим PSP XLink"
CHANNEL_PLAN_STR			= "План каналов"
WL_MODE_STR				= "Режим беспроводной связи"
PREAMBLE_MODE_STR			= "Тип преамбулы"
FRAGTHRESH_STR				= "Порог фрагментации"
RTSTHRESH_STR				= "Порог RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Отключено"
ENABLE_STR 				= "Включено"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Прямое подключение"
INFRASTRUCTURE_STR 			= "Инфраструктура"
AUTO_SELECT_STR 			= "Автовыбор"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Авто"
LONG_PREAMBLE_STR 			= "Длинная преамбула"
SHORT_PREAMBLE_STR 			= "Короткая преамбула"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Испания"
FRANCE_STR 				= "Франция"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Израиль"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Лимит повтора роуминга (с)"
LEISURE_POWER_SAVE_STR			= "Энергосбережение при простое"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Интервал маяка"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0005] ; Czech
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0005"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanál"
NETWORK_TYPE_STR 			= "Typ sítě"
LED_CONTROL_STR				= "Indikátor LED" 
POWER_SAVE_STR				= "Režim úspory napájení"
WIFI_IBSS_STR				= "Výchozí režim IBSS 11b"
RATE_ADAPTIVE_STR			= "Přizpůsobivé na rychlost"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "Měření rádia CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Max. měření offline CCX (0: neomezeno)"
HW_PARA_STR				= "Inic z HwParaFile"
THREE_WIRE_MODE_STR			= "Režim programování Three Wire"
BOARD_TYPE_STR				= "Typ desky"
PROTECTION_MODE_STR			= "Režim ochrany"
TPC_STR					= "Řízení napájení přenosu"
TPC_POLARITY_STR			= "Výběr polarity TPC"
HIGH_POWER_STR				= "Mechanizmus s vysokým výkonem"
INIT_GAIN_STR				= "Počáteční stav zesílení"
CW_MAX_MIN_STR				= "Okno připojení"
PSP_XLINK_STR				= "Režim PSP XLink"
CHANNEL_PLAN_STR			= "Kanálový plán"
WL_MODE_STR				= "Bezdrátový režim"
PREAMBLE_MODE_STR			= "Režim preambule"
FRAGTHRESH_STR				= "Fragmentování prahové hodnoty"
RTSTHRESH_STR				= "Práh RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Deaktivovat"
ENABLE_STR 				= "Aktivovat"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Rychlý_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktura"
AUTO_SELECT_STR 			= "Automatický výběr"
DOMAIN_FROM_EEPROM_STR 			= "DOMÉNA_Z_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Dlouhá preambule"
SHORT_PREAMBLE_STR 			= "Krátká preambule"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Španělsko"
FRANCE_STR 				= "Francie"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Izrael"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Limit opakovaného pokusu o roaming(s.)"
LEISURE_POWER_SAVE_STR			= "Úsporný režim pro volný čas"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Interval blikání"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0015] ; Polsih
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0015"
SSID_STR				= "SSID"
CHANNEL_STR				= "Kanał"
NETWORK_TYPE_STR			= "Rozdaj sieci"
LED_CONTROL_STR				= "Wskaźnik LED " 
POWER_SAVE_STR				= "Tryb oszczędzania energii"
WIFI_IBSS_STR				= "Tryb domyślny IBSS 11b "
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"

CCX_RM_STR				= "Pomiar sygnału radiowego CCX "
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Pomiar maks. CCX off-line (0: nieograniczony)"
HW_PARA_STR				= "Inic z HwParaFile"
THREE_WIRE_MODE_STR			= "Trzyprzewodowy tryb programowania"
BOARD_TYPE_STR				= "Rodzaj płyty"
PROTECTION_MODE_STR			= "Tryb zabezpieczenia"
TPC_STR					= "Kontrola mocy nadawanej"
TPC_POLARITY_STR			= "Wybór biegunowości TPC "
HIGH_POWER_STR				= "Mechanizm wysokiej mocy"
INIT_GAIN_STR				= "Stan początkowego wzrostu"
CW_MAX_MIN_STR				= "Okno rywalizacji"
PSP_XLINK_STR				= "Tryb PSP XLink "
CHANNEL_PLAN_STR			= "Plan kanałów"
WL_MODE_STR				= "Tryb bezprzewodowy"
PREAMBLE_MODE_STR			= "Tryb preambuły"
FRAGTHRESH_STR				= "Próg fragmentacji"
RTSTHRESH_STR				= "Próg RTS "
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Wyłącz"
ENABLE_STR 				= "Włącz"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktura"
AUTO_SELECT_STR 			= "Automatyczne wybieranie"
DOMAIN_FROM_EEPROM_STR 			= "DOMENA_Z_EEPROM"
AUTO_STR 				= "Automatyczny"
LONG_PREAMBLE_STR 			= "Długa preambuła"
SHORT_PREAMBLE_STR 			= "Krótka preambuła "
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Hiszpania"
FRANCE_STR 				= "Francja"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Izrael"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Ograniczenie czasu wędrówki (sek.)"
LEISURE_POWER_SAVE_STR			= "Ograniczenie zużycia energii poza pracą"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Częstotliwość wysyłania ramek"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.001f] ; Turkish
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "001f"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanal"
NETWORK_TYPE_STR 			= "Ağ Tipi"
LED_CONTROL_STR				= "LED Kontrolü" 
POWER_SAVE_STR				= "Güç Tasarruf Modu"
WIFI_IBSS_STR				= "IBSS Varsayılan 11b Modu"
RATE_ADAPTIVE_STR			= "Uyarlanır Oran"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radyo Ölçümü"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Maks Kapalı Hat Ölçümü (0: limitsiz)"
HW_PARA_STR				= "HwParaFile'dan Başlat"
THREE_WIRE_MODE_STR			= "Üç Kablo Programlama Modu"
BOARD_TYPE_STR				= "Kart Tipi"
PROTECTION_MODE_STR			= "Koruma Modu"
TPC_STR					= "İletim Gücü Denetimi"
TPC_POLARITY_STR			= "TPC Kutupsallık Seçimi"
HIGH_POWER_STR				= "Yüksek Güçlü Mekanizma"
INIT_GAIN_STR				= "İlk Edinim Durumu"
CW_MAX_MIN_STR				= "Tartışma Penceresi"
PSP_XLINK_STR				= "PSP XLink Modu"
CHANNEL_PLAN_STR			= "Kanal Planı"
WL_MODE_STR				= "Kablosuz Modu"
PREAMBLE_MODE_STR			= "Başlangıç Modu"
FRAGTHRESH_STR				= "Fragmentasyon Eşiği"
RTSTHRESH_STR				= "RTS Eşiği"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Devredışı Bırak"
ENABLE_STR 				= "Etkinleştir"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"

FAST_PSP_STR 				= "Hızlı_PSP"
AD_HOC_STR 				= "Geçici"
INFRASTRUCTURE_STR 			= "Altyapı"
AUTO_SELECT_STR 			= "Otomatik Seç"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Otomatik"
LONG_PREAMBLE_STR 			= "Uzun Başlangıç"
SHORT_PREAMBLE_STR 			= "Kısa Başlangıç"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "İspanya"
FRANCE_STR 				= "Fransa"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "İsrail"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Dolaşım Modu Yeniden Deneme Sınırı (sn)"
LEISURE_POWER_SAVE_STR			= "Boş Zaman Güç Tasarrufu"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "İşaret Aralığı"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.000e] ; Hungarian
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "000e"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Csatorna"
NETWORK_TYPE_STR 			= "Hálózat típusa"
LED_CONTROL_STR				= "LED-vezérlés" 
POWER_SAVE_STR				= "Energiatakarékos mód"
WIFI_IBSS_STR				= "IBSS alapértelmezett 11b mód"
RATE_ADAPTIVE_STR			= "Adaptív sebességválasztás"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX rádiómérés"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line mérés (0: korlátlan)"
HW_PARA_STR				= "Inicializálás innen: HwParaFile"
THREE_WIRE_MODE_STR			= "Háromvezetékes programozási mód"
BOARD_TYPE_STR				= "Paneltípus"
PROTECTION_MODE_STR			= "Védett mód"
TPC_STR					= "Sugárzási teljesítményvezérlés"

TPC_POLARITY_STR			= "TPC polaritás választás"
HIGH_POWER_STR				= "Nagyteljesítményű mechanizmus"
INIT_GAIN_STR				= "Kezdeti erősítési állapot"
CW_MAX_MIN_STR				= "Vetélkedési ablak"
PSP_XLINK_STR				= "PSP XLink mód"
CHANNEL_PLAN_STR			= "Csatornaterv"

WL_MODE_STR				= "Vezeték nélküli mód"
PREAMBLE_MODE_STR			= "Előtag mód"
FRAGTHRESH_STR				= "Tördelési küszöb"
RTSTHRESH_STR				= "RTS küszöb"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Letiltás"
ENABLE_STR 				= "Engedélyezés"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktúra"
AUTO_SELECT_STR 			= "Automata választás"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Automata"
LONG_PREAMBLE_STR 			= "Hosszú előtag"
SHORT_PREAMBLE_STR 			= "Rövid előtag"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spanyolország"
FRANCE_STR 				= "Franciaország"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Izrael"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Barangolás újraindításának időkorlátja (mp)"
LEISURE_POWER_SAVE_STR			= "Energiatakarékos mód szórakoztató eszközökhöz"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Jelzés időköze"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0008] ; Greek
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0008"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Κανάλι"
NETWORK_TYPE_STR 			= "Τύπος Δικτύου"
LED_CONTROL_STR				= "Ενδείξεις λυχνιών LED" 
POWER_SAVE_STR				= "Λειτουργία εξοικονόμησης ενέργειας"
WIFI_IBSS_STR				= "IBSS Προεπιλεγμένη λειτουργία 11b"
RATE_ADAPTIVE_STR			= "Προσαρμόσιμη ταχύτητα"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "Ραδιομέτρηση CCX"

CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Μέγιστη μέτρηση εκτός σύνδεσης CCX (0: απεριόριστο)"
HW_PARA_STR				= "Αρχικοποίηση από HwParaFile"
THREE_WIRE_MODE_STR			= "Λειτουργία προγραμματισμού τριών καλωδίων"
BOARD_TYPE_STR				= "Τύπος κάρτας"
PROTECTION_MODE_STR			= "Λειτουργία προστασίας"
TPC_STR					= "Έλεγχος μετάδοσης ισχύος"
TPC_POLARITY_STR			= "Επιλογή πολικότητας TPC"
HIGH_POWER_STR				= "Μηχανισμός υψηλής ισχύος"
INIT_GAIN_STR				= "Κατάσταση αρχικού οφέλους"
CW_MAX_MIN_STR				= "Παράθυρο διεκδίκησης"
PSP_XLINK_STR				= "Λειτουργία PSP XLink"
CHANNEL_PLAN_STR			= "Σχέδιο καναλιού"
WL_MODE_STR				= "Λειτουργία ασύρματου"
PREAMBLE_MODE_STR			= "Λειτουργία μπλοκ εισαγωγής"
FRAGTHRESH_STR				= "Κατώφλι τμήματος"
RTSTHRESH_STR				= "Κατώφλι RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Απενεργοποίηση"
ENABLE_STR 				= "Ενεργοποίηση"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Λειτουργία Ad-hoc"
INFRASTRUCTURE_STR 			= "Υποδομή"
AUTO_SELECT_STR 			= "Αυτόματη επιλογή"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Αυτόματο"
LONG_PREAMBLE_STR 			= "Μεγάλο μπλοκ εισαγωγής"
SHORT_PREAMBLE_STR 			= "Μικρό μπλοκ εισαγωγής"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Ισπανία"
FRANCE_STR 				= "Γαλλία"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Ισραήλ"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Όριο επαναλήψεων προσπάθειας περιαγωγής (δευτ.)"
LEISURE_POWER_SAVE_STR			= "Εξοικονόμηση ενέργειας σε κατάσταση αδράνειας"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Διάστημα προειδοποιητικού σήματος"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.001b] ; Slovak
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "001b"
SSID_STR				= "SSID"
CHANNEL_STR				= "แชนเนล"
NETWORK_TYPE_STR			= "ชนิดเน็ตเวิร์ก"
LED_CONTROL_STR				= "LED ควบคุม" 
POWER_SAVE_STR				= "โหมดประหยัดพลังงาน"
WIFI_IBSS_STR				= "โหมด IBSS เริ่มต้น 11b "
RATE_ADAPTIVE_STR			= "อัตราอะแดปทีฟ"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "การวัดวิทยุ CCX "
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "การวัด CCX ออฟไลน์สูงสุด (0: ไม่จำกัด)"
HW_PARA_STR				= "ตั้งค่าเริ่มต้นจาก HwParaFile"
THREE_WIRE_MODE_STR			= "โหมดการโปรแกรม 3 สาย"
BOARD_TYPE_STR				= "ชนิดบอร์ด"
PROTECTION_MODE_STR			= "โหมดการป้องกัน"
TPC_STR					= "ควบคุมพลังงานการส่ง"
TPC_POLARITY_STR			= "เลือกขั้ว TPC "
HIGH_POWER_STR				= "กลไกพลังงานสูง"
INIT_GAIN_STR				= "สถานะเกนเริ่มแรก"
CW_MAX_MIN_STR				= "หน้าต่างการยืนยัน"
PSP_XLINK_STR				= "โหมด PSP XLink "
CHANNEL_PLAN_STR			= "แผนแชนเนล"
WL_MODE_STR				= "โหมดไร้สาย"
PREAMBLE_MODE_STR			= "โหมดส่วนเริ่มต้น"
FRAGTHRESH_STR				= "ขอบเขตชิ้นส่วน"
RTSTHRESH_STR				= "ขอบเขต RTS "
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "ปิดทำงาน"
ENABLE_STR 				= "เปิดทำงาน"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "โครงสร้างพื้นฐาน"
AUTO_SELECT_STR 			= "เลือกอัตโนมัติ"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "อัตโนมัติ"
LONG_PREAMBLE_STR 			= "ส่วนเริ่มต้นยาว"
SHORT_PREAMBLE_STR 			= "ส่วนเริ่มต้นสั้น"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "สเปน"
FRANCE_STR 				= "ฝรั่งเศส"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "อิสราเอล"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "ขีดจำกัดการลองโรมใหม่ (วินาที)"
LEISURE_POWER_SAVE_STR			= "การประหยัดพลังงานขณะที่ว่าง"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "ช่วงไฟสัญญาณ"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0401] ; Arabic (Saudi Arabia)
Realtek 				= "شركة Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0401"
SSID_STR				= "معرف SSID"
CHANNEL_STR				= "القناة"
NETWORK_TYPE_STR			= "نوع الشبكة"
LED_CONTROL_STR				= "التحكم في مؤشر بيان الحالة" 
POWER_SAVE_STR				= "وضع توفير الطاقة"
WIFI_IBSS_STR				= "وضع 11b الافتراضي لـ IBSS"
RATE_ADAPTIVE_STR			= "مهايئ المعدل"
QOS_STR					= "جودة الخدمة"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "القياس اللاسلكي لـ CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "الحد الأقصى لقياس CCX عند عدم الاتصال (0: غير محدود)"
HW_PARA_STR				= "بدء التهيئة من ملف HwparaFile"
THREE_WIRE_MODE_STR			= "وضع البرمجة ثلاثي الأسلاك"
BOARD_TYPE_STR				= "نوع اللوحة"
PROTECTION_MODE_STR			= "وضع الحماية"
TPC_STR					= "نقل التحكم في الطاقة"
TPC_POLARITY_STR			= "تحديد قطبية TPC"
HIGH_POWER_STR				= "آلية الطاقة المرتفعة"
INIT_GAIN_STR				= "حالة الكسب الأولية"
CW_MAX_MIN_STR				= "نافذة التعارض"
PSP_XLINK_STR				= "وضع PSP XLink"
CHANNEL_PLAN_STR			= "خطة القناة"
WL_MODE_STR				= "الوضع اللاسلكي"
PREAMBLE_MODE_STR			= "وضع الإشارة الابتدائية"
FRAGTHRESH_STR				= "حد التجزئة"
RTSTHRESH_STR				= "حد RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "تعطيل"
ENABLE_STR 				= "تمكين"
CAM_STR 				= "الكامة"
MAX_PSP_STR 				= "الحد الأقصى لـ PSP"
FAST_PSP_STR 				= "PSP سريع"
AD_HOC_STR 				= "عشوائي"
INFRASTRUCTURE_STR 			= "البنية الأساسية"
AUTO_SELECT_STR 			= "تحديد تلقائي"
DOMAIN_FROM_EEPROM_STR 			= "المجال من EEPROM"
AUTO_STR 				= "تلقائي"
LONG_PREAMBLE_STR 			= "إشارة ابتدائية طويلة"
SHORT_PREAMBLE_STR 			= "إشارة ابتدائية قصيرة"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "اللجنة الفيدرالية للاتصالات"
IC_STR 					= "دائرة متكاملة"
ETSI_STR 				= "معهد معايير الاتصالات السلكية واللاسلكية"
SPAIN_STR 				= "إسبانيا"
FRANCE_STR 				= "فرنسا"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "إسرائيل"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "حد تكرار التجوال (بالثواني)"
LEISURE_POWER_SAVE_STR			= "توفير الطاقة عند عدم الاستخدام"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "فاصل Beacon الزمني"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.2401] ; Arabic (Yemen)
Realtek 				= "شركة Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "2401"
SSID_STR				= "معرف SSID"
CHANNEL_STR				= "القناة"
NETWORK_TYPE_STR			= "نوع الشبكة"
LED_CONTROL_STR				= "التحكم في مؤشر بيان الحالة" 
POWER_SAVE_STR				= "وضع توفير الطاقة"
WIFI_IBSS_STR				= "وضع 11b الافتراضي لـ IBSS"
RATE_ADAPTIVE_STR			= "مهايئ المعدل"
QOS_STR					= "جودة الخدمة"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "القياس اللاسلكي لـ CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "الحد الأقصى لقياس CCX عند عدم الاتصال (0: غير محدود)"
HW_PARA_STR				= "بدء التهيئة من ملف HwparaFile"
THREE_WIRE_MODE_STR			= "وضع البرمجة ثلاثي الأسلاك"
BOARD_TYPE_STR				= "نوع اللوحة"
PROTECTION_MODE_STR			= "وضع الحماية"
TPC_STR					= "نقل التحكم في الطاقة"
TPC_POLARITY_STR			= "تحديد قطبية TPC"
HIGH_POWER_STR				= "آلية الطاقة المرتفعة"
INIT_GAIN_STR				= "حالة الكسب الأولية"
CW_MAX_MIN_STR				= "نافذة التعارض"
PSP_XLINK_STR				= "وضع PSP XLink"
CHANNEL_PLAN_STR			= "خطة القناة"
WL_MODE_STR				= "الوضع اللاسلكي"
PREAMBLE_MODE_STR			= "وضع الإشارة الابتدائية"
FRAGTHRESH_STR				= "حد التجزئة"
RTSTHRESH_STR				= "حد RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "تعطيل"
ENABLE_STR 				= "تمكين"
CAM_STR 				= "الكامة"
MAX_PSP_STR 				= "الحد الأقصى لـ PSP"
FAST_PSP_STR 				= "PSP سريع"
AD_HOC_STR 				= "عشوائي"
INFRASTRUCTURE_STR 			= "البنية الأساسية"
AUTO_SELECT_STR 			= "تحديد تلقائي"
DOMAIN_FROM_EEPROM_STR 			= "المجال من EEPROM"
AUTO_STR 				= "تلقائي"
LONG_PREAMBLE_STR 			= "إشارة ابتدائية طويلة"
SHORT_PREAMBLE_STR 			= "إشارة ابتدائية قصيرة"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "اللجنة الفيدرالية للاتصالات"
IC_STR 					= "دائرة متكاملة"
ETSI_STR 				= "معهد معايير الاتصالات السلكية واللاسلكية"
SPAIN_STR 				= "إسبانيا"
FRANCE_STR 				= "فرنسا"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "إسرائيل"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "حد تكرار التجوال (بالثواني)"
LEISURE_POWER_SAVE_STR			= "توفير الطاقة عند عدم الاستخدام"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "فاصل Beacon الزمني"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.3801] ; Arabic (UAE)
Realtek 				= "شركة Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "3801"
SSID_STR				= "معرف SSID"
CHANNEL_STR				= "القناة"
NETWORK_TYPE_STR			= "نوع الشبكة"
LED_CONTROL_STR				= "التحكم في مؤشر بيان الحالة" 
POWER_SAVE_STR				= "وضع توفير الطاقة"
WIFI_IBSS_STR				= "وضع 11b الافتراضي لـ IBSS"
RATE_ADAPTIVE_STR			= "مهايئ المعدل"
QOS_STR					= "جودة الخدمة"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "القياس اللاسلكي لـ CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "الحد الأقصى لقياس CCX عند عدم الاتصال (0: غير محدود)"
HW_PARA_STR				= "بدء التهيئة من ملف HwparaFile"
THREE_WIRE_MODE_STR			= "وضع البرمجة ثلاثي الأسلاك"
BOARD_TYPE_STR				= "نوع اللوحة"
PROTECTION_MODE_STR			= "وضع الحماية"
TPC_STR					= "نقل التحكم في الطاقة"
TPC_POLARITY_STR			= "تحديد قطبية TPC"
HIGH_POWER_STR				= "آلية الطاقة المرتفعة"
INIT_GAIN_STR				= "حالة الكسب الأولية"
CW_MAX_MIN_STR				= "نافذة التعارض"
PSP_XLINK_STR				= "وضع PSP XLink"
CHANNEL_PLAN_STR			= "خطة القناة"
WL_MODE_STR				= "الوضع اللاسلكي"
PREAMBLE_MODE_STR			= "وضع الإشارة الابتدائية"
FRAGTHRESH_STR				= "حد التجزئة"
RTSTHRESH_STR				= "حد RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "تعطيل"
ENABLE_STR 				= "تمكين"
CAM_STR 				= "الكامة"
MAX_PSP_STR 				= "الحد الأقصى لـ PSP"
FAST_PSP_STR 				= "PSP سريع"
AD_HOC_STR 				= "عشوائي"
INFRASTRUCTURE_STR 			= "البنية الأساسية"
AUTO_SELECT_STR 			= "تحديد تلقائي"
DOMAIN_FROM_EEPROM_STR 			= "المجال من EEPROM"
AUTO_STR 				= "تلقائي"
LONG_PREAMBLE_STR 			= "إشارة ابتدائية طويلة"
SHORT_PREAMBLE_STR 			= "إشارة ابتدائية قصيرة"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "اللجنة الفيدرالية للاتصالات"
IC_STR 					= "دائرة متكاملة"
ETSI_STR 				= "معهد معايير الاتصالات السلكية واللاسلكية"
SPAIN_STR 				= "إسبانيا"
FRANCE_STR 				= "فرنسا"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "إسرائيل"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "حد تكرار التجوال (بالثواني)"
LEISURE_POWER_SAVE_STR			= "توفير الطاقة عند عدم الاستخدام"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "فاصل Beacon الزمني"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.000d] ; Hebrew
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "000d"
SSID_STR				= "SSID"
CHANNEL_STR				= "ערוץ"
NETWORK_TYPE_STR			= "סוג רשת"
LED_CONTROL_STR				= "בקרת נוריות" 
POWER_SAVE_STR				= "מצב חיסכון בצריכת חשמל"
WIFI_IBSS_STR				= "מצב ברירת מחדל 11b ל-IBSS"
RATE_ADAPTIVE_STR			= "קצב מותאם"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "ערך שידור CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "ערך CCX מרבי במצב לא מקוון (0:  ללא הגבלה)"
HW_PARA_STR				= "אתחל מקובץ HwParaFile"
THREE_WIRE_MODE_STR			= "מצב תכנות Three Wire"
BOARD_TYPE_STR				= "סוג לוח"
PROTECTION_MODE_STR			= "מצב הגנה"
TPC_STR					= "בקרת הספק שידור"
TPC_POLARITY_STR			= "בחירת קוטביות TPC"
HIGH_POWER_STR				= "מנגנון הספק גבוה"
INIT_GAIN_STR				= "מצב הגבר התחלתי"
CW_MAX_MIN_STR				= "חלון Contention"
PSP_XLINK_STR				= "מצב PSP XLink"
CHANNEL_PLAN_STR			= "תכנון ערוצים"
WL_MODE_STR				= "מצב אלחוטי"
PREAMBLE_MODE_STR			= "מצב מקדים"
FRAGTHRESH_STR				= "סף פיצול"
RTSTHRESH_STR				= "סף RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "חסום"
ENABLE_STR 				= "אפשר"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "אד הוק"
INFRASTRUCTURE_STR 			= "תשתית"
AUTO_SELECT_STR 			= "בחירה אוטומטית"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "אוטומטי"
LONG_PREAMBLE_STR 			= "מקדים ארוך"
SHORT_PREAMBLE_STR 			= "מקים קצר"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "ספרד"
FRANCE_STR 				= "צרפת"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "ישראל"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "הגבלת ניסיון חוזר לנדידה (שניות)"
LEISURE_POWER_SAVE_STR			= "מצב חיסכון בחשמל בזמן המתנה"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "מרווח זמן למשואה"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0816] ; Portuguese (Portugal)
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0816"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Canal"
NETWORK_TYPE_STR 			= "Tipo de rede"
LED_CONTROL_STR				= "Controlo dos LEDs" 
POWER_SAVE_STR				= "Modo de poupanca de energia"
WIFI_IBSS_STR				= "Modo IBSS 11b predefinido"
RATE_ADAPTIVE_STR			= "Velocidade adaptativa"
QOS_STR					= "QoS"
WMM_APSD				= "APSD WMM"
CCX_RM_STR				= "Medida de radio CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Medida off-line maxima CCX (0: ilimitada)"
HW_PARA_STR				= "Iniciar a partir de ficheiro de parametros do hardware"
THREE_WIRE_MODE_STR			= "Modo de programacao com tres fios"
BOARD_TYPE_STR				= "Tipo de placa"
PROTECTION_MODE_STR			= "Modo de proteccao"
TPC_STR					= "Controlo da potencia de transmissao"
TPC_POLARITY_STR			= "Seleccao da polaridade TPC"
HIGH_POWER_STR				= "Mecanismo de alta potencia"
INIT_GAIN_STR				= "Estado de ganho inicial"
CW_MAX_MIN_STR				= "Janela de contencao"
PSP_XLINK_STR				= "Modo PSP XLink"
CHANNEL_PLAN_STR			= "Plano de canais"
WL_MODE_STR				= "Modo sem fios"
PREAMBLE_MODE_STR			= "Modo de preambulo"
FRAGTHRESH_STR				= "Limiar de fragmentacao"
RTSTHRESH_STR				= "Limiar RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Desactivar"
ENABLE_STR 				= "Activar"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infraestrutura"
AUTO_SELECT_STR 			= "Seleccao automatica"
DOMAIN_FROM_EEPROM_STR 			= "DOMINIO_DE_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Preambulo longo"
SHORT_PREAMBLE_STR 			= "Preambulo curto"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Espanha"
FRANCE_STR 				= "Franca"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Limite para tentativas de itinerancia (seg.)"
LEISURE_POWER_SAVE_STR			= "Poupanca de energia em diversao"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Intervalo de sinalizacao"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0416] ; Portuguese (Brazil)
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0416"
SSID_STR				= "SSID"
CHANNEL_STR				= "Canal"
NETWORK_TYPE_STR			= "Tipo de Rede"
LED_CONTROL_STR				= "Controle de LED" 
POWER_SAVE_STR				= "Modo de Economia de Energia"
WIFI_IBSS_STR				= "Modo IBSS Default 11b"
RATE_ADAPTIVE_STR			= "Adaptativo à Taxa"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "Medida de Rádio CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Medida offline máx. CCX (0: ilimitada)"
HW_PARA_STR				= "Inicialização de HwParaFile"
THREE_WIRE_MODE_STR			= "Modo de programação de três fios"
BOARD_TYPE_STR				= "Tipo de placa"
PROTECTION_MODE_STR			= "Modo de Proteção"
TPC_STR					= "Controle de Potência de Transmissão"
TPC_POLARITY_STR			= "Seleção de Polaridade TPC"
HIGH_POWER_STR				= "Mecanismo de Alta Potência"
INIT_GAIN_STR				= "Estado de Ganho Inicial"
CW_MAX_MIN_STR				= "Janela de Contenção"
PSP_XLINK_STR				= "Modo PSP XLink"
CHANNEL_PLAN_STR			= "Plano de Canal"

WL_MODE_STR				= "Modo Wireless"
PREAMBLE_MODE_STR			= "Modo de Preâmbulo"
FRAGTHRESH_STR				= "Limite de Fragmentação"
RTSTHRESH_STR				= "Limite RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Desabilitar"
ENABLE_STR 				= "Habilitar"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "PSP MÁX"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infra-estrutura"
AUTO_SELECT_STR 			= "Seleção automática"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Automático"
LONG_PREAMBLE_STR 			= "Preâmbulo longo"
SHORT_PREAMBLE_STR 			= "Preâmbulo curto"
LONG_SHORT_PREAMBLE_STR			= "Long and Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "CI"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Espanha"
FRANCE_STR 				= "França"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Limite de Tentativas de Roam (seg)"
LEISURE_POWER_SAVE_STR			= "Economia de Energia de Descanso"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Intervalo de Sinal"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0421]	;Indonesian
Realtek     				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0421"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Channel"
NETWORK_TYPE_STR 			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"

TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
CHANNEL_PLAN_STR			= "Channel Plan"
WL_MODE_STR				= "Wireless Mode"
PREAMBLE_MODE_STR			= "Preamble Mode"
FRAGTHRESH_STR				= "Fragmentation Threshold"
RTSTHRESH_STR				= "RTS Threshold"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Disabled"
ENABLE_STR 				= "Enabled"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastructure"
AUTO_SELECT_STR 			= "Auto select"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spain"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"	
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Roam Retry Limit(sec)"
LEISURE_POWER_SAVE_STR			= "Leisure Power Save"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Beacon Interval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
;;====================================================================================================================
[Strings.0422] ; Ukrainian
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."
ASUS					= "ASUSTeK Computer Inc."
EDIMAX					= "Edimax Technology Co., Ltd"
TPLINK					= "TP-Link Technologies Co., Ltd."

LOCALE_STR				= "0422"
SSID_STR 				= "SSID"
CHANNEL_STR				= "Channel"
NETWORK_TYPE_STR 			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
CHANNEL_PLAN_STR			= "Channel Plan"
WL_MODE_STR				= "Wireless Mode"
PREAMBLE_MODE_STR			= "Preamble Mode"
FRAGTHRESH_STR				= "Fragmentation Threshold"
RTSTHRESH_STR				= "RTS Threshold"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			= "11n AdHoc"

DISABLE_STR 				= "Disabled"
ENABLE_STR 				= "Enabled"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastructure"
AUTO_SELECT_STR 			= "Auto select"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
SHORT_PREAMBLE_STR 			= "Short Preamble"
LONG_SHORT_PREAMBLE_STR			= "Short & long"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spain"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
Roam_Retry_Limit_STR			= "Roam Retry Limit(sec)"
LEISURE_POWER_SAVE_STR			= "Leisure Power Save"
LEISURE_POWER_SAVE_AUTO			= "AUTO"
LEISURE_POWER_SAVE_ENABLE		= "ENABLE"
LEISURE_POWER_SAVE_DISABLE		= "DISABLE"
AH_BCNINTV_STR 				= "Beacon Interval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
SleepOnDisconnect			= "Sleep on WoWLAN disconnect"

;;Source disk name
DISKNAME 			="Realtek Wireless LAN 802.11n PCI-E Network Adapter Driver Disk"
RTWlanE.DeviceDesc 		="Realtek Wireless LAN 802.11n PCI-E Network Adapter"
RTWlanE.DeviceDesc.DispName	="Realtek Wireless LAN 802.11n PCI-E Network Adapter"

RTL8822be.DeviceDesc		    ="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
RTL8822be.DeviceDesc.DispName	="Realtek 8822BE Wireless LAN 802.11ac PCI-E NIC"
HP8822be.DeviceDesc		    ="Realtek RTL8822BE 802.11ac PCIe Adapter"
HP8822be.DeviceDesc.DispName	="Realtek RTL8822BE 802.11ac PCIe Adapter"

RTL8822ce.DeviceDesc     ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
RTL8822ce.DeviceDesc.DispName ="Realtek 8822CE Wireless LAN 802.11ac PCI-E NIC"
HP8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
HP8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc		    ="Realtek RTL8822CE 802.11ac PCIe Adapter"
MS8822ce.DeviceDesc.DispName	="Realtek RTL8822CE 802.11ac PCIe Adapter"


RTL8821ce.DeviceDesc		    ="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
RTL8821ce.DeviceDesc.DispName	="Realtek 8821CE Wireless LAN 802.11ac PCI-E NIC"
HP8821ce.DeviceDesc		    ="Realtek RTL8821CE 802.11ac PCIe Adapter"
HP8821ce.DeviceDesc.DispName	="Realtek RTL8821CE 802.11ac PCIe Adapter"

RTL8723de.DeviceDesc		    ="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
RTL8723de.DeviceDesc.DispName	="Realtek 8723DE Wireless LAN 802.11n PCI-E NIC"
HP8723de.DeviceDesc		    ="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
HP8723de.DeviceDesc.DispName	="Realtek RTL8723DE 802.11b/g/n PCIe Adapter"
