N16Pro Disassembly and assembly of fingerprint cable
Please remove the bottom cover and internal battery screws first, and then remove the battery;
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The fingerprint plug is shown in the above figure
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Pull the black buckle outward
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Gently pull out the fingerprint cable
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The other end of the fingerprint cable needs to be removed using a different method, which requires pulling the black buckle upwards
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Then pull out the fingerprint cable
Finally, please reinstall the fingerprint cable and push in or press down the buckle; Reinstall the battery screws and battery cables, and install the bottom cover;
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